(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "USLetter")
  (title_block
    (title "USB-Tentacle")
    (date "2022-07-21")
    (rev "1.0")
    (comment 1 "Customizable 3x3 keypad that emulates a USB keyboard.")
    (comment 2 "Designed by Rex McKinnon <0xff@rexploits.com>")
  )
  (layers
    (0 "F.Cu" jumper)
    (31 "B.Cu" signal)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen") (color "#F0F0F0FF"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "#280A41E6") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "#280A41E6") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen") (color "#F0F0F0FF"))
      (copper_finish "ENIG")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (net 0 "")
  (net 1 "VBUS")
  (net 2 "GND")
  (net 3 "Net-(C4-Pad1)")
  (net 4 "/ROW_1")
  (net 5 "Net-(D1-Pad2)")
  (net 6 "/ROW_2")
  (net 7 "Net-(D2-Pad2)")
  (net 8 "/ROW_3")
  (net 9 "Net-(D3-Pad2)")
  (net 10 "Net-(D4-Pad2)")
  (net 11 "Net-(D5-Pad2)")
  (net 12 "Net-(D6-Pad2)")
  (net 13 "Net-(D7-Pad2)")
  (net 14 "Net-(D8-Pad2)")
  (net 15 "Net-(D9-Pad2)")
  (net 16 "unconnected-(J1-Pad4)")
  (net 17 "/COL_3")
  (net 18 "/COL_1")
  (net 19 "/COL_2")
  (net 20 "Net-(R3-Pad2)")
  (net 21 "/D-")
  (net 22 "/D+")
  (net 23 "/PUD-")
  (net 24 "Net-(U1-Pad2)")
  (net 25 "Net-(J1-Pad2)")
  (net 26 "Net-(U1-Pad4)")
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" (layer "F.Cu")
    (tedit 56DDBCCA)
    (at 164.76 141.63)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_Pad_Via" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "1" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  )
  (footprint "kibuzzard-62D88F76" (layer "F.Cu")
    (tedit 62D88F76)
    (at 132.3 139.7)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6ICIyIiwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJNdWx0aUxpbmVUZXh0IjogIkNvbCAyIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogIjIiLCAiUGFkZGluZ0xlZnRDdHJsIjogIjAiLCAiUGFkZGluZ1JpZ2h0Q3RybCI6ICIwIiwgIlBhZGRpbmdUb3BDdHJsIjogIjIiLCAiV2lkdGhDdHJsIjogIjEuNzUifQ==")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-62D88F76" (at 0 -4.425421) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 4.425421) (layer "F.SilkS") hide)
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" (layer "F.Cu")
    (tedit 56DDBCCA)
    (at 99.76 76.63)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_Pad_Via" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "1" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" (layer "F.Cu")
    (tedit 56DDBCCA)
    (at 99.76 141.63)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_Pad_Via" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "1" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" (layer "F.Cu")
    (tedit 56DDBCCA)
    (at 164.76 76.63)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_Pad_Via" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "1" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  )
  (footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB" (layer "F.Cu")
    (tedit 5A02FE24)
    (at 134.8 85)
    (descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u PCB")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW2" (at -2.54 -2.794) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at -2.54 12.954) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.54 -2.794) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -7.62 5.08) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 5.08) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.54 5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 7 "Net-(D2-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -6.35 2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 19 "/COL_2") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_PCB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB" (layer "F.Cu")
    (tedit 5A02FE24)
    (at 115.75 85)
    (descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u PCB")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW1" (at -2.54 -2.794) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at -2.54 12.954) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.54 -2.794) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -7.62 5.08) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.54 5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 5.08) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -6.35 2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 18 "/COL_1") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_PCB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB" (layer "F.Cu")
    (tedit 5A02FE24)
    (at 153.85 104.05)
    (descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u PCB")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW6" (at -2.54 -2.794) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at -2.54 12.954) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.54 -2.794) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -2.54 5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 5.08) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -7.62 5.08) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 12 "Net-(D6-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -6.35 2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 17 "/COL_3") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_PCB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kibuzzard-62D88F18" (layer "F.Cu")
    (tedit 62D88F18)
    (at 162.7 109.1 -90)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6ICIyIiwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJNdWx0aUxpbmVUZXh0IjogIlJvdyAyIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogIjIiLCAiUGFkZGluZ0xlZnRDdHJsIjogIjAiLCAiUGFkZGluZ1JpZ2h0Q3RybCI6ICIwIiwgIlBhZGRpbmdUb3BDdHJsIjogIjIiLCAiV2lkdGhDdHJsIjogIjEuNzUifQ==")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-62D88F18" (at 0 -4.338108 90) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 4.338108 90) (layer "F.SilkS") hide)
  )
  (footprint "kibuzzard-62D88F88" (layer "F.Cu")
    (tedit 62D88F88)
    (at 151.2 139.7)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6ICIyIiwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJNdWx0aUxpbmVUZXh0IjogIkNvbCAzIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogIjIiLCAiUGFkZGluZ0xlZnRDdHJsIjogIjAiLCAiUGFkZGluZ1JpZ2h0Q3RybCI6ICIwIiwgIlBhZGRpbmdUb3BDdHJsIjogIjIiLCAiV2lkdGhDdHJsIjogIjEuNzUifQ==")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-62D88F88" (at 0 -4.425421) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 4.425421) (layer "F.SilkS") hide)
  )
  (footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB" (layer "F.Cu")
    (tedit 5A02FE24)
    (at 115.75 123.1)
    (descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u PCB")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW7" (at -2.54 -2.794) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at -2.54 12.954) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.54 -2.794) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -7.62 5.08) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.54 5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 5.08) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 13 "Net-(D7-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -6.35 2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 18 "/COL_1") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_PCB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB" (layer "F.Cu")
    (tedit 5A02FE24)
    (at 134.8 123.1)
    (descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u PCB")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW8" (at -2.54 -2.794) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at -2.54 12.954) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.54 -2.794) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -2.54 5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -7.62 5.08) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 5.08) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 14 "Net-(D8-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -6.35 2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 19 "/COL_2") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_PCB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB" (layer "F.Cu")
    (tedit 5A02FE24)
    (at 115.75 104.05)
    (descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u PCB")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW4" (at -2.54 -2.794) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at -2.54 12.954) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.54 -2.794) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -7.62 5.08) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.54 5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 5.08) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 10 "Net-(D4-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -6.35 2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 18 "/COL_1") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_PCB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB" (layer "F.Cu")
    (tedit 5A02FE24)
    (at 153.85 85)
    (descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u PCB")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW3" (at -2.54 -2.794) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at -2.54 12.954) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.54 -2.794) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 2.54 5.08) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.54 5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -7.62 5.08) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 9 "Net-(D3-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -6.35 2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 17 "/COL_3") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_PCB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kibuzzard-62D88F2B" (layer "F.Cu")
    (tedit 62D88F2B)
    (at 162.7 128 -90)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6ICIyIiwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJNdWx0aUxpbmVUZXh0IjogIlJvdyAzIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogIjIiLCAiUGFkZGluZ0xlZnRDdHJsIjogIjAiLCAiUGFkZGluZ1JpZ2h0Q3RybCI6ICIwIiwgIlBhZGRpbmdUb3BDdHJsIjogIjIiLCAiV2lkdGhDdHJsIjogIjEuNzUifQ==")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-62D88F2B" (at 0 -4.338108 90) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 4.338108 90) (layer "F.SilkS") hide)
  )
  (footprint "kibuzzard-62D88EEF" (layer "F.Cu")
    (tedit 62D88EEF)
    (at 162.7 90.1 -90)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6ICIyIiwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJNdWx0aUxpbmVUZXh0IjogIlJvdyAxIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogIjIiLCAiUGFkZGluZ0xlZnRDdHJsIjogIjAiLCAiUGFkZGluZ1JpZ2h0Q3RybCI6ICIwIiwgIlBhZGRpbmdUb3BDdHJsIjogIjIiLCAiV2lkdGhDdHJsIjogIjEuNzUifQ==")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-62D88EEF" (at 0 -4.326996 -90) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 4.326996 -90) (layer "F.SilkS") hide)
  )
  (footprint "kibuzzard-62D88F66" (layer "F.Cu")
    (tedit 62D88F66)
    (at 113.2 139.7)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6ICIyIiwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJNdWx0aUxpbmVUZXh0IjogIkNvbCAxIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogIjIiLCAiUGFkZGluZ0xlZnRDdHJsIjogIjAiLCAiUGFkZGluZ1JpZ2h0Q3RybCI6ICIwIiwgIlBhZGRpbmdUb3BDdHJsIjogIjIiLCAiV2lkdGhDdHJsIjogIjEuNzUifQ==")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-62D88F66" (at 0 -4.425421) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 4.425421) (layer "F.SilkS") hide)
  )
  (footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB" (layer "F.Cu")
    (tedit 5A02FE24)
    (at 153.85 123.1)
    (descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u PCB")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW9" (at -2.54 -2.794) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at -2.54 12.954) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.54 -2.794) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 2.54 5.08) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -7.62 5.08) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.54 5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 15 "Net-(D9-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -6.35 2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 17 "/COL_3") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_PCB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB" (layer "F.Cu")
    (tedit 5A02FE24)
    (at 134.8 104.05)
    (descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
    (tags "Cherry MX keyswitch 1.00u PCB")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW5" (at -2.54 -2.794) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at -2.54 12.954) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.54 -2.794) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 2.54 5.08) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.54 5.08) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -7.62 5.08) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 11 "Net-(D5-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -6.35 2.54) (size 2.2 2.2) (drill 1.5) (layers *.Cu *.Mask)
      (net 19 "/COL_2") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_PCB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 156.425 116.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at -2.725 0) (layer "B.SilkS"))
    (fp_text value "1.5K" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(J1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 23 "/PUD-") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_1206_3216Metric" (layer "B.Cu")
    (tedit 5F68FEF0)
    (at 116 118.35 -90)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D7" (at 0 1.82 90) (layer "B.SilkS"))
    (fp_text value "D" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 8 "/ROW_3") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 13 "Net-(D7-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_1206_3216Metric" (layer "B.Cu")
    (tedit 5F68FEF0)
    (at 139.1 123.7 180)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D8" (at 0 1.82) (layer "B.SilkS"))
    (fp_text value "D" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 8 "/ROW_3") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 14 "Net-(D8-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 150.75 114.85)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.35) (layer "B.SilkS"))
    (fp_text value "TBD" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(U1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm" (layer "B.Cu")
    (tedit 5A0FD1B2)
    (at 146.9 115.65)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Y1" (at 0 2.45) (layer "B.SilkS"))
    (fp_text value "12MHz" (at 0 -2.45) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect (at -1.1 -0.85) (size 1.4 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "Net-(U1-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 1.1 -0.85) (size 1.4 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 1.1 0.85) (size 1.4 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "Net-(C4-Pad1)") (pinfunction "3") (pintype "passive"))
    (pad "4" smd rect (at -1.1 0.85) (size 1.4 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 156.4 120.45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 2.75 -0.05) (layer "B.SilkS"))
    (fp_text value "680" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "/D+") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(R3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "B.Cu")
    (tedit 5D9F72B1)
    (at 137.85 116.3 180)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 5.28) (layer "B.SilkS"))
    (fp_text value "ATtiny44A-SS" (at 0 -5.28) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.475 3.81 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "VBUS") (pinfunction "VCC") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.475 2.54 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(U1-Pad2)") (pinfunction "XTAL1/PB0") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -2.475 1.27 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C4-Pad1)") (pinfunction "XTAL2/PB1") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -2.475 0 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(U1-Pad4)") (pinfunction "~{RESET}/PB3") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -2.475 -1.27 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 23 "/PUD-") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -2.475 -2.54 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 21 "/D-") (pinfunction "PA7") (pintype "bidirectional"))
    (pad "7" smd roundrect (at -2.475 -3.81 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "/D+") (pinfunction "PA6") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 2.475 -3.81 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "/COL_3") (pinfunction "PA5") (pintype "bidirectional"))
    (pad "9" smd roundrect (at 2.475 -2.54 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "/COL_2") (pinfunction "PA4") (pintype "bidirectional"))
    (pad "10" smd roundrect (at 2.475 -1.27 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "/COL_1") (pinfunction "PA3") (pintype "bidirectional"))
    (pad "11" smd roundrect (at 2.475 0 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/ROW_3") (pinfunction "PA2") (pintype "bidirectional"))
    (pad "12" smd roundrect (at 2.475 1.27 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "/ROW_1") (pinfunction "PA1") (pintype "bidirectional"))
    (pad "13" smd roundrect (at 2.475 2.54 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "/ROW_2") (pinfunction "AREF/PA0") (pintype "bidirectional"))
    (pad "14" smd roundrect (at 2.475 3.81 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "UPL-Connectors:USB_Micro-B_Receptacle_AdamTech_MCR-B-S-RA-SMT-CS5A-NF-TR" (layer "B.Cu")
    (tedit 0)
    (at 168 109.13)
    (descr "USB Micro-B Receptacle - SMD pads with Through Hole")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at -2.3 -4.6 unlocked) (layer "B.SilkS"))
    (fp_text value "USB_B_Micro" (at 0 -5.25 180 unlocked) (layer "B.Fab"))
    (fp_text user "pcb edge" (at 2.5 -0.25 -90 unlocked) (layer "Dwgs.User"))
    (fp_text user "${REFERENCE}" (at 0 5 180 unlocked) (layer "B.Fab"))
    (pad "1" smd rect (at -2.625 -1.3) (size 1.25 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "VBUS") (pinfunction "VBUS") (pintype "power_out"))
    (pad "2" smd rect (at -2.625 -0.65) (size 1.25 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "Net-(J1-Pad2)") (pinfunction "D-") (pintype "bidirectional"))
    (pad "3" smd rect (at -2.625 0) (size 1.25 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "Net-(R3-Pad2)") (pinfunction "D+") (pintype "bidirectional"))
    (pad "4" smd rect (at -2.625 0.65) (size 1.25 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "unconnected-(J1-Pad4)") (pinfunction "ID") (pintype "passive+no_connect"))
    (pad "5" smd rect (at -2.625 1.3) (size 1.25 0.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "6" thru_hole circle (at -2.65 -2.6) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole circle (at -2.65 2.6) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -3.6) (size 1.9 1.1) (drill oval 1.3 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 3.6) (size 1.9 1.1) (drill oval 1.3 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
  )
  (footprint "Diode_SMD:D_1206_3216Metric" (layer "B.Cu")
    (tedit 5F68FEF0)
    (at 151.6 96.3 90)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D3" (at 0 -1.8 90) (layer "B.SilkS"))
    (fp_text value "D" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 4 "/ROW_1") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 9 "Net-(D3-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 156.4 118.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 2.75 0) (layer "B.SilkS"))
    (fp_text value "680" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 21 "/D-") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(J1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 129.72 74.8225 -90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 1.27 2.52 90) (layer "B.SilkS"))
    (fp_text value "AVR-ISP-6" (at 1.27 -7.41 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -2.54) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/COL_3") (pinfunction "MISO") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "VBUS") (pinfunction "VCC") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/COL_2") (pinfunction "SCK") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/D+") (pinfunction "MOSI") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(U1-Pad4)") (pinfunction "~{RST}") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_1206_3216Metric" (layer "B.Cu")
    (tedit 5F68FEF0)
    (at 150.55 102.65 -90)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D6" (at 0 1.82 90) (layer "B.SilkS"))
    (fp_text value "D" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 6 "/ROW_2") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 12 "Net-(D6-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_1206_3216Metric" (layer "B.Cu")
    (tedit 5F68FEF0)
    (at 131.95 96.3 90)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at 0 -1.85 90) (layer "B.SilkS"))
    (fp_text value "D" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 4 "/ROW_1") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 7 "Net-(D2-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_1206_3216Metric" (layer "B.Cu")
    (tedit 5F68FEF0)
    (at 115.75 95.85 90)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at 0 -1.85 90) (layer "B.SilkS"))
    (fp_text value "D" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 4 "/ROW_1") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 5 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_1206_3216Metric" (layer "B.Cu")
    (tedit 5F68FEF0)
    (at 122.7 103.3 180)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D4" (at 0 1.82) (layer "B.SilkS"))
    (fp_text value "D" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 6 "/ROW_2") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 10 "Net-(D4-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 160.7 106.425 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.85 90) (layer "B.SilkS"))
    (fp_text value "1uF" (at 0 -1.85 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "VBUS") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2173913043)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_1206_3216Metric" (layer "B.Cu")
    (tedit 5F68FEF0)
    (at 131.9 102.65 -90)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D5" (at 0 1.82 90) (layer "B.SilkS"))
    (fp_text value "D" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 6 "/ROW_2") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 11 "Net-(D5-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kibuzzard-62D873FF" (layer "B.Cu")
    (tedit 62D873FF)
    (at 164.7 127.2 -90)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiWyIsICJDYXBSaWdodENob2ljZSI6ICI8IiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6ICI0LjUiLCAiTGF5ZXJDb21ib0JveCI6ICJGLlNpbGtTIiwgIk11bHRpTGluZVRleHQiOiAidjEuMCIsICJQYWRkaW5nQm90dG9tQ3RybCI6ICIzIiwgIlBhZGRpbmdMZWZ0Q3RybCI6ICI0IiwgIlBhZGRpbmdSaWdodEN0cmwiOiAiNCIsICJQYWRkaW5nVG9wQ3RybCI6ICIzIiwgIldpZHRoQ3RybCI6ICI0In0=")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-62D873FF" (at 0 6.2484 90) (layer "B.SilkS") hide)
    (fp_text value "G***" (at 0 -6.2484 90) (layer "B.SilkS") hide)
  )
  (footprint "Diode_SMD:D_1206_3216Metric" (layer "B.Cu")
    (tedit 5F68FEF0)
    (at 148.7 122.85)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D9" (at 0 -1.85) (layer "B.SilkS"))
    (fp_text value "D" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4 0) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 8 "/ROW_3") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0) (size 1.25 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 15 "Net-(D9-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 143.05 110.225 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.65 90) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 0 -1.85 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "VBUS") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2173913043)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kibuzzard-62D87684" (layer "B.Cu")
    (tedit 62D87684)
    (at 164.8 92.1 -90)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6ICI0IiwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJNdWx0aUxpbmVUZXh0IjogIjA3LzIyIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogIjIiLCAiUGFkZGluZ0xlZnRDdHJsIjogIjAiLCAiUGFkZGluZ1JpZ2h0Q3RybCI6ICIwIiwgIlBhZGRpbmdUb3BDdHJsIjogIjIiLCAiV2lkdGhDdHJsIjogIjMuNSJ9")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-62D87684" (at 0 6.320367 90) (layer "B.SilkS") hide)
    (fp_text value "G***" (at 0 -6.320367 90) (layer "B.SilkS") hide)
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 150.75 116.75)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "at-tentacle.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0 1.55) (layer "B.SilkS"))
    (fp_text value "TBD" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kibuzzard-62D87485" (layer "B.Cu")
    (tedit 62D87485)
    (at 146.4 76.1 180)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiPiIsICJDYXBSaWdodENob2ljZSI6ICI+IiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6ICI0LjUiLCAiTGF5ZXJDb21ib0JveCI6ICJGLlNpbGtTIiwgIk11bHRpTGluZVRleHQiOiAiSVNQIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogIjMiLCAiUGFkZGluZ0xlZnRDdHJsIjogIjQiLCAiUGFkZGluZ1JpZ2h0Q3RybCI6ICI0IiwgIlBhZGRpbmdUb3BDdHJsIjogIjMiLCAiV2lkdGhDdHJsIjogIjQifQ==")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-62D87485" (at 0 6.2484) (layer "B.SilkS") hide)
    (fp_text value "G***" (at 0 -6.2484) (layer "B.SilkS") hide)
  )
  (gr_rect (start 94.76 71.63) (end 169.76 146.63) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "rexploits.com" (at 99.8 81.5 270) (layer "B.SilkS"))
  (gr_text "JLCJLCJLCJLC" (at 104.9 76.6) (layer "B.SilkS"))
  (gr_text "Rex McKinnon" (at 99.7 136.3 270) (layer "B.SilkS"))
  (gr_text "USB-Tentacle" (at 132.8 138.1) (layer "B.SilkS"))
  (gr_text "19.05mm" (at 102.2 90.1 90) (layer "F.SilkS"))
  (gr_text "9.525" (at 102.2 104.2 90) (layer "F.SilkS"))
  (gr_text "19.05mm" (at 102.2 118.6 90) (layer "F.SilkS"))
  (gr_text "75mm" (at 97 109.4 270) (layer "F.SilkS"))
  (gr_text "M3 D3.2mm (x4)" (at 98.2 137.5 90) (layer "F.SilkS"))
  (gr_text "57.15mm" (at 99.3 109.1 90) (layer "F.SilkS"))
  (gr_text "65mm" (at 104.4 109.3 270) (layer "F.SilkS"))
  (gr_text "9.525" (at 102.2 133.1 90) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.3 145.2)
        (xy 95.9 145.2)
        (xy 95.9 137.6)
        (xy 103.3 137.6)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 168.5 145.4)
        (xy 161.1 145.4)
        (xy 161.1 137.8)
        (xy 168.5 137.8)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.4 80.4)
        (xy 96 80.4)
        (xy 96 72.8)
        (xy 103.4 72.8)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 170.35 69.3)
        (xy 170.55 148.05)
        (xy 91.25 148.75)
        (xy 91.75 69.15)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 168.4 80.2)
        (xy 161 80.2)
        (xy 161 72.6)
        (xy 168.4 72.6)
      )
    )
  )
)
