(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "USLetter")
  (title_block
    (title "ISP Programmer based on FabISP, USBTinyISP")
    (date "2022-10-22")
    (rev "1.0")
    (comment 2 "Designed by Rex McKinnon <0xff@rexploits.com>")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "VBUS")
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(C4-Pad1)")
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(J1-Pad2)")
  (net 7 "Net-(J1-Pad3)")
  (net 8 "/MISO")
  (net 9 "Net-(J2-Pad2)")
  (net 10 "/SCK")
  (net 11 "/MOSI")
  (net 12 "/SCS")
  (net 13 "/~{Reset}")
  (net 14 "Net-(R2-Pad2)")
  (net 15 "Net-(R3-Pad2)")
  (net 16 "Net-(R4-Pad2)")
  (net 17 "unconnected-(U1-Pad6)")
  (net 18 "unconnected-(U1-Pad7)")
  (net 19 "unconnected-(U1-Pad10)")
  (net 20 "unconnected-(U1-Pad14)")
  (net 21 "unconnected-(U1-Pad15)")
  (net 22 "unconnected-(U1-Pad17)")
  (net 23 "unconnected-(U1-Pad18)")
  (net 24 "unconnected-(U1-Pad19)")
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 134.7025 70.5 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "File: usbtiny.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at 2.4525 0.54) (layer "F.SilkS"))
    (fp_text value "Blue" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 128.25 81.5 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: usbtiny.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at -0.5 -1.35 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VBUS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 126 79 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: usbtiny.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at -2.4 0.2 180) (layer "F.SilkS"))
    (fp_text value "1K5" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(J1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VBUS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 132.25 81.5 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: usbtiny.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0.5 -1.25 90) (layer "F.SilkS"))
    (fp_text value "TBD" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm" (layer "F.Cu")
    (tedit 5DC5F6A3)
    (at 132.25 76 -45)
    (descr "QFN, 20 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/doc2535.pdf#page=164), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (property "Sheetfile" "File: usbtiny.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at -3.146625 -3.075914) (layer "F.SilkS"))
    (fp_text value "ATtiny44V-15MT" (at 0 3.3 135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "" smd roundrect (at 0.65 -0.65 315) (size 1.05 1.05) (layers "F.Paste") (roundrect_rratio 0.2380952381))
    (pad "" smd roundrect (at 0.65 0.65 315) (size 1.05 1.05) (layers "F.Paste") (roundrect_rratio 0.2380952381))
    (pad "" smd roundrect (at -0.65 -0.65 315) (size 1.05 1.05) (layers "F.Paste") (roundrect_rratio 0.2380952381))
    (pad "" smd roundrect (at -0.65 0.65 315) (size 1.05 1.05) (layers "F.Paste") (roundrect_rratio 0.2380952381))
    (pad "1" smd roundrect (at -1.925 -1 315) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/SCK") (pinfunction "PA4") (pintype "bidirectional"))
    (pad "2" smd roundrect (at -1.925 -0.5 315) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/SCS") (pinfunction "PA3") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -1.925 0 315) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(R4-Pad2)") (pinfunction "PA2") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -1.925 0.5 315) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(R3-Pad2)") (pinfunction "PA1") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -1.925 1 315) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(R2-Pad2)") (pinfunction "AREF/PA0") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -1 1.925 315) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "unconnected-(U1-Pad6)") (pinfunction "NC") (pintype "no_connect"))
    (pad "7" smd roundrect (at -0.5 1.925 315) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "unconnected-(U1-Pad7)") (pinfunction "NC") (pintype "no_connect"))
    (pad "8" smd roundrect (at 0 1.925 315) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" smd roundrect (at 0.5 1.925 315) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VBUS") (pinfunction "VCC") (pintype "power_in"))
    (pad "10" smd roundrect (at 1 1.925 315) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "unconnected-(U1-Pad10)") (pinfunction "NC") (pintype "no_connect"))
    (pad "11" smd roundrect (at 1.925 1 315) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C3-Pad1)") (pinfunction "XTAL1/PB0") (pintype "bidirectional"))
    (pad "12" smd roundrect (at 1.925 0.5 315) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C4-Pad1)") (pinfunction "XTAL2/PB1") (pintype "bidirectional"))
    (pad "13" smd roundrect (at 1.925 0 315) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/~{Reset}") (pinfunction "~{RESET}/PB3") (pintype "bidirectional"))
    (pad "14" smd roundrect (at 1.925 -0.5 315) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "unconnected-(U1-Pad14)") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 1.925 -1 315) (size 0.85 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "unconnected-(U1-Pad15)") (pinfunction "PA7") (pintype "bidirectional"))
    (pad "16" smd roundrect (at 1 -1.925 315) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/MOSI") (pinfunction "PA6") (pintype "bidirectional"))
    (pad "17" smd roundrect (at 0.5 -1.925 315) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "unconnected-(U1-Pad17)") (pinfunction "NC") (pintype "no_connect"))
    (pad "18" smd roundrect (at 0 -1.925 315) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "unconnected-(U1-Pad18)") (pinfunction "NC") (pintype "no_connect"))
    (pad "19" smd roundrect (at -0.5 -1.925 315) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "unconnected-(U1-Pad19)") (pinfunction "NC") (pintype "no_connect"))
    (pad "20" smd roundrect (at -1 -1.925 315) (size 0.25 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/MISO") (pinfunction "PA5") (pintype "bidirectional"))
    (pad "21" smd rect (at 0 0 315) (size 2.6 2.6) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm" (layer "F.Cu")
    (tedit 5A0FD1B2)
    (at 135.25 80.75 180)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (property "Sheetfile" "File: usbtiny.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Y1" (at -3.15 0.95) (layer "F.SilkS"))
    (fp_text value ">12MHz" (at 0 2.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.1 0.85 180) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(C4-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 1.1 0.85 180) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 1.1 -0.85 180) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C3-Pad1)") (pinfunction "3") (pintype "passive"))
    (pad "4" smd rect (at -1.1 -0.85 180) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kibuzzard-63531BD1" (layer "F.Cu")
    (tedit 63531BD1)
    (at 137.82 74.11 -15)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJGcmVkb2thT25lIiwgIkhlaWdodEN0cmwiOiAiMS41IiwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJNdWx0aUxpbmVUZXh0IjogIklTUCIsICJQYWRkaW5nQm90dG9tQ3RybCI6ICIiLCAiUGFkZGluZ0xlZnRDdHJsIjogIjAiLCAiUGFkZGluZ1JpZ2h0Q3RybCI6ICIwIiwgIlBhZGRpbmdUb3BDdHJsIjogIjUiLCAiV2lkdGhDdHJsIjogIjEuMjUifQ==")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-63531BD1" (at 0 -4.451284 165) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 4.451284 165) (layer "F.SilkS") hide)
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 59FED5CB)
    (at 142.34 73.46)
    (descr "Through hole angled pin header, 2x03, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "File: usbtiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -2.54 -0.06 90) (layer "F.SilkS") hide)
    (fp_text value "AVR-ISP-6" (at 1.687 7.06) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.232 2.541 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/MISO") (pinfunction "MISO") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad2)") (pinfunction "VCC") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/SCK") (pinfunction "SCK") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/MOSI") (pinfunction "MOSI") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "/SCS") (pinfunction "~{RST}") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 126 75)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: usbtiny.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 2.4 -0.2 180) (layer "F.SilkS"))
    (fp_text value "680" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(J1-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(R3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.125 78.25)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: usbtiny.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0.475 -1.25) (layer "F.SilkS"))
    (fp_text value "TBD" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "UPL-Connectors:USB_A_Plug_CUIDevices_UP2-AH-1-TH" (layer "F.Cu")
    (tedit 0)
    (at 120.03 76 180)
    (descr "USB-A Male Plug - Through Hole, Right Angle")
    (property "Sheetfile" "File: usbtiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -0.25 -8 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "USB_A" (at 7.62 8 180 unlocked) (layer "F.Fab"))
    (fp_text user "pcb edge" (at 3.75 0.5 90 unlocked) (layer "Dwgs.User"))
    (fp_text user "${REFERENCE}" (at -0.275 -8 180 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -0.275 2.25 270) (size 1.1 1.1) (drill 1.1) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.275 -2.25 270) (size 1.1 1.1) (drill 1.1) (layers F&B.Cu *.Mask))
    (pad "1" thru_hole circle (at -2.275 -3.5 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 2 "VBUS") (pinfunction "VBUS") (pintype "power_in"))
    (pad "2" thru_hole circle (at -2.275 -1 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad2)") (pinfunction "D-") (pintype "bidirectional"))
    (pad "3" thru_hole circle (at -2.275 1 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad3)") (pinfunction "D+") (pintype "bidirectional"))
    (pad "4" thru_hole circle (at -2.275 3.5 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole oval (at -0.275 5.85 270) (size 2 3.2) (drill oval 1 2.2) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "5" thru_hole oval (at -0.275 -5.85 270) (size 2 3.2) (drill oval 1 2.2) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (model "${UPL_DIR}/3dmodels/UPL-Connectors.3dshapes/USB_A_Plug_CUIDevices_UP2-AH-1-TH.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 126 77)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: usbtiny.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 2.4 0.2 180) (layer "F.SilkS"))
    (fp_text value "680" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(J1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(R2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 129 72 -135)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: usbtiny.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at -2.163747 0.721249 180) (layer "F.SilkS"))
    (fp_text value "TBD" (at 0 1.43 45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 225) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 225) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(R4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 125.25 81.5 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: usbtiny.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0.5 1.35 90) (layer "F.SilkS"))
    (fp_text value "4.7uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VBUS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "B.Cu")
    (tedit 5B391E66)
    (at 135.75 79)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "File: usbtiny.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP2" (at 3.25 0) (layer "B.SilkS"))
    (fp_text value "PWR" (at 0 -1.9) (layer "B.Fab"))
    (pad "1" smd custom (at -0.65 0) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 2 "VBUS") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0.5 -0.75)
            (xy 0 -0.75)
            (xy 0 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 9 "Net-(J2-Pad2)") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0 -0.75)
            (xy -0.5 -0.75)
            (xy -0.5 0.75)
            (xy 0 0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "kibuzzard-631E71F9" (layer "B.Cu")
    (tedit 631E71F9)
    (at 130.4 79 180)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJGcmVkb2thT25lIiwgIkhlaWdodEN0cmwiOiAiMS4yNSIsICJMYXllckNvbWJvQm94IjogIkYuU2lsa1MiLCAiTXVsdGlMaW5lVGV4dCI6ICI1ViBFTiIsICJQYWRkaW5nQm90dG9tQ3RybCI6ICIyIiwgIlBhZGRpbmdMZWZ0Q3RybCI6ICIwIiwgIlBhZGRpbmdSaWdodEN0cmwiOiAiMCIsICJQYWRkaW5nVG9wQ3RybCI6ICIyIiwgIldpZHRoQ3RybCI6ICIxLjUifQ==")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-631E71F9" (at 0 3.960482) (layer "B.SilkS") hide)
    (fp_text value "G***" (at 0 -3.960482) (layer "B.SilkS") hide)
  )
  (footprint "kibuzzard-631E71DC" (layer "B.Cu")
    (tedit 631E71DC)
    (at 130.4 73 180)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJGcmVkb2thT25lIiwgIkhlaWdodEN0cmwiOiAiMS4yNSIsICJMYXllckNvbWJvQm94IjogIkYuU2lsa1MiLCAiTXVsdGlMaW5lVGV4dCI6ICJQUkdNIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogIjIiLCAiUGFkZGluZ0xlZnRDdHJsIjogIjAiLCAiUGFkZGluZ1JpZ2h0Q3RybCI6ICIwIiwgIlBhZGRpbmdUb3BDdHJsIjogIjIiLCAiV2lkdGhDdHJsIjogIjEuNSJ9")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-631E71DC" (at 0 3.963458) (layer "B.SilkS") hide)
    (fp_text value "G***" (at 0 -3.963458) (layer "B.SilkS") hide)
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "B.Cu")
    (tedit 5B391E66)
    (at 135.75 73)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "File: usbtiny.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP1" (at 3.17 0) (layer "B.SilkS"))
    (fp_text value "PRGM" (at 0 -1.9) (layer "B.Fab"))
    (pad "1" smd custom (at -0.65 0) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 12 "/SCS") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0.5 -0.75)
            (xy 0 -0.75)
            (xy 0 0.75)
            (xy 0.5 0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 13 "/~{Reset}") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0 -0.75)
            (xy -0.5 -0.75)
            (xy -0.5 0.75)
            (xy 0 0.75)
          ) (width 0) (fill yes))
      ))
  )
  (gr_arc (start 139.55 71.5) (mid 138.842893 71.207107) (end 138.55 70.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 145.84 71.5) (end 139.55 71.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 117.5 68.5) (end 117.5 83.5) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 146.84 79.5) (mid 146.547107 80.207107) (end 145.84 80.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 139.55 80.5) (end 145.84 80.5) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 138.55 82.5) (mid 138.257107 83.207107) (end 137.55 83.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 138.55 70.5) (end 138.55 69.5) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 138.55 81.5) (mid 138.842893 80.792893) (end 139.55 80.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 138.55 82.5) (end 138.55 81.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 117.5 68.5) (end 137.55 68.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 117.5 83.5) (end 137.55 83.5) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 145.84 71.5) (mid 146.547107 71.792893) (end 146.84 72.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 146.84 79.5) (end 146.84 72.5) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 137.55 68.5) (mid 138.257107 68.792893) (end 138.55 69.5) (layer "Edge.Cuts") (width 0.1))
  (gr_text "ATinyISP" (at 132.22 76) (layer "B.SilkS"))
  (gr_text "Ver 1.0" (at 133.4 70.2) (layer "B.SilkS"))
  (gr_text "October 2022" (at 137.71 82.27) (layer "B.SilkS"))
  (gr_text "Rex McKinnon" (at 132.4 81) (layer "B.SilkS"))
  (gr_text "ACT" (at 137.27 70.5 90) (layer "F.SilkS"))
  (gr_text " A\nTiny" (at 122.96 72.69 45) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.5 84.75)
        (xy 116.5 84.75)
        (xy 116.5 66.5)
        (xy 147.5 66.5)
      )
    )
  )
)
