(kicad_sch (version 20211123) (generator eeschema)
  (paper "USLetter")
  (title_block
    (title "ISP Programmer based on FabISP, USBTinyISP")
    (date "2022-10-22")
    (rev "1.0")
    (comment 2 "Designed by Rex McKinnon <0xff@rexploits.com>")
    (comment 3 "DEVELOPMENT")
  )
  (lib_symbols
    (symbol "Connector:AVR-ISP-6" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J?" (id 0) (at 9.525 2.5401 0))
      (property "Value" "AVR-ISP-6" (id 1) (at 9.525 0.0001 0))
      (property "Footprint" "" (id 2) (at 6.35 1.27 90))
      (property "Datasheet" " ~" (id 3) (at 32.385 -13.97 0))
      (property "ki_keywords" "AVR ISP Connector" (id 4) (at 0 0 0))
      (property "ki_description" "Atmel 6-pin ISP connector" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "IDC?Header*2x03* Pin?Header*2x03*" (id 6) (at 0 0 0))
      (symbol "AVR-ISP-6_0_1"
        (rectangle (start -2.667 -6.858) (end -2.413 -7.62)
          (fill (type none))
        )
        (rectangle (start -2.667 10.16) (end -2.413 9.398)
          (fill (type none))
        )
        (rectangle (start 7.62 -2.413) (end 6.858 -2.667)
          (fill (type none))
        )
        (rectangle (start 7.62 0.127) (end 6.858 -0.127)
          (fill (type none))
        )
        (rectangle (start 7.62 2.667) (end 6.858 2.413)
          (fill (type none))
        )
        (rectangle (start 7.62 5.207) (end 6.858 4.953)
          (fill (type none))
        )
        (rectangle (start 7.62 10.16) (end -7.62 -7.62)
          (fill (type background))
        )
      )
      (symbol "AVR-ISP-6_1_1"
        (pin passive line (at 10.16 2.54 180) (length 2.54)
          (name "MISO")
          (number "1")
        )
        (pin passive line (at -2.54 -10.16 90) (length 2.54)
          (name "VCC")
          (number "2")
        )
        (pin passive line (at 10.16 0 180) (length 2.54)
          (name "SCK")
          (number "3")
        )
        (pin passive line (at 10.16 5.08 180) (length 2.54)
          (name "MOSI")
          (number "4")
        )
        (pin passive line (at 10.16 -2.54 180) (length 2.54)
          (name "~{RST}")
          (number "5")
        )
        (pin passive line (at -2.54 12.7 270) (length 2.54)
          (name "GND")
          (number "6")
        )
      )
    )
    (symbol "Connector:USB_A" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J1" (id 0) (at 0 10.795 90))
      (property "Value" "USB_A" (id 1) (at 0 8.255 90))
      (property "Footprint" "UPL-Connectors:USB_A_Plug_CUIDevices_UP2-AH-1-TH" (id 2) (at 1.27 -3.81 0))
      (property "Datasheet" " ~" (id 3) (at 1.27 -3.81 0))
      (property "ki_keywords" "connector USB" (id 4) (at 0 0 0))
      (property "ki_description" "USB Type A connector" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "USB*" (id 6) (at 0 0 0))
      (symbol "USB_A_0_1"
        (rectangle (start -5.08 -7.62) (end 5.08 7.62)
          (fill (type background))
        )
        (circle (center -3.81 2.159) (radius 0.635)
          (fill (type outline))
        )
        (rectangle (start -1.524 4.826) (end -4.318 5.334)
          (fill (type outline))
        )
        (rectangle (start -1.27 4.572) (end -4.572 5.842)
          (fill (type none))
        )
        (circle (center -0.635 3.429) (radius 0.381)
          (fill (type outline))
        )
        (rectangle (start -0.127 -7.62) (end 0.127 -6.858)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.175 2.159)
            (xy -2.54 2.159)
            (xy -1.27 3.429)
            (xy -0.635 3.429)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 2.159)
            (xy -1.905 2.159)
            (xy -1.27 0.889)
            (xy 0 0.889)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 2.794)
            (xy 0.635 1.524)
            (xy 1.905 2.159)
            (xy 0.635 2.794)
          )
          (fill (type outline))
        )
        (rectangle (start 0.254 1.27) (end -0.508 0.508)
          (fill (type outline))
        )
        (rectangle (start 5.08 -2.667) (end 4.318 -2.413)
          (fill (type none))
        )
        (rectangle (start 5.08 -0.127) (end 4.318 0.127)
          (fill (type none))
        )
        (rectangle (start 5.08 4.953) (end 4.318 5.207)
          (fill (type none))
        )
      )
      (symbol "USB_A_1_1"
        (polyline
          (pts
            (xy -1.905 2.159)
            (xy 0.635 2.159)
          )
          (fill (type none))
        )
        (pin power_in line (at 7.62 5.08 180) (length 2.54)
          (name "VBUS")
          (number "1")
        )
        (pin bidirectional line (at 7.62 0 180) (length 2.54)
          (name "D-")
          (number "2")
        )
        (pin bidirectional line (at 7.62 -2.54 180) (length 2.54)
          (name "D+")
          (number "3")
        )
        (pin power_in line (at 0 -10.16 90) (length 2.54)
          (name "GND")
          (number "4")
        )
        (pin passive line (at -2.54 -10.16 90) (length 2.54)
          (name "Shield")
          (number "5")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:C_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.254 1.778 0))
      (property "Value" "C_Small" (id 1) (at 0.254 -2.032 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "capacitor cap" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_Small_0_1"
        (polyline
          (pts
            (xy -1.524 -0.508)
            (xy 1.524 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.524 0.508)
            (xy 1.524 0.508)
          )
          (fill (type none))
        )
      )
      (symbol "C_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 2.032)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 2.032)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:Crystal_GND24" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Y" (id 0) (at 3.175 5.08 0))
      (property "Value" "Crystal_GND24" (id 1) (at 3.175 3.175 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "quartz ceramic resonator oscillator" (id 4) (at 0 0 0))
      (property "ki_description" "Four pin crystal, GND on pins 2 and 4" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Crystal*" (id 6) (at 0 0 0))
      (symbol "Crystal_GND24_0_1"
        (rectangle (start -1.143 2.54) (end 1.143 -2.54)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 0)
            (xy -2.032 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 -1.27)
            (xy -2.032 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -3.81)
            (xy 0 -3.556)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 3.556)
            (xy 0 3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.032 -1.27)
            (xy 2.032 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.032 0)
            (xy 2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -2.286)
            (xy -2.54 -3.556)
            (xy 2.54 -3.556)
            (xy 2.54 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 2.286)
            (xy -2.54 3.556)
            (xy 2.54 3.556)
            (xy 2.54 2.286)
          )
          (fill (type none))
        )
      )
      (symbol "Crystal_GND24_1_1"
        (pin passive line (at -3.81 0 0) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at 0 5.08 270) (length 1.27)
          (name "2")
          (number "2")
        )
        (pin passive line (at 3.81 0 180) (length 1.27)
          (name "3")
          (number "3")
        )
        (pin passive line (at 0 -5.08 90) (length 1.27)
          (name "4")
          (number "4")
        )
      )
    )
    (symbol "Device:LED" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "LED" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "LED diode" (id 4) (at 0 0 0))
      (property "ki_description" "Light emitting diode" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (id 6) (at 0 0 0))
      (symbol "LED_0_1"
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy -1.27 0)
            (xy 1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.048 -0.762)
            (xy -4.572 -2.286)
            (xy -3.81 -2.286)
            (xy -4.572 -2.286)
            (xy -4.572 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 -0.762)
            (xy -3.302 -2.286)
            (xy -2.54 -2.286)
            (xy -3.302 -2.286)
            (xy -3.302 -1.524)
          )
          (fill (type none))
        )
      )
      (symbol "LED_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Jumper:SolderJumper_2_Open" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "JP" (id 0) (at 0 2.032 0))
      (property "Value" "SolderJumper_2_Open" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "solder jumper SPST" (id 4) (at 0 0 0))
      (property "ki_description" "Solder Jumper, 2-pole, open" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SolderJumper*Open*" (id 6) (at 0 0 0))
      (symbol "SolderJumper_2_Open_0_1"
        (arc (start -0.254 1.016) (mid -1.27 0) (end -0.254 -1.016)
          (fill (type none))
        )
        (arc (start -0.254 1.016) (mid -1.27 0) (end -0.254 -1.016)
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -0.254 1.016)
            (xy -0.254 -1.016)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.254 1.016)
            (xy 0.254 -1.016)
          )
          (fill (type none))
        )
        (arc (start 0.254 -1.016) (mid 1.27 0) (end 0.254 1.016)
          (fill (type none))
        )
        (arc (start 0.254 -1.016) (mid 1.27 0) (end 0.254 1.016)
          (fill (type outline))
        )
      )
      (symbol "SolderJumper_2_Open_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "A")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "B")
          (number "2")
        )
      )
    )
    (symbol "MCU_Microchip_ATtiny:ATtiny44V-10M" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -12.7 21.59 0))
      (property "Value" "ATtiny44V-10M" (id 1) (at 2.54 -21.59 0))
      (property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm" (id 2) (at 0 0 0))
      (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "AVR 8bit Microcontroller tinyAVR" (id 4) (at 0 0 0))
      (property "ki_description" "10MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, QFN-20" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*" (id 6) (at 0 0 0))
      (symbol "ATtiny44V-10M_0_1"
        (rectangle (start -12.7 -20.32) (end 12.7 20.32)
          (fill (type background))
        )
      )
      (symbol "ATtiny44V-10M_1_1"
        (pin bidirectional line (at 15.24 5.08 180) (length 2.54)
          (name "PA4")
          (number "1")
        )
        (pin no_connect line (at -12.7 -10.16 0) (length 2.54) hide
          (name "NC")
          (number "10")
        )
        (pin bidirectional line (at 15.24 -7.62 180) (length 2.54)
          (name "XTAL1/PB0")
          (number "11")
        )
        (pin bidirectional line (at 15.24 -10.16 180) (length 2.54)
          (name "XTAL2/PB1")
          (number "12")
        )
        (pin bidirectional line (at 15.24 -15.24 180) (length 2.54)
          (name "~{RESET}/PB3")
          (number "13")
        )
        (pin bidirectional line (at 15.24 -12.7 180) (length 2.54)
          (name "PB2")
          (number "14")
        )
        (pin bidirectional line (at 15.24 -2.54 180) (length 2.54)
          (name "PA7")
          (number "15")
        )
        (pin bidirectional line (at 15.24 0 180) (length 2.54)
          (name "PA6")
          (number "16")
        )
        (pin no_connect line (at -12.7 -12.7 0) (length 2.54) hide
          (name "NC")
          (number "17")
        )
        (pin no_connect line (at -12.7 -15.24 0) (length 2.54) hide
          (name "NC")
          (number "18")
        )
        (pin no_connect line (at -12.7 -17.78 0) (length 2.54) hide
          (name "NC")
          (number "19")
        )
        (pin bidirectional line (at 15.24 7.62 180) (length 2.54)
          (name "PA3")
          (number "2")
        )
        (pin bidirectional line (at 15.24 2.54 180) (length 2.54)
          (name "PA5")
          (number "20")
        )
        (pin passive line (at 0 -22.86 90) (length 2.54) hide
          (name "GND")
          (number "21")
        )
        (pin bidirectional line (at 15.24 10.16 180) (length 2.54)
          (name "PA2")
          (number "3")
        )
        (pin bidirectional line (at 15.24 12.7 180) (length 2.54)
          (name "PA1")
          (number "4")
        )
        (pin bidirectional line (at 15.24 15.24 180) (length 2.54)
          (name "AREF/PA0")
          (number "5")
        )
        (pin no_connect line (at -12.7 -5.08 0) (length 2.54) hide
          (name "NC")
          (number "6")
        )
        (pin no_connect line (at -12.7 -7.62 0) (length 2.54) hide
          (name "NC")
          (number "7")
        )
        (pin power_in line (at 0 -22.86 90) (length 2.54)
          (name "GND")
          (number "8")
        )
        (pin power_in line (at 0 22.86 270) (length 2.54)
          (name "VCC")
          (number "9")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
    (symbol "power:VBUS" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "VBUS" (id 1) (at 0 3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"VBUS\"" (id 5) (at 0 0 0))
      (symbol "VBUS_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "VBUS_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "VBUS")
          (number "1")
        )
      )
    )
  )
  (junction (at 67.945 90.17) (diameter 0) (color 0 0 0 0))
  (junction (at 152.4 125.095) (diameter 0) (color 0 0 0 0))
  (junction (at 170.18 111.125) (diameter 0) (color 0 0 0 0))
  (junction (at 149.225 79.375) (diameter 0) (color 0 0 0 0))
  (junction (at 131.445 90.17) (diameter 0) (color 0 0 0 0))
  (junction (at 131.445 103.505) (diameter 0) (color 0 0 0 0))
  (junction (at 98.425 90.17) (diameter 0) (color 0 0 0 0))
  (junction (at 79.375 90.17) (diameter 0) (color 0 0 0 0))
  (junction (at 132.715 121.285) (diameter 0) (color 0 0 0 0))
  (junction (at 73.66 100.33) (diameter 0) (color 0 0 0 0))
  (junction (at 132.715 128.905) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 113.665 111.125) (xy 170.18 111.125)))
  (wire (pts (xy 73.66 102.87) (xy 73.66 100.33)))
  (wire (pts (xy 152.4 121.285) (xy 152.4 125.095)))
  (wire (pts (xy 79.375 100.33) (xy 79.375 97.79)))
  (wire (pts (xy 132.715 128.905) (xy 139.7 128.905)))
  (wire (pts (xy 79.375 90.17) (xy 98.425 90.17)))
  (wire (pts (xy 67.945 100.33) (xy 73.66 100.33)))
  (wire (pts (xy 113.665 116.205) (xy 175.26 116.205)))
  (wire (pts (xy 139.065 106.045) (xy 139.065 86.995)))
  (wire (pts (xy 63.5 90.17) (xy 67.945 90.17)))
  (wire (pts (xy 113.665 133.985) (xy 170.18 133.985)))
  (wire (pts (xy 149.225 108.585) (xy 151.765 108.585)))
  (wire (pts (xy 98.425 144.145) (xy 98.425 141.605)))
  (wire (pts (xy 113.665 113.665) (xy 175.26 113.665)))
  (wire (pts (xy 136.525 103.505) (xy 136.525 86.995)))
  (wire (pts (xy 113.665 118.745) (xy 175.26 118.745)))
  (wire (pts (xy 187.96 90.805) (xy 187.96 93.345)))
  (wire (pts (xy 131.445 103.505) (xy 136.525 103.505)))
  (wire (pts (xy 113.665 106.045) (xy 117.475 106.045)))
  (wire (pts (xy 170.18 131.445) (xy 170.18 133.985)))
  (wire (pts (xy 113.665 126.365) (xy 122.555 126.365)))
  (wire (pts (xy 144.78 128.905) (xy 152.4 128.905)))
  (wire (pts (xy 122.555 121.285) (xy 122.555 126.365)))
  (wire (pts (xy 67.945 97.79) (xy 67.945 100.33)))
  (wire (pts (xy 122.555 121.285) (xy 132.715 121.285)))
  (wire (pts (xy 131.445 86.995) (xy 131.445 90.17)))
  (wire (pts (xy 159.385 108.585) (xy 161.925 108.585)))
  (wire (pts (xy 113.665 103.505) (xy 117.475 103.505)))
  (wire (pts (xy 149.225 79.375) (xy 149.225 81.915)))
  (wire (pts (xy 113.665 128.905) (xy 132.715 128.905)))
  (wire (pts (xy 170.18 111.125) (xy 170.18 123.825)))
  (wire (pts (xy 125.095 103.505) (xy 131.445 103.505)))
  (wire (pts (xy 146.685 76.835) (xy 149.225 76.835)))
  (wire (pts (xy 98.425 95.885) (xy 98.425 90.17)))
  (wire (pts (xy 67.945 90.17) (xy 79.375 90.17)))
  (wire (pts (xy 131.445 100.33) (xy 131.445 103.505)))
  (wire (pts (xy 187.96 126.365) (xy 187.96 128.905)))
  (wire (pts (xy 73.66 100.33) (xy 79.375 100.33)))
  (wire (pts (xy 149.225 76.835) (xy 149.225 79.375)))
  (wire (pts (xy 132.715 121.285) (xy 139.7 121.285)))
  (wire (pts (xy 187.96 100.965) (xy 187.96 103.505)))
  (wire (pts (xy 152.4 125.095) (xy 154.94 125.095)))
  (wire (pts (xy 131.445 90.17) (xy 131.445 92.71)))
  (wire (pts (xy 170.18 111.125) (xy 175.26 111.125)))
  (wire (pts (xy 125.095 106.045) (xy 139.065 106.045)))
  (wire (pts (xy 113.665 108.585) (xy 141.605 108.585)))
  (wire (pts (xy 152.4 125.095) (xy 152.4 128.905)))
  (wire (pts (xy 146.685 79.375) (xy 149.225 79.375)))
  (wire (pts (xy 98.425 90.17) (xy 131.445 90.17)))
  (wire (pts (xy 144.78 121.285) (xy 152.4 121.285)))
  (label "MOSI" (at 116.84 118.745 0))
  (label "~{Reset}" (at 116.84 133.985 0))
  (label "SCS" (at 116.84 111.125 0))
  (label "SCK" (at 116.84 113.665 0))
  (label "MISO" (at 116.84 116.205 0))
  (symbol (lib_id "power:GND") (at 137.795 125.095 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR07" (id 0) (at 144.145 125.095 0))
    (property "Value" "GND" (id 1) (at 140.97 125.0951 90))
    (property "Footprint" "" (id 2) (at 137.795 125.095 0))
    (property "Datasheet" "" (id 3) (at 137.795 125.095 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 187.96 128.905 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR09" (id 0) (at 187.96 135.255 0))
    (property "Value" "GND" (id 1) (at 187.96 133.985 0))
    (property "Footprint" "" (id 2) (at 187.96 128.905 0))
    (property "Datasheet" "" (id 3) (at 187.96 128.905 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 145.415 108.585 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R4" (id 0) (at 140.97 107.315 90))
    (property "Value" "TBD" (id 1) (at 145.415 108.585 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 145.415 106.807 90))
    (property "Datasheet" "~" (id 3) (at 145.415 108.585 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 149.225 81.915 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR01" (id 0) (at 149.225 88.265 0))
    (property "Value" "GND" (id 1) (at 149.225 86.36 0))
    (property "Footprint" "" (id 2) (at 149.225 81.915 0))
    (property "Datasheet" "" (id 3) (at 149.225 81.915 0))
    (pin "1")
  )
  (symbol (lib_id "Jumper:SolderJumper_2_Open") (at 170.18 127.635 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "JP1" (id 0) (at 168.275 127.635 90))
    (property "Value" "PRGM" (id 1) (at 172.085 127.635 90))
    (property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (id 2) (at 170.18 127.635 0))
    (property "Datasheet" "~" (id 3) (at 170.18 127.635 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:AVR-ISP-6") (at 185.42 113.665 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J2" (id 0) (at 178.435 104.775 0))
    (property "Value" "AVR-ISP-6" (id 1) (at 194.945 113.665 90))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Horizontal" (id 2) (at 179.07 114.935 90))
    (property "Datasheet" " ~" (id 3) (at 153.035 99.695 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
  )
  (symbol (lib_id "Device:R") (at 131.445 96.52 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R1" (id 0) (at 130.175 94.488 0))
    (property "Value" "1K5" (id 1) (at 131.445 96.52 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 129.667 96.52 90))
    (property "Datasheet" "~" (id 3) (at 131.445 96.52 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Jumper:SolderJumper_2_Open") (at 187.96 97.155 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "JP2" (id 0) (at 186.055 97.155 90))
    (property "Value" "PWR" (id 1) (at 189.865 97.155 90))
    (property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (id 2) (at 187.96 97.155 0))
    (property "Datasheet" "~" (id 3) (at 187.96 97.155 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 121.285 103.505 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R2" (id 0) (at 118.11 103.505 90))
    (property "Value" "680" (id 1) (at 121.285 103.505 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 121.285 101.727 90))
    (property "Datasheet" "~" (id 3) (at 121.285 103.505 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 67.945 93.98 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C1" (id 0) (at 68.58 91.44 0))
    (property "Value" "4.7uF" (id 1) (at 68.58 96.52 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 66.9798 90.17 0))
    (property "Datasheet" "~" (id 3) (at 67.945 93.98 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 142.24 121.285 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C3" (id 0) (at 144.78 120.015 90))
    (property "Value" "TBD" (id 1) (at 147.32 122.555 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 142.24 121.285 0))
    (property "Datasheet" "~" (id 3) (at 142.24 121.285 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 154.94 125.095 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR08" (id 0) (at 161.29 125.095 0))
    (property "Value" "GND" (id 1) (at 160.02 125.095 0))
    (property "Footprint" "" (id 2) (at 154.94 125.095 0))
    (property "Datasheet" "" (id 3) (at 154.94 125.095 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:USB_A") (at 136.525 79.375 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J1" (id 0) (at 129.54 73.025 90))
    (property "Value" "USB_A" (id 1) (at 141.605 73.025 90))
    (property "Footprint" "UPL-Connectors:USB_A_Plug_CUIDevices_UP2-AH-1-TH" (id 2) (at 140.335 80.645 0))
    (property "Datasheet" " ~" (id 3) (at 140.335 80.645 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:R") (at 121.285 106.045 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R3" (id 0) (at 118.11 106.045 90))
    (property "Value" "680" (id 1) (at 121.285 106.045 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 121.285 104.267 90))
    (property "Datasheet" "~" (id 3) (at 121.285 106.045 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:VBUS") (at 63.5 90.17 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR02" (id 0) (at 67.31 90.17 0))
    (property "Value" "VBUS" (id 1) (at 60.325 90.1699 90))
    (property "Footprint" "" (id 2) (at 63.5 90.17 0))
    (property "Datasheet" "" (id 3) (at 63.5 90.17 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 98.425 144.145 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR010" (id 0) (at 98.425 150.495 0))
    (property "Value" "GND" (id 1) (at 98.425 148.59 0))
    (property "Footprint" "" (id 2) (at 98.425 144.145 0))
    (property "Datasheet" "" (id 3) (at 98.425 144.145 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C_Small") (at 142.24 128.905 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C4" (id 0) (at 144.78 127.635 90))
    (property "Value" "TBD" (id 1) (at 147.32 130.175 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 142.24 128.905 0))
    (property "Datasheet" "~" (id 3) (at 142.24 128.905 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 73.66 102.87 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR04" (id 0) (at 73.66 109.22 0))
    (property "Value" "GND" (id 1) (at 73.66 106.045 0))
    (property "Footprint" "" (id 2) (at 73.66 102.87 0))
    (property "Datasheet" "" (id 3) (at 73.66 102.87 0))
    (pin "1")
  )
  (symbol (lib_id "power:VBUS") (at 187.96 90.805 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR03" (id 0) (at 187.96 94.615 0))
    (property "Value" "VBUS" (id 1) (at 187.96 85.725 0))
    (property "Footprint" "" (id 2) (at 187.96 90.805 0))
    (property "Datasheet" "" (id 3) (at 187.96 90.805 0))
    (pin "1")
  )
  (symbol (lib_id "MCU_Microchip_ATtiny:ATtiny44V-10M") (at 98.425 118.745 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U1" (id 0) (at 84.455 117.4749 0))
    (property "Value" "ATtiny44V-15MT" (id 1) (at 84.455 120.0149 0))
    (property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm" (id 2) (at 98.425 118.745 0))
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf" (id 3) (at 98.425 118.745 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "power:GND") (at 161.925 108.585 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR05" (id 0) (at 168.275 108.585 0))
    (property "Value" "GND" (id 1) (at 165.735 108.5849 90))
    (property "Footprint" "" (id 2) (at 161.925 108.585 0))
    (property "Datasheet" "" (id 3) (at 161.925 108.585 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 79.375 93.98 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C2" (id 0) (at 80.01 91.44 0))
    (property "Value" "0.1uF" (id 1) (at 80.01 96.52 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 80.3402 97.79 0))
    (property "Datasheet" "~" (id 3) (at 79.375 93.98 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 127.635 125.095 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR06" (id 0) (at 121.285 125.095 0))
    (property "Value" "GND" (id 1) (at 124.46 125.0949 90))
    (property "Footprint" "" (id 2) (at 127.635 125.095 0))
    (property "Datasheet" "" (id 3) (at 127.635 125.095 0))
    (pin "1")
  )
  (symbol (lib_id "Device:Crystal_GND24") (at 132.715 125.095 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Y1" (id 0) (at 130.175 120.015 90))
    (property "Value" ">12MHz" (id 1) (at 132.715 130.81 90))
    (property "Footprint" "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm" (id 2) (at 132.715 125.095 0))
    (property "Datasheet" "~" (id 3) (at 132.715 125.095 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "Device:LED") (at 155.575 108.585 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D1" (id 0) (at 152.4 107.315 0))
    (property "Value" "Blue" (id 1) (at 159.385 109.855 0))
    (property "Footprint" "LED_SMD:LED_0603_1608Metric" (id 2) (at 155.575 108.585 0))
    (property "Datasheet" "~" (id 3) (at 155.575 108.585 0))
    (pin "1")
    (pin "2")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#PWR01") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR02") (unit 1) (value "VBUS") (footprint "")
    )
    (path
      (reference "#PWR03") (unit 1) (value "VBUS") (footprint "")
    )
    (path
      (reference "#PWR04") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR05") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR06") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR07") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR08") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR09") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR010") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "C1") (unit 1) (value "4.7uF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C2") (unit 1) (value "0.1uF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C3") (unit 1) (value "TBD") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C4") (unit 1) (value "TBD") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "D1") (unit 1) (value "Blue") (footprint "LED_SMD:LED_0603_1608Metric")
    )
    (path
      (reference "J1") (unit 1) (value "USB_A") (footprint "UPL-Connectors:USB_A_Plug_CUIDevices_UP2-AH-1-TH")
    )
    (path
      (reference "J2") (unit 1) (value "AVR-ISP-6") (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Horizontal")
    )
    (path
      (reference "JP1") (unit 1) (value "PRGM") (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm")
    )
    (path
      (reference "JP2") (unit 1) (value "PWR") (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm")
    )
    (path
      (reference "R1") (unit 1) (value "1K5") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R2") (unit 1) (value "680") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R3") (unit 1) (value "680") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R4") (unit 1) (value "TBD") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "U1") (unit 1) (value "ATtiny44V-15MT") (footprint "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm")
    )
    (path
      (reference "Y1") (unit 1) (value ">12MHz") (footprint "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm")
    )
  )
)
