(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (grid_origin 133.8 123)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Fabrication outputs/")
    )
  )
  (net 0 "")
  (net 1 "/CHAN_0_IN")
  (net 2 "/CHAN_1_IN")
  (net 3 "/CHAN_2_IN")
  (net 4 "/CHAN_3_IN")
  (net 5 "/CHAN_4_IN")
  (net 6 "/CHAN_5_IN")
  (net 7 "/CHAN_6_IN")
  (net 8 "/CHAN_7_IN")
  (net 9 "/CHAN_8_IN")
  (net 10 "/CHAN_9_IN")
  (net 11 "/CHAN_10_IN")
  (net 12 "/CHAN_11_IN")
  (net 13 "/GND")
  (net 14 "/3V3")
  (net 15 "/5V")
  (net 16 "/CHAN_0_OUT")
  (net 17 "/CHAN_1_OUT")
  (net 18 "/CHAN_2_OUT")
  (net 19 "/CHAN_3_OUT")
  (net 20 "/CHAN_4_OUT")
  (net 21 "/CHAN_5_OUT")
  (net 22 "/CHAN_6_OUT")
  (net 23 "/CHAN_7_OUT")
  (net 24 "/CHAN_8_OUT")
  (net 25 "/CHAN_9_OUT")
  (net 26 "/CHAN_10_OUT")
  (net 27 "/CHAN_11_OUT")
  (net 28 "unconnected-(U1-Pad6)")
  (net 29 "unconnected-(U1-Pad9)")
  (net 30 "unconnected-(U2-Pad6)")
  (net 31 "unconnected-(U2-Pad9)")
  (net 32 "unconnected-(U3-Pad6)")
  (net 33 "unconnected-(U3-Pad9)")
  (net 34 "/CHAN_23_IN")
  (net 35 "/CHAN_22_IN")
  (net 36 "/CHAN_21_IN")
  (net 37 "/CHAN_20_IN")
  (net 38 "/CHAN_19_IN")
  (net 39 "/CHAN_18_IN")
  (net 40 "/CHAN_17_IN")
  (net 41 "/CHAN_16_IN")
  (net 42 "/CHAN_15_IN")
  (net 43 "/CHAN_14_IN")
  (net 44 "/CHAN_13_IN")
  (net 45 "/CHAN_12_IN")
  (net 46 "/CHAN_23_OUT")
  (net 47 "/CHAN_22_OUT")
  (net 48 "/CHAN_21_OUT")
  (net 49 "/CHAN_20_OUT")
  (net 50 "/CHAN_19_OUT")
  (net 51 "/CHAN_18_OUT")
  (net 52 "/CHAN_17_OUT")
  (net 53 "/CHAN_16_OUT")
  (net 54 "/CHAN_15_OUT")
  (net 55 "/CHAN_14_OUT")
  (net 56 "/CHAN_13_OUT")
  (net 57 "/CHAN_12_OUT")
  (net 58 "unconnected-(U4-Pad6)")
  (net 59 "unconnected-(U4-Pad9)")
  (net 60 "unconnected-(U5-Pad6)")
  (net 61 "unconnected-(U5-Pad9)")
  (net 62 "unconnected-(U6-Pad6)")
  (net 63 "unconnected-(U6-Pad9)")
  (net 64 "/5V_VREF")
  (net 65 "/EXT_T")
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x15_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 5A19A41F)
    (at 149.895 80)
    (descr "Through hole angled socket strip, 2x15, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole angled socket strip THT 2x15 2.54mm double row")
    (property "Sheetfile" "LevelShifter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -5.65 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_02x15_Odd_Even" (at -5.65 38.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -8.315 17.78 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/CHAN_0_IN") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at -2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "/CHAN_23_IN") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "/CHAN_1_IN") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at -2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "/CHAN_22_IN") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/CHAN_2_IN") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at -2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "/CHAN_21_IN") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/CHAN_3_IN") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at -2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "/CHAN_20_IN") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "/CHAN_4_IN") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at -2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "/CHAN_19_IN") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/CHAN_5_IN") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at -2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "/CHAN_18_IN") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "/CHAN_6_IN") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at -2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "/CHAN_17_IN") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/CHAN_7_IN") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at -2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "/CHAN_16_IN") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/CHAN_8_IN") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at -2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "/CHAN_15_IN") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/CHAN_9_IN") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at -2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "/CHAN_14_IN") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/CHAN_10_IN") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval (at -2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "/CHAN_13_IN") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "/CHAN_11_IN") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole oval (at -2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "/CHAN_12_IN") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "/GND") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole oval (at -2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "/GND") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "/EXT_T") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole oval (at -2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "/3V3") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "/EXT_T") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole oval (at -2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "/5V_VREF") (pinfunction "Pin_30") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x15_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 163.995 108.8 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LevelShifter.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 2.3 0.1 180) (layer "F.SilkS"))
    (fp_text value "100nf 16v" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 159.595 108.7 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LevelShifter.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at -2.2 -0.195 180) (layer "F.SilkS"))
    (fp_text value "100nf 16v" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/5V_VREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TXU0104PWR" (layer "F.Cu")
    (tedit 0)
    (at 159.895 93.5)
    (property "Sheetfile" "LevelShifter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U6" (at 5.8 0) (layer "F.SilkS"))
    (fp_text value "TXU0104PWR" (at 0 4.2) (layer "F.SilkS") hide)
    (fp_text user "*" (at -3.20395 -3.447758) (layer "F.SilkS"))
    (fp_text user "*" (at -3.20395 -3.447758) (layer "F.SilkS"))
    (fp_text user "0.232in/5.9mm" (at 0 -4.9657) (layer "Cmts.User"))
    (fp_text user "0.055in/1.404mm" (at -2.94995 4.9657) (layer "Cmts.User"))
    (fp_text user "0.026in/0.65mm" (at -5.99795 -1.624965) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "0.014in/0.355mm" (at 5.99795 -1.949958) (layer "Cmts.User"))
    (fp_text user "*" (at -1.8669 -2.4765) (layer "F.Fab"))
    (fp_text user "*" (at -1.8669 -2.4765) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.949948 -1.949958) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/5V_VREF") (pinfunction "VCCA") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.949948 -1.299972) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "/CHAN_19_IN") (pinfunction "A1") (pintype "bidirectional"))
    (pad "3" smd rect locked (at -2.949948 -0.649986) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/CHAN_18_IN") (pinfunction "A2") (pintype "bidirectional"))
    (pad "4" smd rect locked (at -2.949948 0) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "/CHAN_17_IN") (pinfunction "A3") (pintype "bidirectional"))
    (pad "5" smd rect locked (at -2.949948 0.649986) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "/CHAN_16_IN") (pinfunction "A4") (pintype "bidirectional"))
    (pad "6" smd rect locked (at -2.949948 1.299972) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "unconnected-(U6-Pad6)") (pinfunction "NC") (pintype "no_connect"))
    (pad "7" smd rect locked (at -2.949948 1.949958) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" smd rect locked (at 2.949948 1.949958) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/3V3") (pinfunction "OE") (pintype "unspecified"))
    (pad "9" smd rect locked (at 2.949948 1.299972) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "unconnected-(U6-Pad9)") (pinfunction "NC") (pintype "no_connect"))
    (pad "10" smd rect locked (at 2.949948 0.649986) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "/CHAN_16_OUT") (pinfunction "B4Y") (pintype "bidirectional"))
    (pad "11" smd rect locked (at 2.949948 0) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "/CHAN_17_OUT") (pinfunction "B3Y") (pintype "bidirectional"))
    (pad "12" smd rect locked (at 2.949948 -0.649986) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "/CHAN_18_OUT") (pinfunction "B2Y") (pintype "bidirectional"))
    (pad "13" smd rect locked (at 2.949948 -1.299972) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "/CHAN_19_OUT") (pinfunction "B1Y") (pintype "bidirectional"))
    (pad "14" smd rect locked (at 2.949948 -1.949958) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/3V3") (pinfunction "VCCB") (pintype "power_in"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 159.795 87.9)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LevelShifter.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at -3.1 0) (layer "F.SilkS"))
    (fp_text value "100nf 16v" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/5V_VREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TXU0104PWR" (layer "F.Cu")
    (tedit 0)
    (at 159.895 104)
    (property "Sheetfile" "LevelShifter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U5" (at 5.8 0) (layer "F.SilkS"))
    (fp_text value "TXU0104PWR" (at 0 5.4) (layer "F.SilkS") hide)
    (fp_text user "*" (at -3.20395 -3.447758) (layer "F.SilkS"))
    (fp_text user "*" (at -3.20395 -3.447758) (layer "F.SilkS"))
    (fp_text user "0.055in/1.404mm" (at -2.94995 4.9657) (layer "Cmts.User"))
    (fp_text user "0.026in/0.65mm" (at -5.99795 -1.624965) (layer "Cmts.User"))
    (fp_text user "0.014in/0.355mm" (at 5.99795 -1.949958) (layer "Cmts.User"))
    (fp_text user "0.232in/5.9mm" (at 0 -4.9657) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "*" (at -1.8669 -2.4765) (layer "F.Fab"))
    (fp_text user "*" (at -1.8669 -2.4765) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.949948 -1.949958) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/5V_VREF") (pinfunction "VCCA") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.949948 -1.299972) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "/CHAN_15_IN") (pinfunction "A1") (pintype "bidirectional"))
    (pad "3" smd rect locked (at -2.949948 -0.649986) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "/CHAN_14_IN") (pinfunction "A2") (pintype "bidirectional"))
    (pad "4" smd rect locked (at -2.949948 0) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "/CHAN_13_IN") (pinfunction "A3") (pintype "bidirectional"))
    (pad "5" smd rect locked (at -2.949948 0.649986) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/CHAN_12_IN") (pinfunction "A4") (pintype "bidirectional"))
    (pad "6" smd rect locked (at -2.949948 1.299972) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "unconnected-(U5-Pad6)") (pinfunction "NC") (pintype "no_connect"))
    (pad "7" smd rect locked (at -2.949948 1.949958) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" smd rect locked (at 2.949948 1.949958) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/3V3") (pinfunction "OE") (pintype "unspecified"))
    (pad "9" smd rect locked (at 2.949948 1.299972) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "unconnected-(U5-Pad9)") (pinfunction "NC") (pintype "no_connect"))
    (pad "10" smd rect locked (at 2.949948 0.649986) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "/CHAN_12_OUT") (pinfunction "B4Y") (pintype "bidirectional"))
    (pad "11" smd rect locked (at 2.949948 0) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/CHAN_13_OUT") (pinfunction "B3Y") (pintype "bidirectional"))
    (pad "12" smd rect locked (at 2.949948 -0.649986) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/CHAN_14_OUT") (pinfunction "B2Y") (pintype "bidirectional"))
    (pad "13" smd rect locked (at 2.949948 -1.299972) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "/CHAN_15_OUT") (pinfunction "B1Y") (pintype "bidirectional"))
    (pad "14" smd rect locked (at 2.949948 -1.949958) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/3V3") (pinfunction "VCCB") (pintype "power_in"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 159.995 98)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LevelShifter.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at -3.3 0) (layer "F.SilkS"))
    (fp_text value "100nf 16v" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/5V_VREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x15_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 59FED5CB)
    (at 169.995 80)
    (descr "Through hole angled pin header, 2x15, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x15 2.54mm double row")
    (property "Sheetfile" "LevelShifter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 5.655 -2.27) (layer "F.SilkS"))
    (fp_text value "Conn_02x15_Odd_Even" (at 5.655 37.83) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.31 17.78 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/CHAN_0_OUT") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "/CHAN_23_OUT") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/CHAN_1_OUT") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "/CHAN_22_OUT") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "/CHAN_2_OUT") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "/CHAN_21_OUT") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/CHAN_3_OUT") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "/CHAN_20_OUT") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/CHAN_4_OUT") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "/CHAN_19_OUT") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/CHAN_5_OUT") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "/CHAN_18_OUT") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/CHAN_6_OUT") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "/CHAN_17_OUT") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "/CHAN_7_OUT") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "/CHAN_16_OUT") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "/CHAN_8_OUT") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "/CHAN_15_OUT") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "/CHAN_9_OUT") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "/CHAN_14_OUT") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "/CHAN_10_OUT") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval (at 2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "/CHAN_13_OUT") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "/CHAN_11_OUT") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole oval (at 2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "/CHAN_12_OUT") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "/GND") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole oval (at 2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "/GND") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "/EXT_T") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole oval (at 2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "/3V3") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "/EXT_T") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole oval (at 2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/5V") (pinfunction "Pin_30") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x15_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TXU0104PWR" (layer "F.Cu")
    (tedit 0)
    (at 159.895 83.5)
    (property "Sheetfile" "LevelShifter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U4" (at 5.9 0) (layer "F.SilkS"))
    (fp_text value "TXU0104PWR" (at 0 4.4) (layer "F.SilkS") hide)
    (fp_text user "*" (at -3.20395 -3.447758) (layer "F.SilkS"))
    (fp_text user "*" (at -3.20395 -3.447758) (layer "F.SilkS"))
    (fp_text user "0.055in/1.404mm" (at -2.94995 4.9657) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "0.014in/0.355mm" (at 5.99795 -1.949958) (layer "Cmts.User"))
    (fp_text user "0.232in/5.9mm" (at 0 -4.9657) (layer "Cmts.User"))
    (fp_text user "0.026in/0.65mm" (at -5.99795 -1.624965) (layer "Cmts.User"))
    (fp_text user "*" (at -1.8669 -2.4765) (layer "F.Fab"))
    (fp_text user "*" (at -1.8669 -2.4765) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.949948 -1.949958) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/5V_VREF") (pinfunction "VCCA") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.949948 -1.299972) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/CHAN_23_IN") (pinfunction "A1") (pintype "bidirectional"))
    (pad "3" smd rect locked (at -2.949948 -0.649986) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "/CHAN_22_IN") (pinfunction "A2") (pintype "bidirectional"))
    (pad "4" smd rect locked (at -2.949948 0) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "/CHAN_21_IN") (pinfunction "A3") (pintype "bidirectional"))
    (pad "5" smd rect locked (at -2.949948 0.649986) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "/CHAN_20_IN") (pinfunction "A4") (pintype "bidirectional"))
    (pad "6" smd rect locked (at -2.949948 1.299972) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "unconnected-(U4-Pad6)") (pinfunction "NC") (pintype "no_connect"))
    (pad "7" smd rect locked (at -2.949948 1.949958) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" smd rect locked (at 2.949948 1.949958) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/3V3") (pinfunction "OE") (pintype "unspecified"))
    (pad "9" smd rect locked (at 2.949948 1.299972) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "unconnected-(U4-Pad9)") (pinfunction "NC") (pintype "no_connect"))
    (pad "10" smd rect locked (at 2.949948 0.649986) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "/CHAN_20_OUT") (pinfunction "B4Y") (pintype "bidirectional"))
    (pad "11" smd rect locked (at 2.949948 0) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "/CHAN_21_OUT") (pinfunction "B3Y") (pintype "bidirectional"))
    (pad "12" smd rect locked (at 2.949948 -0.649986) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "/CHAN_22_OUT") (pinfunction "B2Y") (pintype "bidirectional"))
    (pad "13" smd rect locked (at 2.949948 -1.299972) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/CHAN_23_OUT") (pinfunction "B1Y") (pintype "bidirectional"))
    (pad "14" smd rect locked (at 2.949948 -1.949958) (size 1.404099 0.3548) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/3V3") (pinfunction "VCCB") (pintype "power_in"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 161.9 115.5 -90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "LevelShifter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "JP1" (at 0 -2.33 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 0 4.87 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "/5V_VREF") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 160.995 99.8 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LevelShifter.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at -2.6 -0.2) (layer "F.SilkS"))
    (fp_text value "100nf 16v" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 160.795 89.5 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LevelShifter.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at -3.1 0) (layer "F.SilkS"))
    (fp_text value "100nf 16v" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 160.095 87.8)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LevelShifter.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at -2.5 0) (layer "B.SilkS"))
    (fp_text value "100nf 16v" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "/GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 64 "/5V_VREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TXU0104PWR" (layer "B.Cu")
    (tedit 0)
    (at 159.895 83.5)
    (property "Sheetfile" "LevelShifter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at -5.2 0) (layer "B.SilkS"))
    (fp_text value "TXU0104PWR" (at 0 4.2) (layer "B.SilkS") hide)
    (fp_text user "*" (at -3.20395 3.447758) (layer "B.SilkS"))
    (fp_text user "*" (at -3.20395 3.447758) (layer "B.SilkS"))
    (fp_text user "0.026in/0.65mm" (at -5.99795 1.624965) (layer "Cmts.User"))
    (fp_text user "0.014in/0.355mm" (at 5.99795 1.949958) (layer "Cmts.User"))
    (fp_text user "0.232in/5.9mm" (at 0 4.9657) (layer "Cmts.User"))
    (fp_text user "0.055in/1.404mm" (at -2.94995 -4.9657) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "*" (at -1.8669 2.4765) (layer "B.Fab"))
    (fp_text user "*" (at -1.8669 2.4765) (layer "B.Fab"))
    (pad "1" smd rect locked (at -2.949948 1.949958) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 64 "/5V_VREF") (pinfunction "VCCA") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.949948 1.299972) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "/CHAN_3_IN") (pinfunction "A1") (pintype "bidirectional"))
    (pad "3" smd rect locked (at -2.949948 0.649986) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "/CHAN_2_IN") (pinfunction "A2") (pintype "bidirectional"))
    (pad "4" smd rect locked (at -2.949948 0) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "/CHAN_1_IN") (pinfunction "A3") (pintype "bidirectional"))
    (pad "5" smd rect locked (at -2.949948 -0.649986) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "/CHAN_0_IN") (pinfunction "A4") (pintype "bidirectional"))
    (pad "6" smd rect locked (at -2.949948 -1.299972) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "unconnected-(U2-Pad6)") (pinfunction "NC") (pintype "no_connect"))
    (pad "7" smd rect locked (at -2.949948 -1.949958) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "/GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" smd rect locked (at 2.949948 -1.949958) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "/3V3") (pinfunction "OE") (pintype "unspecified"))
    (pad "9" smd rect locked (at 2.949948 -1.299972) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "unconnected-(U2-Pad9)") (pinfunction "NC") (pintype "no_connect"))
    (pad "10" smd rect locked (at 2.949948 -0.649986) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "/CHAN_0_OUT") (pinfunction "B4Y") (pintype "bidirectional"))
    (pad "11" smd rect locked (at 2.949948 0) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "/CHAN_1_OUT") (pinfunction "B3Y") (pintype "bidirectional"))
    (pad "12" smd rect locked (at 2.949948 0.649986) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "/CHAN_2_OUT") (pinfunction "B2Y") (pintype "bidirectional"))
    (pad "13" smd rect locked (at 2.949948 1.299972) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "/CHAN_3_OUT") (pinfunction "B1Y") (pintype "bidirectional"))
    (pad "14" smd rect locked (at 2.949948 1.949958) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "/3V3") (pinfunction "VCCB") (pintype "power_in"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 159.895 107.7)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LevelShifter.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at -3 0.5) (layer "B.SilkS"))
    (fp_text value "100nf 16v" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "/GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 64 "/5V_VREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 159.995 97.8)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LevelShifter.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at -2.4 0.1) (layer "B.SilkS"))
    (fp_text value "100nf 16v" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "/GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 64 "/5V_VREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TXU0104PWR" (layer "B.Cu")
    (tedit 0)
    (at 159.895 104)
    (property "Sheetfile" "LevelShifter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at -5.3 0) (layer "B.SilkS"))
    (fp_text value "TXU0104PWR" (at 0 5.6) (layer "B.SilkS") hide)
    (fp_text user "*" (at -3.20395 3.447758) (layer "B.SilkS"))
    (fp_text user "*" (at -3.20395 3.447758) (layer "B.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "0.014in/0.355mm" (at 5.99795 1.949958) (layer "Cmts.User"))
    (fp_text user "0.232in/5.9mm" (at 0 4.9657) (layer "Cmts.User"))
    (fp_text user "0.055in/1.404mm" (at -2.94995 -4.9657) (layer "Cmts.User"))
    (fp_text user "0.026in/0.65mm" (at -5.99795 1.624965) (layer "Cmts.User"))
    (fp_text user "*" (at -1.8669 2.4765) (layer "B.Fab"))
    (fp_text user "*" (at -1.8669 2.4765) (layer "B.Fab"))
    (pad "1" smd rect locked (at -2.949948 1.949958) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 64 "/5V_VREF") (pinfunction "VCCA") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.949948 1.299972) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "/CHAN_11_IN") (pinfunction "A1") (pintype "bidirectional"))
    (pad "3" smd rect locked (at -2.949948 0.649986) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "/CHAN_10_IN") (pinfunction "A2") (pintype "bidirectional"))
    (pad "4" smd rect locked (at -2.949948 0) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "/CHAN_9_IN") (pinfunction "A3") (pintype "bidirectional"))
    (pad "5" smd rect locked (at -2.949948 -0.649986) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "/CHAN_8_IN") (pinfunction "A4") (pintype "bidirectional"))
    (pad "6" smd rect locked (at -2.949948 -1.299972) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "unconnected-(U1-Pad6)") (pinfunction "NC") (pintype "no_connect"))
    (pad "7" smd rect locked (at -2.949948 -1.949958) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "/GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" smd rect locked (at 2.949948 -1.949958) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "/3V3") (pinfunction "OE") (pintype "unspecified"))
    (pad "9" smd rect locked (at 2.949948 -1.299972) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "unconnected-(U1-Pad9)") (pinfunction "NC") (pintype "no_connect"))
    (pad "10" smd rect locked (at 2.949948 -0.649986) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "/CHAN_8_OUT") (pinfunction "B4Y") (pintype "bidirectional"))
    (pad "11" smd rect locked (at 2.949948 0) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "/CHAN_9_OUT") (pinfunction "B3Y") (pintype "bidirectional"))
    (pad "12" smd rect locked (at 2.949948 0.649986) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "/CHAN_10_OUT") (pinfunction "B2Y") (pintype "bidirectional"))
    (pad "13" smd rect locked (at 2.949948 1.299972) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "/CHAN_11_OUT") (pinfunction "B1Y") (pintype "bidirectional"))
    (pad "14" smd rect locked (at 2.949948 1.949958) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "/3V3") (pinfunction "VCCB") (pintype "power_in"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 160.595 89.3 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LevelShifter.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at -2.6 0) (layer "B.SilkS"))
    (fp_text value "100nf 16v" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "/3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "/GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 160.595 99.3 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LevelShifter.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at -2.5 0) (layer "B.SilkS"))
    (fp_text value "100nf 16v" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "/3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "/GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 160.595 109.3 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "LevelShifter.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at -2.4 0) (layer "B.SilkS"))
    (fp_text value "100nf 16v" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "/3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "/GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TXU0104PWR" (layer "B.Cu")
    (tedit 0)
    (at 159.895 93.5)
    (property "Sheetfile" "LevelShifter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U3" (at -5.4 0) (layer "B.SilkS"))
    (fp_text value "TXU0104PWR" (at -0.1 4.2) (layer "B.SilkS") hide)
    (fp_text user "*" (at -3.20395 3.447758) (layer "B.SilkS"))
    (fp_text user "*" (at -3.20395 3.447758) (layer "B.SilkS"))
    (fp_text user "0.026in/0.65mm" (at -5.99795 1.624965) (layer "Cmts.User"))
    (fp_text user "0.055in/1.404mm" (at -2.94995 -4.9657) (layer "Cmts.User"))
    (fp_text user "0.014in/0.355mm" (at 5.99795 1.949958) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "0.232in/5.9mm" (at 0 4.9657) (layer "Cmts.User"))
    (fp_text user "*" (at -1.8669 2.4765) (layer "B.Fab"))
    (fp_text user "*" (at -1.8669 2.4765) (layer "B.Fab"))
    (pad "1" smd rect locked (at -2.949948 1.949958) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 64 "/5V_VREF") (pinfunction "VCCA") (pintype "power_in"))
    (pad "2" smd rect locked (at -2.949948 1.299972) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "/CHAN_7_IN") (pinfunction "A1") (pintype "bidirectional"))
    (pad "3" smd rect locked (at -2.949948 0.649986) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "/CHAN_6_IN") (pinfunction "A2") (pintype "bidirectional"))
    (pad "4" smd rect locked (at -2.949948 0) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "/CHAN_5_IN") (pinfunction "A3") (pintype "bidirectional"))
    (pad "5" smd rect locked (at -2.949948 -0.649986) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "/CHAN_4_IN") (pinfunction "A4") (pintype "bidirectional"))
    (pad "6" smd rect locked (at -2.949948 -1.299972) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "unconnected-(U3-Pad6)") (pinfunction "NC") (pintype "no_connect"))
    (pad "7" smd rect locked (at -2.949948 -1.949958) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "/GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" smd rect locked (at 2.949948 -1.949958) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "/3V3") (pinfunction "OE") (pintype "unspecified"))
    (pad "9" smd rect locked (at 2.949948 -1.299972) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "unconnected-(U3-Pad9)") (pinfunction "NC") (pintype "no_connect"))
    (pad "10" smd rect locked (at 2.949948 -0.649986) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "/CHAN_4_OUT") (pinfunction "B4Y") (pintype "bidirectional"))
    (pad "11" smd rect locked (at 2.949948 0) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "/CHAN_5_OUT") (pinfunction "B3Y") (pintype "bidirectional"))
    (pad "12" smd rect locked (at 2.949948 0.649986) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "/CHAN_6_OUT") (pinfunction "B2Y") (pintype "bidirectional"))
    (pad "13" smd rect locked (at 2.949948 1.299972) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "/CHAN_7_OUT") (pinfunction "B1Y") (pintype "bidirectional"))
    (pad "14" smd rect locked (at 2.949948 1.949958) (size 1.404099 0.3548) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "/3V3") (pinfunction "VCCB") (pintype "power_in"))
  )
  (gr_rect (start 145.795 117.6) (end 174.095 77.8) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "LevelShifter 1.5\nby El Dr.Gusman\n(c)2022" (at 160.6 112.3) (layer "B.SilkS"))
  (gr_text "Ext. VRef" (at 156.2 110.223606 90) (layer "F.SilkS"))
  (gr_text "5v VRef" (at 153.7 110.623606 90) (layer "F.SilkS"))
  (gr_text "VRef" (at 161.1 113.1) (layer "F.SilkS"))
  (zone (net 13) (net_name "/GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.499232 73.484597)
        (xy 143.099232 122.084597)
        (xy 178.199232 121.584597)
        (xy 177.599232 73.284597)
      )
    )
  )
  (zone (net 13) (net_name "/GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.786421 121.261136)
        (xy 174.886421 120.961136)
        (xy 174.886421 74.361136)
        (xy 174.788642 74.034617)
        (xy 145.388642 73.834617)
      )
    )
  )
)
