(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A")
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" signal)
		(2 "In2.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user "Board Edge")
	)
	(setup
		(stackup
			(layer "dielectric 1"
				(type "core")
				(thickness 0.019)
				(material "unknown")
				(epsilon_r 3.9)
				(loss_tangent 0.02)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 0.1)
				(material "unknown")
				(epsilon_r 4.05)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 3"
				(type "core")
				(thickness 1.265)
				(material "unknown")
				(epsilon_r 4.26)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 4"
				(type "core")
				(thickness 0.1)
				(material "unknown")
				(epsilon_r 4.05)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 5"
				(type "core")
				(thickness 0.019)
				(material "unknown")
				(epsilon_r 3.9)
				(loss_tangent 0.02)
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00000fc_fffffff9)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue no)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "output/")
		)
	)
	(net 0 "")
	(net 1 "DOUT20")
	(net 2 "DIN24")
	(net 3 "DOUT6")
	(net 4 "DIN14")
	(net 5 "DIN17")
	(net 6 "DOUT12")
	(net 7 "POWER_3v3")
	(net 8 "DOUT1")
	(net 9 "DOUT19")
	(net 10 "EXT_CHAIN")
	(net 11 "DIN6")
	(net 12 "DOUT22")
	(net 13 "DIN18")
	(net 14 "DIN12")
	(net 15 "EXT_VREF")
	(net 16 "DIN1")
	(net 17 "DOUT18")
	(net 18 "DOUT11")
	(net 19 "DOUT5")
	(net 20 "DIN19")
	(net 21 "DIN11")
	(net 22 "DIN5")
	(net 23 "DOUT17")
	(net 24 "DOUT10")
	(net 25 "VREF")
	(net 26 "DIN20")
	(net 27 "GND")
	(net 28 "DOUT4")
	(net 29 "DOUT16")
	(net 30 "DIN10")
	(net 31 "DIN4")
	(net 32 "DIN21")
	(net 33 "DOUT9")
	(net 34 "DOUT3")
	(net 35 "DOUT15")
	(net 36 "POWER_5v")
	(net 37 "DOUT24")
	(net 38 "DIN22")
	(net 39 "DIN9")
	(net 40 "DIN3")
	(net 41 "DOUT14")
	(net 42 "DOUT8")
	(net 43 "DIN13")
	(net 44 "DIN15")
	(net 45 "DIN23")
	(net 46 "DIN8")
	(net 47 "DOUT2")
	(net 48 "DOUT21")
	(net 49 "EXT_TRIG")
	(net 50 "DOUT7")
	(net 51 "DOUT23")
	(net 52 "DIN16")
	(net 53 "DOUT13")
	(net 54 "DIN7")
	(net 55 "DIN2")
	(footprint "jitx-design:HDR_TH_32P_P2_54_H_M_R2_C16_S2_54_1"
		(layer "F.Cu")
		(at 112.600441 112.450949 -90)
		(property "Reference" "J2"
			(at 0.049051 -0.149559 0)
			(layer "F.SilkS")
		)
		(property "Value" "C97095"
			(at -0.75 -7.6641 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at 19.05 -5.9075 90)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "GND")
			(solder_mask_margin 0.051)
		)
		(pad "2" thru_hole circle
			(at 19.05 -3.3675 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "GND")
			(solder_mask_margin 0.051)
		)
		(pad "3" thru_hole circle
			(at 16.51 -5.9075 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "EXT_VREF")
			(solder_mask_margin 0.051)
		)
		(pad "4" thru_hole circle
			(at 16.51 -3.3675 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "EXT_TRIG")
			(solder_mask_margin 0.051)
		)
		(pad "5" thru_hole circle
			(at 13.97 -5.9075 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "POWER_5v")
			(solder_mask_margin 0.051)
		)
		(pad "6" thru_hole circle
			(at 13.97 -3.3675 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "POWER_5v")
			(solder_mask_margin 0.051)
		)
		(pad "7" thru_hole circle
			(at 11.43 -5.9075 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "POWER_3v3")
			(solder_mask_margin 0.051)
		)
		(pad "8" thru_hole circle
			(at 11.43 -3.3675 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "POWER_3v3")
			(solder_mask_margin 0.051)
		)
		(pad "9" thru_hole circle
			(at 8.89 -5.9075 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "DIN12")
			(solder_mask_margin 0.051)
		)
		(pad "10" thru_hole circle
			(at 8.89 -3.3675 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "DIN13")
			(solder_mask_margin 0.051)
		)
		(pad "11" thru_hole circle
			(at 6.35 -5.9075 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "DIN11")
			(solder_mask_margin 0.051)
		)
		(pad "12" thru_hole circle
			(at 6.35 -3.3675 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "DIN14")
			(solder_mask_margin 0.051)
		)
		(pad "13" thru_hole circle
			(at 3.81 -5.9075 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "DIN10")
			(solder_mask_margin 0.051)
		)
		(pad "14" thru_hole circle
			(at 3.81 -3.3675 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "DIN15")
			(solder_mask_margin 0.051)
		)
		(pad "15" thru_hole circle
			(at 1.27 -5.9075 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "DIN9")
			(solder_mask_margin 0.051)
		)
		(pad "16" thru_hole circle
			(at 1.27 -3.3675 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "DIN16")
			(solder_mask_margin 0.051)
		)
		(pad "17" thru_hole circle
			(at -1.27 -5.9075 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "DIN8")
			(solder_mask_margin 0.051)
		)
		(pad "18" thru_hole circle
			(at -1.27 -3.3675 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "DIN17")
			(solder_mask_margin 0.051)
		)
		(pad "19" thru_hole circle
			(at -3.81 -5.9075 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "DIN7")
			(solder_mask_margin 0.051)
		)
		(pad "20" thru_hole circle
			(at -3.81 -3.3675 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "DIN18")
			(solder_mask_margin 0.051)
		)
		(pad "21" thru_hole circle
			(at -6.35 -5.9075 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "DIN6")
			(solder_mask_margin 0.051)
		)
		(pad "22" thru_hole circle
			(at -6.35 -3.3675 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "DIN19")
			(solder_mask_margin 0.051)
		)
		(pad "23" thru_hole circle
			(at -8.89 -5.9075 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "DIN5")
			(solder_mask_margin 0.051)
		)
		(pad "24" thru_hole circle
			(at -8.89 -3.3675 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "DIN20")
			(solder_mask_margin 0.051)
		)
		(pad "25" thru_hole circle
			(at -11.43 -5.9075 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "DIN4")
			(solder_mask_margin 0.051)
		)
		(pad "26" thru_hole circle
			(at -11.43 -3.3675 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "DIN21")
			(solder_mask_margin 0.051)
		)
		(pad "27" thru_hole circle
			(at -13.97 -5.9075 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "DIN3")
			(solder_mask_margin 0.051)
		)
		(pad "28" thru_hole circle
			(at -13.97 -3.3675 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "DIN22")
			(solder_mask_margin 0.051)
		)
		(pad "29" thru_hole circle
			(at -16.51 -5.9075 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "DIN2")
			(solder_mask_margin 0.051)
		)
		(pad "30" thru_hole circle
			(at -16.51 -3.3675 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "DIN23")
			(solder_mask_margin 0.051)
		)
		(pad "31" thru_hole circle
			(at -19.05 -5.9075 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "DIN1")
			(solder_mask_margin 0.051)
		)
		(pad "32" thru_hole circle
			(at -19.05 -3.3675 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "DIN24")
			(solder_mask_margin 0.051)
		)
		(model "${KIPRJMOD}/3d-models/jitx-64d1fa94b789d8dc4b8f5892.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "jitx-design:TSSOP_14_L5_0_W4_4_P0_65_LS6_4_BL_5"
		(layer "F.Cu")
		(at 129.408407 94.417618 -90)
		(property "Reference" "U1"
			(at 0.082382 0.408407 0)
			(layer "F.SilkS")
		)
		(property "Value" "TXU0104PWR"
			(at -0.75 -4.4066 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.9425 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "VREF")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "2" smd rect
			(at -1.2925 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "DIN1")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "3" smd rect
			(at -0.6425 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "DIN2")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "4" smd rect
			(at 0.0075 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "DIN3")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "5" smd rect
			(at 0.6575 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "DIN4")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "6" smd rect
			(at 1.3075 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "7" smd rect
			(at 1.9575 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "8" smd rect
			(at 1.9575 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "POWER_3v3")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "9" smd rect
			(at 1.3075 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "10" smd rect
			(at 0.6575 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "DOUT4")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "11" smd rect
			(at 0.0075 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "DOUT3")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "12" smd rect
			(at -0.6425 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "DOUT2")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "13" smd rect
			(at -1.2925 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "DOUT1")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "14" smd rect
			(at -1.9425 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "POWER_3v3")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(model "${KIPRJMOD}/3d-models/jitx-64d14121b789d8dc4b7a3884.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "jitx-design:Pkg0402_2"
		(layer "F.Cu")
		(at 139.36309 82.928795)
		(property "Reference" "R2"
			(at 1.2572 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "8K2"
			(at 0.6 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at 0 -0.409861)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "EXT_CHAIN")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0 0.409861)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.05)
		)
	)
	(footprint "jitx-design:Pkg0402_10"
		(layer "F.Cu")
		(at 130.647747 120.320808 90)
		(property "Reference" "C9"
			(at 0 1.31 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0.6 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at 0 -0.409861 90)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0 0.409861 90)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "POWER_3v3")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/3d-models/jitx-64d1493ab789d8dc4b7b3f0a.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad"
		(layer "F.Cu")
		(at 116.5 136.5)
		(descr "Mounting Hole 2.7mm, M2.5, DIN965")
		(tags "mounting hole 2.7mm m2.5 din965")
		(property "Reference" "REF**"
			(at 0 -3.35 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.7mm_M2.5_DIN965_Pad"
			(at 0 3.35 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 4.7 4.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "jitx-design:TSSOP_14_L5_0_W4_4_P0_65_LS6_4_BL_1"
		(layer "F.Cu")
		(at 129.408407 116.505971 -90)
		(property "Reference" "U5"
			(at 0.244029 0.408407 0)
			(layer "F.SilkS")
		)
		(property "Value" "TXU0104PWR"
			(at -0.75 -4.4066 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.9425 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "VREF")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "2" smd rect
			(at -1.2925 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "DIN20")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "3" smd rect
			(at -0.6425 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "DIN19")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "4" smd rect
			(at 0.0075 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "DIN18")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "5" smd rect
			(at 0.6575 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "DIN17")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "6" smd rect
			(at 1.3075 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "7" smd rect
			(at 1.9575 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "8" smd rect
			(at 1.9575 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "POWER_3v3")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "9" smd rect
			(at 1.3075 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "10" smd rect
			(at 0.6575 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "DOUT17")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "11" smd rect
			(at 0.0075 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "DOUT18")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "12" smd rect
			(at -0.6425 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "DOUT19")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "13" smd rect
			(at -1.2925 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "DOUT20")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "14" smd rect
			(at -1.9425 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "POWER_3v3")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(model "${KIPRJMOD}/3d-models/jitx-64d14121b789d8dc4b7a3884.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "jitx-design:TSSOP_14_L5_0_W4_4_P0_65_LS6_4_BL_3"
		(layer "F.Cu")
		(at 129.408407 101.780402 -90)
		(property "Reference" "U4"
			(at -0.030402 0.408407 0)
			(layer "F.SilkS")
		)
		(property "Value" "TXU0104PWR"
			(at -0.75 -4.4066 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.9425 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "VREF")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "2" smd rect
			(at -1.2925 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "DIN24")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "3" smd rect
			(at -0.6425 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "DIN23")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "4" smd rect
			(at 0.0075 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "DIN22")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "5" smd rect
			(at 0.6575 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "DIN21")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "6" smd rect
			(at 1.3075 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "7" smd rect
			(at 1.9575 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "8" smd rect
			(at 1.9575 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "POWER_3v3")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "9" smd rect
			(at 1.3075 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "10" smd rect
			(at 0.6575 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "DOUT21")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "11" smd rect
			(at 0.0075 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "DOUT22")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "12" smd rect
			(at -0.6425 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "DOUT23")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "13" smd rect
			(at -1.2925 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "DOUT24")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "14" smd rect
			(at -1.9425 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "POWER_3v3")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(model "${KIPRJMOD}/3d-models/jitx-64d14121b789d8dc4b7a3884.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "jitx-design:TSSOP_14_L5_0_W4_4_P0_65_LS6_4_BL_2"
		(layer "F.Cu")
		(at 129.408407 109.143187 -90)
		(property "Reference" "U6"
			(at 0.106813 0.408407 0)
			(layer "F.SilkS")
		)
		(property "Value" "TXU0104PWR"
			(at -0.75 -4.4066 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.9425 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "VREF")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "2" smd rect
			(at -1.2925 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "DIN5")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "3" smd rect
			(at -0.6425 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "DIN6")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "4" smd rect
			(at 0.0075 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "DIN7")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "5" smd rect
			(at 0.6575 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "DIN8")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "6" smd rect
			(at 1.3075 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "7" smd rect
			(at 1.9575 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "8" smd rect
			(at 1.9575 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "POWER_3v3")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "9" smd rect
			(at 1.3075 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "10" smd rect
			(at 0.6575 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "DOUT8")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "11" smd rect
			(at 0.0075 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "DOUT7")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "12" smd rect
			(at -0.6425 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "DOUT6")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "13" smd rect
			(at -1.2925 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "DOUT5")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "14" smd rect
			(at -1.9425 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "POWER_3v3")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(model "${KIPRJMOD}/3d-models/jitx-64d14121b789d8dc4b7a3884.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "jitx-design:COMM_SMD_L51_0_W21_0_P2_54_SC0916"
		(layer "F.Cu")
		(at 154.030966 102.61541 -90)
		(property "Reference" "U7"
			(at 0 12.5885 0)
			(layer "F.SilkS")
		)
		(property "Value" "PICO"
			(at -0.75 -12.4441 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -23.557 10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "EXT_CHAIN")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "2" smd rect
			(at -21.017 10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "EXT_CHAIN")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "3" smd rect
			(at -18.477 10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "4" smd rect
			(at -15.937 10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "DOUT1")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "5" smd rect
			(at -13.397 10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "DOUT2")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "6" smd rect
			(at -10.857 10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "DOUT3")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "7" smd rect
			(at -8.317 10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "DOUT4")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "8" smd rect
			(at -5.777 10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "9" smd rect
			(at -3.237 10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "DOUT5")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "10" smd rect
			(at -0.697 10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "DOUT6")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "11" smd rect
			(at 1.843 10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "DOUT7")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "12" smd rect
			(at 4.383 10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "DOUT8")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "13" smd rect
			(at 6.923 10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "14" smd rect
			(at 9.463 10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "DOUT9")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "15" smd rect
			(at 12.003 10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "DOUT10")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "16" smd rect
			(at 14.543 10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "DOUT11")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "17" smd rect
			(at 17.083 10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "DOUT12")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "18" smd rect
			(at 19.623 10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "19" smd rect
			(at 22.163 10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "DOUT13")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "20" smd rect
			(at 24.703 10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "DOUT14")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "21" smd rect
			(at 24.703 -10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "DOUT15")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "22" smd rect
			(at 22.163 -10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "DOUT16")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "23" smd rect
			(at 19.623 -10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "24" smd rect
			(at 17.083 -10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "DOUT17")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "25" smd rect
			(at 14.543 -10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "DOUT18")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "26" smd rect
			(at 12.003 -10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "DOUT19")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "27" smd rect
			(at 9.463 -10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "DOUT20")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "28" smd rect
			(at 6.923 -10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "29" smd rect
			(at 4.383 -10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "DOUT21")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "30" smd rect
			(at 1.843 -10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "31" smd rect
			(at -0.697 -10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "DOUT22")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "32" smd rect
			(at -3.237 -10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "DOUT23")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "33" smd rect
			(at -5.777 -10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "34" smd rect
			(at -8.317 -10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "DOUT24")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "35" smd rect
			(at -10.857 -10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "36" smd rect
			(at -13.397 -10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "POWER_3v3")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "37" smd rect
			(at -15.937 -10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "38" smd rect
			(at -18.477 -10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "39" smd rect
			(at -21.017 -10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "40" smd rect
			(at -23.557 -10.0875 270)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "POWER_5v")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "41" smd rect
			(at 25.503 2.5395)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "42" smd rect
			(at 25.503 -0.0005)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "43" smd rect
			(at 25.503 -2.5405)
			(size 1.6 3.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
	)
	(footprint "jitx-design:Pkg0402"
		(layer "F.Cu")
		(at 128.284379 127.710388 -90)
		(property "Reference" "C2"
			(at -0.079186 1.31 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0.6 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at 0 -0.409861 270)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0 0.409861 270)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "VREF")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/3d-models/jitx-64d1493ab789d8dc4b7b3f0a.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "jitx-design:TSSOP_14_L5_0_W4_4_P0_65_LS6_4_BL"
		(layer "F.Cu")
		(at 129.408407 123.868755 -90)
		(property "Reference" "U3"
			(at 0.131245 0.408407 0)
			(layer "F.SilkS")
		)
		(property "Value" "TXU0104PWR"
			(at -0.75 -4.4066 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.9425 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "VREF")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "2" smd rect
			(at -1.2925 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "DIN9")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "3" smd rect
			(at -0.6425 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "DIN10")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "4" smd rect
			(at 0.0075 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "DIN11")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "5" smd rect
			(at 0.6575 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "DIN12")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "6" smd rect
			(at 1.3075 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "7" smd rect
			(at 1.9575 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "8" smd rect
			(at 1.9575 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "POWER_3v3")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "9" smd rect
			(at 1.3075 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "10" smd rect
			(at 0.6575 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "DOUT12")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "11" smd rect
			(at 0.0075 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "DOUT11")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "12" smd rect
			(at -0.6425 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "DOUT10")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "13" smd rect
			(at -1.2925 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "DOUT9")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "14" smd rect
			(at -1.9425 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "POWER_3v3")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(model "${KIPRJMOD}/3d-models/jitx-64d14121b789d8dc4b7a3884.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "jitx-design:Pkg0402_11"
		(layer "F.Cu")
		(at 130.647747 98.15207 90)
		(property "Reference" "C10"
			(at 0 1.49 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0.6 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at 0 -0.409861 90)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0 0.409861 90)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "POWER_3v3")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/3d-models/jitx-64d1493ab789d8dc4b7b3f0a.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad"
		(layer "F.Cu")
		(at 163.5 136.5)
		(descr "Mounting Hole 2.7mm, M2.5, DIN965")
		(tags "mounting hole 2.7mm m2.5 din965")
		(property "Reference" "REF**"
			(at 0 -3.35 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.7mm_M2.5_DIN965_Pad"
			(at 0 3.35 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 4.7 4.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "jitx-design:Pkg0402_3"
		(layer "F.Cu")
		(at 128.184379 90.76614 -90)
		(property "Reference" "C1"
			(at -1 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0.6 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at 0 -0.409861 270)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0 0.409861 270)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "VREF")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/3d-models/jitx-64d1493ab789d8dc4b7b3f0a.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "jitx-design:Pkg0402_5"
		(layer "F.Cu")
		(at 130.647747 90.762491 90)
		(property "Reference" "C7"
			(at 1 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0.6 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at 0 -0.409861 90)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0 0.409861 90)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "POWER_3v3")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/3d-models/jitx-64d1493ab789d8dc4b7b3f0a.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "jitx-design:HDR_TH_3P_P2_54_H_F_W10_0_N"
		(layer "F.Cu")
		(at 129.508688 80.551297 180)
		(property "Reference" "J1"
			(at 4.927 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "PM254-1-03-W-8.5"
			(at -0.75 -6.2691 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -2.54 -4.5635 180)
			(size 1.9 1.9)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "EXT_CHAIN")
			(solder_mask_margin 0.05)
		)
		(pad "2" thru_hole circle
			(at 0 -4.5635 180)
			(size 1.9 1.9)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.05)
		)
		(pad "3" thru_hole circle
			(at 2.54 -4.5635 180)
			(size 1.9 1.9)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "GND")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/3d-models/jitx-64d25c31b789d8dc4b9a488a.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "jitx-design:Pkg0402_12"
		(layer "F.Cu")
		(at 128.184379 120.321538 -90)
		(property "Reference" "C3"
			(at -0.02759 1.31 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0.6 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at 0 -0.409861 270)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0 0.409861 270)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "VREF")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/3d-models/jitx-64d1493ab789d8dc4b7b3f0a.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "jitx-design:LL_34_L3_5_W1_5_RD"
		(layer "F.Cu")
		(at 136.915062 80.798588 90)
		(property "Reference" "D1"
			(at 0 -1.827 0)
			(layer "F.SilkS")
		)
		(property "Value" "LL4148"
			(at -0.75 -1.6326 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.7 0 270)
			(size 1.1 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "EXT_TRIG")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "2" smd rect
			(at 1.7 0 270)
			(size 1.1 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "EXT_CHAIN")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(model "${KIPRJMOD}/3d-models/jitx-64d15923b789d8dc4b7d1a30.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "jitx-design:HDR_TH_3P_P2_54_H_M_W10_0"
		(layer "F.Cu")
		(at 129.508688 141.017927 180)
		(property "Reference" "J3"
			(at 4.341 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "DZ254W-11-03-65"
			(at -0.75 -6.3246 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at -2.54 4.668 180)
			(size 1.8 1.8)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "EXT_CHAIN")
			(solder_mask_margin 0.051)
		)
		(pad "2" thru_hole circle
			(at 0 4.668 180)
			(size 1.8 1.8)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.051)
		)
		(pad "3" thru_hole circle
			(at 2.54 4.668 180)
			(size 1.8 1.8)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "GND")
			(solder_mask_margin 0.051)
		)
		(model "${KIPRJMOD}/3d-models/jitx-64d18ba2b789d8dc4b830bf3.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad"
		(layer "F.Cu")
		(at 121 80)
		(descr "Mounting Hole 2.7mm, M2.5, DIN965")
		(tags "mounting hole 2.7mm m2.5 din965")
		(property "Reference" "REF**"
			(at 0 -3.35 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.7mm_M2.5_DIN965_Pad"
			(at 0 3.35 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 4.7 4.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "jitx-design:Pkg0402_4"
		(layer "F.Cu")
		(at 136.915062 84.452309)
		(property "Reference" "R1"
			(at -1.06 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100K"
			(at 0.6 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at 0 -0.409861)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "EXT_TRIG")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0 0.409861)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.05)
		)
	)
	(footprint "jitx-design:Pkg0402_9"
		(layer "F.Cu")
		(at 128.184379 105.543839 -90)
		(property "Reference" "C6"
			(at 0 1.31 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0.6 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at 0 -0.409861 270)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0 0.409861 270)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "VREF")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/3d-models/jitx-64d1493ab789d8dc4b7b3f0a.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "jitx-design:TSSOP_14_L5_0_W4_4_P0_65_LS6_4_BL_4"
		(layer "F.Cu")
		(at 129.508407 131.231539 -90)
		(property "Reference" "U2"
			(at 0.018461 0.508407 0)
			(layer "F.SilkS")
		)
		(property "Value" "TXU0104PWR"
			(at -0.75 -4.4066 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.9425 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "VREF")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "2" smd rect
			(at -1.2925 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "DIN16")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "3" smd rect
			(at -0.6425 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "DIN15")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "4" smd rect
			(at 0.0075 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "DIN14")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "5" smd rect
			(at 0.6575 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "DIN13")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "6" smd rect
			(at 1.3075 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "7" smd rect
			(at 1.9575 2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "8" smd rect
			(at 1.9575 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "POWER_3v3")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "9" smd rect
			(at 1.3075 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "10" smd rect
			(at 0.6575 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "DOUT13")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "11" smd rect
			(at 0.0075 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "DOUT14")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "12" smd rect
			(at -0.6425 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "DOUT15")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "13" smd rect
			(at -1.2925 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "DOUT16")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(pad "14" smd rect
			(at -1.9425 -2.8 270)
			(size 0.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "POWER_3v3")
			(solder_mask_margin 0.051)
			(solder_paste_margin 0.051)
		)
		(model "${KIPRJMOD}/3d-models/jitx-64d14121b789d8dc4b7a3884.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "jitx-design:SW_TH_SK_13D01_G030"
		(layer "F.Cu")
		(at 113.128033 83.279627 -90)
		(property "Reference" "S1"
			(at 0 4.77 0)
			(layer "F.SilkS")
		)
		(property "Value" "SK-13D01-G030"
			(at -0.75 -4.6256 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -4 -1.507 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "EXT_VREF")
			(solder_mask_margin 0.05)
		)
		(pad "2" thru_hole circle
			(at 0 -1.507 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "VREF")
			(solder_mask_margin 0.05)
		)
		(pad "3" thru_hole circle
			(at 2 -1.507 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "POWER_3v3")
			(solder_mask_margin 0.05)
		)
		(pad "4" thru_hole circle
			(at 4 -1.507 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "POWER_5v")
			(solder_mask_margin 0.05)
		)
		(pad "5" thru_hole oval
			(at 6.35 -1.507 270)
			(size 1.2 2)
			(drill oval 0.6 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.05)
		)
		(pad "6" thru_hole oval
			(at -6.35 -1.507 270)
			(size 1.2 2)
			(drill oval 0.6 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/3d-models/jitx-64d17702b789d8dc4b808140.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "jitx-design:Pkg0402_6"
		(layer "F.Cu")
		(at 128.184379 98.154989 -90)
		(property "Reference" "C4"
			(at 0 1.31 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0.6 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at 0 -0.409861 270)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0 0.409861 270)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "VREF")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/3d-models/jitx-64d1493ab789d8dc4b7b3f0a.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "jitx-design:Pkg0402_7"
		(layer "F.Cu")
		(at 128.184379 112.932689 -90)
		(property "Reference" "C5"
			(at 0 1.31 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0.6 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at 0 -0.409861 270)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0 0.409861 270)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "VREF")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/3d-models/jitx-64d1493ab789d8dc4b7b3f0a.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "jitx-design:Pkg0402_1"
		(layer "F.Cu")
		(at 130.647747 112.931229 90)
		(property "Reference" "C11"
			(at 0 1.49 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0.6 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at 0 -0.409861 90)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0 0.409861 90)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "POWER_3v3")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/3d-models/jitx-64d1493ab789d8dc4b7b3f0a.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "jitx-design:Pkg0402_13"
		(layer "F.Cu")
		(at 130.647747 105.54165 90)
		(property "Reference" "C12"
			(at 0 1.49 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0.6 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at 0 -0.409861 90)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0 0.409861 90)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "POWER_3v3")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/3d-models/jitx-64d1493ab789d8dc4b7b3f0a.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "jitx-design:Pkg0402_8"
		(layer "F.Cu")
		(at 130.747747 127.710388 90)
		(property "Reference" "C8"
			(at 0 1.31 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0.6 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at 0 -0.409861 90)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd rect
			(at 0 0.409861 90)
			(size 0.6 0.280278)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "POWER_3v3")
			(solder_mask_margin 0.05)
		)
		(model "${KIPRJMOD}/3d-models/jitx-64d1493ab789d8dc4b7b3f0a.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Logo:sembei_scale_small"
		(layer "B.Cu")
		(at 141.5 110.5 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "Logo:sembei_scale_small"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(gr_line
		(start 167.207867 75.611107)
		(end 167.176777 75.573223)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.176777 75.573223)
		(end 167.138893 75.542133)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.861107 140.457867)
		(end 111.904329 140.48097)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.951227 75.504804)
		(end 111.904329 75.51903)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.245196 75.701227)
		(end 167.23097 75.654329)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.754804 140.298773)
		(end 111.76903 140.345671)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.207867 140.388893)
		(end 167.23097 140.345671)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.861107 75.542133)
		(end 111.823223 75.573223)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.176777 140.426777)
		(end 167.207867 140.388893)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.904329 75.51903)
		(end 111.861107 75.542133)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112 75.5)
		(end 111.951227 75.504804)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.823223 75.573223)
		(end 111.792133 75.611107)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112 140.5)
		(end 167 140.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.76903 140.345671)
		(end 111.792133 140.388893)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.095671 140.48097)
		(end 167.138893 140.457867)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.095671 75.51903)
		(end 167.048773 75.504804)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.904329 140.48097)
		(end 111.951227 140.495196)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167 75.5)
		(end 112 75.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.25 75.75)
		(end 167.245196 75.701227)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.75 140.25)
		(end 111.754804 140.298773)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.75 75.75)
		(end 111.75 140.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.048773 75.504804)
		(end 167 75.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.792133 75.611107)
		(end 111.76903 75.654329)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167 140.5)
		(end 167.048773 140.495196)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.25 140.25)
		(end 167.25 75.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.951227 140.495196)
		(end 112 140.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.048773 140.495196)
		(end 167.095671 140.48097)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.823223 140.426777)
		(end 111.861107 140.457867)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.138893 75.542133)
		(end 167.095671 75.51903)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.792133 140.388893)
		(end 111.823223 140.426777)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.76903 75.654329)
		(end 111.754804 75.701227)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.23097 75.654329)
		(end 167.207867 75.611107)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.754804 75.701227)
		(end 111.75 75.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.138893 140.457867)
		(end 167.176777 140.426777)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.23097 140.345671)
		(end 167.245196 140.298773)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.245196 140.298773)
		(end 167.25 140.25)
		(layer "Edge.Cuts")
	)
	(gr_text "By El Dr. Gusman - 2024"
		(at 151.25 129.75 0)
		(layer "B.SilkS")
	)
	(gr_text "LogicAnalyzer"
		(at 158.75 92 0)
		(layer "B.SilkS")
	)
	(gr_text "https://github.com/gusmanb/logicanalyzer"
		(at 157.75 131.75 0)
		(layer "B.SilkS")
	)
	(gr_text "10"
		(at 122.75 117 0)
		(layer "F.SilkS")
	)
	(gr_text "7"
		(at 123.25 109.5 0)
		(layer "F.SilkS")
	)
	(gr_text "3V3"
		(at 120.25 124.5 0)
		(layer "F.SilkS")
	)
	(gr_text "C"
		(at 118.25 87.5 0)
		(layer "F.SilkS")
	)
	(gr_text "11"
		(at 122.75 119.5 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 123.25 94.5 0)
		(layer "F.SilkS")
	)
	(gr_text "12"
		(at 122.75 122 0)
		(layer "F.SilkS")
	)
	(gr_text "16"
		(at 120.25 114.5 0)
		(layer "F.SilkS")
	)
	(gr_text "18"
		(at 120.25 109.5 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 120.25 132 0)
		(layer "F.SilkS")
	)
	(gr_text "17"
		(at 120.25 112 0)
		(layer "F.SilkS")
	)
	(gr_text "TRG"
		(at 120.25 129.5 0)
		(layer "F.SilkS")
	)
	(gr_text "24"
		(at 120.25 94.5 0)
		(layer "F.SilkS")
	)
	(gr_text "20"
		(at 120.25 104.5 0)
		(layer "F.SilkS")
	)
	(gr_text "8"
		(at 123.25 112 0)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 123.25 97 0)
		(layer "F.SilkS")
	)
	(gr_text "L"
		(at 118.25 85.75 0)
		(layer "F.SilkS")
	)
	(gr_text "21"
		(at 120.25 102 0)
		(layer "F.SilkS")
	)
	(gr_text "6"
		(at 123.25 107 0)
		(layer "F.SilkS")
	)
	(gr_text "3"
		(at 123.25 99.5 0)
		(layer "F.SilkS")
	)
	(gr_text "23"
		(at 120.25 97 0)
		(layer "F.SilkS")
	)
	(gr_text "5v0"
		(at 120.75 89.25 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 122.75 132 0)
		(layer "F.SilkS")
	)
	(gr_text "9"
		(at 123.25 114.5 0)
		(layer "F.SilkS")
	)
	(gr_text "19"
		(at 120.25 107 0)
		(layer "F.SilkS")
	)
	(gr_text "VRF"
		(at 122.75 129.5 0)
		(layer "F.SilkS")
	)
	(gr_text "15"
		(at 120.25 117 0)
		(layer "F.SilkS")
	)
	(gr_text "EXT"
		(at 120.75 85.75 0)
		(layer "F.SilkS")
	)
	(gr_text "22"
		(at 120.25 99.5 0)
		(layer "F.SilkS")
	)
	(gr_text "3v3"
		(at 120.75 87.5 0)
		(layer "F.SilkS")
	)
	(gr_text "R"
		(at 118.25 89.25 0)
		(layer "F.SilkS")
	)
	(gr_text "3V3"
		(at 122.75 124.5 0)
		(layer "F.SilkS")
	)
	(gr_text "13"
		(at 120.25 122 0)
		(layer "F.SilkS")
	)
	(gr_text "4"
		(at 123.25 102 0)
		(layer "F.SilkS")
	)
	(gr_text "14"
		(at 120.25 119.5 0)
		(layer "F.SilkS")
	)
	(gr_text "5"
		(at 123.25 104.5 0)
		(layer "F.SilkS")
	)
	(gr_text "5V0"
		(at 120.25 127 0)
		(layer "F.SilkS")
	)
	(gr_text "5V0"
		(at 122.75 127 0)
		(layer "F.SilkS")
	)
	(zone
		(net 27)
		(net_name "GND")
		(layer "F.Cu")
		(hatch none 0.1)
		(connect_pads
			(clearance 0.1)
		)
		(min_thickness 0.03)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 168 75.75) (xy 167.995196 75.701227) (xy 167.98097 75.654329) (xy 167.957867 75.611107) (xy 167.926777 75.573223)
				(xy 167.888893 75.542133) (xy 167.845671 75.51903) (xy 167.798773 75.504804) (xy 167.75 75.5) (xy 111.25 75.5)
				(xy 111.201227 75.504804) (xy 111.154329 75.51903) (xy 111.111107 75.542133) (xy 111.073223 75.573223)
				(xy 111.042133 75.611107) (xy 111.01903 75.654329) (xy 111.004804 75.701227) (xy 111 75.75) (xy 111 140.25)
				(xy 111.004804 140.298773) (xy 111.01903 140.345671) (xy 111.042133 140.388893) (xy 111.073223 140.426777)
				(xy 111.111107 140.457867) (xy 111.154329 140.48097) (xy 111.201227 140.495196) (xy 111.25 140.5)
				(xy 167.75 140.5) (xy 167.798773 140.495196) (xy 167.845671 140.48097) (xy 167.888893 140.457867)
				(xy 167.926777 140.426777) (xy 167.957867 140.388893) (xy 167.98097 140.345671) (xy 167.995196 140.298773)
				(xy 168 140.25)
			)
		)
	)
	(zone
		(net 27)
		(net_name "GND")
		(layer "B.Cu")
		(hatch none 0.1)
		(connect_pads
			(clearance 0.1)
		)
		(min_thickness 0.03)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 168 75.75) (xy 167.995196 75.701227) (xy 167.98097 75.654329) (xy 167.957867 75.611107) (xy 167.926777 75.573223)
				(xy 167.888893 75.542133) (xy 167.845671 75.51903) (xy 167.798773 75.504804) (xy 167.75 75.5) (xy 111.25 75.5)
				(xy 111.201227 75.504804) (xy 111.154329 75.51903) (xy 111.111107 75.542133) (xy 111.073223 75.573223)
				(xy 111.042133 75.611107) (xy 111.01903 75.654329) (xy 111.004804 75.701227) (xy 111 75.75) (xy 111 140.25)
				(xy 111.004804 140.298773) (xy 111.01903 140.345671) (xy 111.042133 140.388893) (xy 111.073223 140.426777)
				(xy 111.111107 140.457867) (xy 111.154329 140.48097) (xy 111.201227 140.495196) (xy 111.25 140.5)
				(xy 167.75 140.5) (xy 167.798773 140.495196) (xy 167.845671 140.48097) (xy 167.888893 140.457867)
				(xy 167.926777 140.426777) (xy 167.957867 140.388893) (xy 167.98097 140.345671) (xy 167.995196 140.298773)
				(xy 168 140.25)
			)
		)
	)
)
