(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal "Top Layer")
		(1 "In1.Cu" signal "Inner1")
		(2 "In2.Cu" signal "Inner2")
		(31 "B.Cu" signal "Bottom Layer")
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user "Bottom Paste Mask Layer")
		(35 "F.Paste" user "Top Paste Mask Layer")
		(36 "B.SilkS" user "Bottom Silkscreen Layer")
		(37 "F.SilkS" user "Top Silkscreen Layer")
		(38 "B.Mask" user "Bottom Solder Mask Layer")
		(39 "F.Mask" user "Top Solder Mask Layer")
		(40 "Dwgs.User" user "Document Layer")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "Mechanical Layer")
		(44 "Edge.Cuts" user "Multi-Layer")
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user "Bottom Assembly Layer")
		(49 "F.Fab" user "Top Assembly Layer")
		(50 "User.1" user "Ratline Layer")
		(51 "User.2" user "Component Shape Layer")
		(52 "User.3" user "Component Marking Layer")
		(53 "User.4" user "3D Shell Outline Layer")
		(54 "User.5" user "3D Shell Top Layer")
		(55 "User.6" user "3D Shell Bottom Layer")
		(56 "User.7" user "Drill Drawing Layer")
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(aux_axis_origin 120 130)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "EXT_CHAIN")
	(net 2 "GND")
	(net 3 "CHAN_0")
	(net 4 "CHAN_1")
	(net 5 "CHAN_2")
	(net 6 "CHAN_3")
	(net 7 "CHAN_8")
	(net 8 "CHAN_7")
	(net 9 "CHAN_6")
	(net 10 "CHAN_5")
	(net 11 "CHAN_4")
	(net 12 "CHAN_13")
	(net 13 "CHAN_12")
	(net 14 "CHAN_11")
	(net 15 "CHAN_10")
	(net 16 "CHAN_9")
	(net 17 "CHAN_18")
	(net 18 "CHAN_17")
	(net 19 "CHAN_16")
	(net 20 "CHAN_15")
	(net 21 "CHAN_14")
	(net 22 "CHAN_22")
	(net 23 "CHAN_21")
	(net 24 "CHAN_20")
	(net 25 "CHAN_19")
	(net 26 "CHAN_23")
	(net 27 "+3.3V")
	(net 28 "+5V")
	(net 29 "EXT_T")
	(net 30 "$1N6412")
	(net 31 "$1N6457")
	(net 32 "$1N6576")
	(net 33 "$1N6580")
	(net 34 "$1N6666")
	(net 35 "$1N6670")
	(net 36 "$1N6756")
	(net 37 "$1N6760")
	(net 38 "$1N6846")
	(net 39 "$1N6850")
	(net 40 "$1N6936")
	(net 41 "$1N6940")
	(net 42 "$1N7395")
	(net 43 "$1N7399")
	(net 44 "$1N7403")
	(net 45 "$1N7407")
	(net 46 "$1N7411")
	(net 47 "$1N7415")
	(net 48 "$1N7419")
	(net 49 "$1N7423")
	(net 50 "$1N7427")
	(net 51 "$1N7431")
	(net 52 "$1N7435")
	(net 53 "$1N7439")
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "F.Cu")
		(at 133.224 118.361 90)
		(property "Reference" "D3"
			(at -1.77 -1.7395 450)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "CHAN_2")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:树莓派pico多层"
		(layer "F.Cu")
		(at 171.4135 105.381 90)
		(property "Reference" "U2"
			(at -0.77 -51.802 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "91c3a650c2554be89bd7aee39cbda0b8"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "21 3.687"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" thru_hole oval
			(at 0.86 -49.5295 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "EXT_CHAIN")
		)
		(pad "2" thru_hole oval
			(at 0.86 -46.99 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "EXT_CHAIN")
		)
		(pad "3" thru_hole rect
			(at 0.86 -44.4495 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "4" thru_hole oval
			(at 0.86 -41.9095 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "CHAN_0")
		)
		(pad "5" thru_hole oval
			(at 0.86 -39.3695 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "CHAN_1")
		)
		(pad "6" thru_hole oval
			(at 0.86 -36.8295 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "CHAN_2")
		)
		(pad "7" thru_hole oval
			(at 0.86 -34.2895 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "CHAN_3")
		)
		(pad "8" thru_hole rect
			(at 0.86 -31.7495 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "9" thru_hole oval
			(at 0.86 -29.2095 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "CHAN_4")
		)
		(pad "10" thru_hole oval
			(at 0.86 -26.6695 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "CHAN_5")
		)
		(pad "11" thru_hole oval
			(at 0.86 -24.1295 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "CHAN_6")
		)
		(pad "12" thru_hole oval
			(at 0.86 -21.5895 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "CHAN_7")
		)
		(pad "13" thru_hole rect
			(at 0.86 -19.0495 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "14" thru_hole oval
			(at 0.86 -16.5095 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "CHAN_8")
		)
		(pad "15" thru_hole oval
			(at 0.86 -13.9695 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "CHAN_9")
		)
		(pad "16" thru_hole oval
			(at 0.86 -11.4295 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "CHAN_10")
		)
		(pad "17" thru_hole oval
			(at 0.86 -8.8895 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "CHAN_11")
		)
		(pad "18" thru_hole rect
			(at 0.86 -6.3495 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "19" thru_hole oval
			(at 0.86 -3.8095 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "CHAN_12")
		)
		(pad "20" thru_hole oval
			(at 0.86 -1.2695 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "CHAN_13")
		)
		(pad "21" thru_hole oval
			(at 20.04 -1.2695 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "CHAN_14")
		)
		(pad "22" thru_hole oval
			(at 20.04 -3.8095 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "CHAN_15")
		)
		(pad "23" thru_hole rect
			(at 20.04 -6.3495 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "24" thru_hole oval
			(at 20.04 -8.8895 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "CHAN_16")
		)
		(pad "25" thru_hole oval
			(at 20.04 -11.4295 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "CHAN_17")
		)
		(pad "26" thru_hole oval
			(at 20.04 -13.9695 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "CHAN_18")
		)
		(pad "27" thru_hole oval
			(at 20.04 -16.5095 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "CHAN_19")
		)
		(pad "28" thru_hole rect
			(at 20.04 -19.0495 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "29" thru_hole oval
			(at 20.04 -21.5895 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "CHAN_20")
		)
		(pad "30" thru_hole oval
			(at 20.04 -24.1295 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "31" thru_hole oval
			(at 20.04 -26.6695 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "CHAN_21")
		)
		(pad "32" thru_hole oval
			(at 20.04 -29.2095 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "CHAN_22")
		)
		(pad "33" thru_hole rect
			(at 20.04 -31.7495 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "34" thru_hole oval
			(at 20.04 -34.2895 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "CHAN_23")
		)
		(pad "35" thru_hole oval
			(at 20.04 -36.8295 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "36" thru_hole oval
			(at 20.04 -39.3695 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "+3.3V")
		)
		(pad "37" thru_hole oval
			(at 20.04 -41.9095 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "38" thru_hole rect
			(at 20.04 -44.4495 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
		(pad "39" thru_hole oval
			(at 20.04 -46.9895 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "40" thru_hole oval
			(at 20.04 -49.5295 90)
			(size 3.2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "+5V")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/树莓派pico.step"
			(offset
				(xyz 10.5 52.3 2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -0)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "F.Cu")
		(at 145.9235 121.9115 -90)
		(property "Reference" "R9"
			(at -1.4615 -0.864 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "CHAN_7")
		)
		(pad "2" smd rect
			(at 0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "$1N6760")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "F.Cu")
		(at 151.003 121.9115 -90)
		(property "Reference" "R11"
			(at -1.4615 -0.864 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "CHAN_9")
		)
		(pad "2" smd rect
			(at 0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "$1N6850")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "F.Cu")
		(at 143.3805 118.361 90)
		(property "Reference" "D7"
			(at -1.77 -1.7395 450)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "CHAN_6")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "F.Cu")
		(at 128.1455 121.9115 -90)
		(property "Reference" "R2"
			(at -1.4615 -0.8635 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "CHAN_0")
		)
		(pad "2" smd rect
			(at 0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "$1N6412")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "F.Cu")
		(at 135.788 115.2845 90)
		(property "Reference" "D4"
			(at -1.77 -1.739 450)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "CHAN_3")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "F.Cu")
		(at 156.0825 121.9115 -90)
		(property "Reference" "R13"
			(at -1.4615 -0.864 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "CHAN_11")
		)
		(pad "2" smd rect
			(at 0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "$1N6940")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:HDR-TH_30P-P2.54-V-F-R2-C15-S2.54-A"
		(layer "F.Cu")
		(at 144.599 127.814 90)
		(property "Reference" "U3"
			(at -15.667 -2.247 450)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd oval
			(at 0.337 -16.4535)
			(size 1.524 3.556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "$1N6412")
		)
		(pad "2" smd oval
			(at 0.337 -13.9135)
			(size 1.524 3.556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "$1N6457")
		)
		(pad "3" smd oval
			(at 0.337 -11.3735)
			(size 1.524 3.556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "$1N6576")
		)
		(pad "4" smd oval
			(at 0.337 -8.8335)
			(size 1.524 3.556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "$1N6580")
		)
		(pad "5" smd oval
			(at 0.337 -6.2935)
			(size 1.524 3.556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "$1N6666")
		)
		(pad "6" smd oval
			(at 0.337 -3.7535)
			(size 1.524 3.556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "$1N6670")
		)
		(pad "7" smd oval
			(at 0.337 -1.2135)
			(size 1.524 3.556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "$1N6756")
		)
		(pad "8" smd oval
			(at 0.337 1.3265)
			(size 1.524 3.556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "$1N6760")
		)
		(pad "9" smd oval
			(at 0.337 3.8665)
			(size 1.524 3.556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "$1N6846")
		)
		(pad "10" smd oval
			(at 0.337 6.4065)
			(size 1.524 3.556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "$1N6850")
		)
		(pad "11" smd oval
			(at 0.337 8.9465)
			(size 1.524 3.556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "$1N6936")
		)
		(pad "12" smd oval
			(at 0.337 11.4865)
			(size 1.524 3.556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "$1N6940")
		)
		(pad "13" smd oval
			(at 0.337 14.0265)
			(size 1.524 3.556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
		)
		(pad "14" smd oval
			(at 0.337 16.5665)
			(size 1.524 3.556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "EXT_T")
		)
		(pad "15" smd oval
			(at 0.337 19.1065)
			(size 1.524 3.556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "EXT_T")
		)
		(pad "16" smd oval
			(at 0.337 19.1065 180)
			(size 1.524 3.556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 28 "+5V")
		)
		(pad "17" smd oval
			(at 0.337 16.5665 180)
			(size 1.524 3.556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "+3.3V")
		)
		(pad "18" smd oval
			(at 0.337 14.0265 180)
			(size 1.524 3.556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "GND")
		)
		(pad "19" smd oval
			(at 0.337 11.4865 180)
			(size 1.524 3.556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 42 "$1N7395")
		)
		(pad "20" smd oval
			(at 0.337 8.9465 180)
			(size 1.524 3.556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 43 "$1N7399")
		)
		(pad "21" smd oval
			(at 0.337 6.4065 180)
			(size 1.524 3.556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 44 "$1N7403")
		)
		(pad "22" smd oval
			(at 0.337 3.8665 180)
			(size 1.524 3.556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 45 "$1N7407")
		)
		(pad "23" smd oval
			(at 0.337 1.3265 180)
			(size 1.524 3.556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 46 "$1N7411")
		)
		(pad "24" smd oval
			(at 0.337 -1.2135 180)
			(size 1.524 3.556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 47 "$1N7415")
		)
		(pad "25" smd oval
			(at 0.337 -3.7535 180)
			(size 1.524 3.556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 48 "$1N7419")
		)
		(pad "26" smd oval
			(at 0.337 -6.2935 180)
			(size 1.524 3.556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 49 "$1N7423")
		)
		(pad "27" smd oval
			(at 0.337 -8.8335 180)
			(size 1.524 3.556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 50 "$1N7427")
		)
		(pad "28" smd oval
			(at 0.337 -11.3735 180)
			(size 1.524 3.556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 51 "$1N7431")
		)
		(pad "29" smd oval
			(at 0.337 -13.9135 180)
			(size 1.524 3.556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 52 "$1N7435")
		)
		(pad "30" smd oval
			(at 0.337 -16.4535 180)
			(size 1.524 3.556)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 53 "$1N7439")
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "F.Cu")
		(at 140.863 115.2845 90)
		(property "Reference" "D6"
			(at -1.77 -1.7395 450)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "CHAN_5")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "F.Cu")
		(at 138.302 118.361 90)
		(property "Reference" "D5"
			(at -1.77 -1.739 450)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "CHAN_4")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "F.Cu")
		(at 130.685 121.9115 -90)
		(property "Reference" "R3"
			(at -1.4615 -0.864 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "CHAN_1")
		)
		(pad "2" smd rect
			(at 0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "$1N6457")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "F.Cu")
		(at 153.543 121.9115 -90)
		(property "Reference" "R12"
			(at -1.4615 -0.8635 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "CHAN_10")
		)
		(pad "2" smd rect
			(at 0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "$1N6936")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "F.Cu")
		(at 133.225 121.9115 -90)
		(property "Reference" "R4"
			(at -1.4615 -0.8635 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "CHAN_2")
		)
		(pad "2" smd rect
			(at 0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "$1N6576")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "F.Cu")
		(at 130.7135 115.2845 90)
		(property "Reference" "D1"
			(at -1.77 -1.7395 450)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "CHAN_1")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "F.Cu")
		(at 145.938 115.2845 90)
		(property "Reference" "D8"
			(at -1.77 -1.7395 450)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "CHAN_7")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "F.Cu")
		(at 151.0125 115.2845 90)
		(property "Reference" "D10"
			(at -1.77 -1.739 450)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "CHAN_9")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "F.Cu")
		(at 153.537 118.361 90)
		(property "Reference" "D11"
			(at -1.77 -1.739 450)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "CHAN_10")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "F.Cu")
		(at 135.7645 121.9115 -90)
		(property "Reference" "R5"
			(at -1.4615 -0.864 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "CHAN_3")
		)
		(pad "2" smd rect
			(at 0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "$1N6580")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "F.Cu")
		(at 156.0875 115.2845 90)
		(property "Reference" "D12"
			(at -1.77 -1.7395 450)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "CHAN_11")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "F.Cu")
		(at 124.475 117.7805 90)
		(property "Reference" "R1"
			(at -1.461 -0.8635 810)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 90)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 0.7535 0 90)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "EXT_T")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "F.Cu")
		(at 138.3045 121.9115 -90)
		(property "Reference" "R6"
			(at -1.4615 -0.8635 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "CHAN_4")
		)
		(pad "2" smd rect
			(at 0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "$1N6666")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOD-80_L3.5-W1.5-RD"
		(layer "F.Cu")
		(at 124.475 113.449 90)
		(property "Reference" "D2"
			(at -2.485 -1.029 810)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "27d27552bafd41ceb1963a6ed4584087"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "3.302 1.5995"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.765 0 90)
			(size 1.44 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "EXT_T")
		)
		(pad "2" smd rect
			(at 1.765 0 90)
			(size 1.44 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "EXT_CHAIN")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOD-80_BD1.5-L3.5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -0)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "F.Cu")
		(at 140.844 121.9115 -90)
		(property "Reference" "R7"
			(at -1.4615 -0.864 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "CHAN_5")
		)
		(pad "2" smd rect
			(at 0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "$1N6670")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "F.Cu")
		(at 148.4635 121.9115 -90)
		(property "Reference" "R10"
			(at -1.4615 -0.8635 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "CHAN_8")
		)
		(pad "2" smd rect
			(at 0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "$1N6846")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "F.Cu")
		(at 128.1455 118.361 90)
		(property "Reference" "D25"
			(at -1.77 -1.7395 1170)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "CHAN_0")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:HDR-TH_3P-P2.54-V-M"
		(layer "F.Cu")
		(at 121.4715 115.0945 -90)
		(property "Reference" "H2"
			(at -4.147 -1.524 990)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "bb473b6d38ff42a99216a4fcdbdcc4cb"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "7.62 2.54"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at -2.54 0 270)
			(size 1.7 1.7)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "EXT_CHAIN")
		)
		(pad "2" thru_hole circle
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(thermal_bridge_angle 90)
		)
		(pad "3" thru_hole circle
			(at 2.54 0 270)
			(size 1.7 1.7)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(thermal_bridge_angle 90)
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/HDR-TH_3P-P2.54-M-LI-1X3P.step"
			(offset
				(xyz 0 0 -3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -0)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "F.Cu")
		(at 148.459 118.361 90)
		(property "Reference" "D9"
			(at -1.77 -1.7395 450)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "CHAN_8")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "F.Cu")
		(at 143.384 121.9115 -90)
		(property "Reference" "R8"
			(at -1.4615 -0.8635 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "CHAN_6")
		)
		(pad "2" smd rect
			(at 0.7535 0 270)
			(size 0.8065 0.864)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "$1N6756")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:HDR-TH_3P-P2.54-V-F"
		(layer "F.Cu")
		(at 169.991 115.3045 -90)
		(property "Reference" "H1"
			(at -3.937 -1.524 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "f3b3cc5aae9641bf9e56fc160cef875b"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "7.62 2.54"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at -2.54 0 270)
			(size 1.575 1.575)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "EXT_CHAIN")
		)
		(pad "2" thru_hole circle
			(at 0 0 270)
			(size 1.575 1.575)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(thermal_bridge_angle 90)
		)
		(pad "3" thru_hole circle
			(at 2.54 0 270)
			(size 1.575 1.575)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(thermal_bridge_angle 90)
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/HDR2.54-F-LI-1X3P.step"
			(offset
				(xyz 0 0 -3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -0)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "B.Cu")
		(at 143.3805 118.361 90)
		(property "Reference" "D18"
			(at -1.77 1.7395 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 18 "CHAN_17")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "B.Cu")
		(at 148.459 118.361 90)
		(property "Reference" "D16"
			(at -1.77 1.739 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 20 "CHAN_15")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "B.Cu")
		(at 130.701 121.9115 90)
		(property "Reference" "R15"
			(at -1.4615 0.864 270)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 52 "$1N7435")
		)
		(pad "2" smd rect
			(at 0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 22 "CHAN_22")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "B.Cu")
		(at 135.788 115.2845 90)
		(property "Reference" "D21"
			(at -1.77 1.7395 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 24 "CHAN_20")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "B.Cu")
		(at 156.0875 115.2845 90)
		(property "Reference" "D13"
			(at -1.77 1.7395 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 13 "CHAN_12")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "B.Cu")
		(at 151.0065 121.9115 90)
		(property "Reference" "R23"
			(at -1.4615 0.8635 270)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 44 "$1N7403")
		)
		(pad "2" smd rect
			(at 0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 21 "CHAN_14")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "B.Cu")
		(at 148.468 121.9115 90)
		(property "Reference" "R22"
			(at -1.4615 0.864 270)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 45 "$1N7407")
		)
		(pad "2" smd rect
			(at 0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 20 "CHAN_15")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "B.Cu")
		(at 145.93 121.9115 90)
		(property "Reference" "R21"
			(at -1.4615 0.864 270)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 46 "$1N7411")
		)
		(pad "2" smd rect
			(at 0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 19 "CHAN_16")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "B.Cu")
		(at 153.537 118.361 90)
		(property "Reference" "D14"
			(at -1.77 1.7395 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 12 "CHAN_13")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "B.Cu")
		(at 130.7135 115.2845 90)
		(property "Reference" "D23"
			(at -1.77 1.7395 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 22 "CHAN_22")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "B.Cu")
		(at 133.224 118.361 90)
		(property "Reference" "D22"
			(at -1.77 1.739 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 23 "CHAN_21")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "B.Cu")
		(at 133.239 121.9115 90)
		(property "Reference" "R16"
			(at -1.4615 0.864 270)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 51 "$1N7431")
		)
		(pad "2" smd rect
			(at 0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 23 "CHAN_21")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "B.Cu")
		(at 143.392 121.9115 90)
		(property "Reference" "R20"
			(at -1.4615 0.8635 270)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 47 "$1N7415")
		)
		(pad "2" smd rect
			(at 0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 18 "CHAN_17")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "B.Cu")
		(at 156.0825 121.9115 90)
		(property "Reference" "R25"
			(at -1.4615 0.864 270)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 42 "$1N7395")
		)
		(pad "2" smd rect
			(at 0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 13 "CHAN_12")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "B.Cu")
		(at 145.938 115.2845 90)
		(property "Reference" "D17"
			(at -1.77 1.739 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 19 "CHAN_16")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "B.Cu")
		(at 128.1455 118.361 90)
		(property "Reference" "D24"
			(at -1.77 1.7395 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 26 "CHAN_23")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "B.Cu")
		(at 128.163 121.9115 90)
		(property "Reference" "R14"
			(at -1.4615 0.8635 630)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 53 "$1N7439")
		)
		(pad "2" smd rect
			(at 0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 26 "CHAN_23")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "B.Cu")
		(at 140.863 115.2845 90)
		(property "Reference" "D19"
			(at -1.77 1.7395 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 17 "CHAN_18")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "B.Cu")
		(at 151.0125 115.2845 90)
		(property "Reference" "D15"
			(at -1.77 1.7395 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 21 "CHAN_14")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:SOT-23-3_L2.9-W1.6-P1.90-LS2.8-BR"
		(layer "B.Cu")
		(at 138.302 118.361 90)
		(property "Reference" "D20"
			(at -1.77 1.7395 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "89cb27a44ab2466697082bb9fd73a7d0"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "2.8 2.9"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.235 -0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "GND")
		)
		(pad "2" smd rect
			(at 1.235 0.95 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "+3.3V")
		)
		(pad "3" smd rect
			(at -1.235 0 90)
			(size 1.07 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 25 "CHAN_19")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOT-23-3L_L2.9-W1.6-H1.1-LS2.8-P0.95.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "B.Cu")
		(at 153.5445 121.9115 90)
		(property "Reference" "R24"
			(at -1.4615 0.8635 270)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 43 "$1N7399")
		)
		(pad "2" smd rect
			(at 0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 12 "CHAN_13")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "B.Cu")
		(at 138.3155 121.9115 90)
		(property "Reference" "R18"
			(at -1.4615 0.864 270)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 49 "$1N7423")
		)
		(pad "2" smd rect
			(at 0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 25 "CHAN_19")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "B.Cu")
		(at 140.8535 121.9115 90)
		(property "Reference" "R19"
			(at -1.4615 0.864 270)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 48 "$1N7419")
		)
		(pad "2" smd rect
			(at 0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 17 "CHAN_18")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "AnalyzerBoxPCB_fork:R0603"
		(layer "B.Cu")
		(at 135.7775 121.9115 90)
		(property "Reference" "R17"
			(at -1.4615 0.8635 270)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "JLC_3DModel_Q" "fc143cca1e79419f9cd78b61e9279f08"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(property "JLC_3D_Size" "0.81 1.62"
			(at 0 0 -90)
			(unlocked yes)
			(layer "Cmts.User")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 50 "$1N7427")
		)
		(pad "2" smd rect
			(at 0.7535 0 90)
			(size 0.8065 0.864)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 24 "CHAN_20")
		)
		(model "${KIPRJMOD}/EASYEDA_MODELS/R0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(gr_arc
		(start 172.3375 126.727)
		(mid 171.444761 128.882261)
		(end 169.2895 129.775)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 169.2895 81.831)
		(mid 171.444761 82.723739)
		(end 172.3375 84.879)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.666 129.775)
		(end 169.2895 129.775)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.3375 126.727)
		(end 172.3375 84.879)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 119.618 126.727)
		(end 119.618 84.879001)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 119.618 84.879001)
		(mid 120.510739 82.723739)
		(end 122.666002 81.831)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 122.666 129.775)
		(mid 120.510739 128.882261)
		(end 119.618 126.727)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.666002 81.831)
		(end 169.2895 81.831)
		(layer "Edge.Cuts")
	)
	(gr_text "GND"
		(at 159.624 124.92 -0)
		(layer "B.SilkS")
	)
	(gr_text "14"
		(at 154.29 125.0215 -0)
		(layer "B.SilkS")
	)
	(gr_text "13"
		(at 156.881 125.0725 -0)
		(layer "B.SilkS")
	)
	(gr_text "22"
		(at 134.173 125.174 -0)
		(layer "B.SilkS")
	)
	(gr_text "16"
		(at 149.21 125.0725 -0)
		(layer "B.SilkS")
	)
	(gr_text "23"
		(at 131.684 125.174 -0)
		(layer "B.SilkS")
	)
	(gr_text "18"
		(at 144.079 125.123 -0)
		(layer "B.SilkS")
	)
	(gr_text "3V3"
		(at 162.215 124.971 -0)
		(layer "B.SilkS")
	)
	(gr_text "17"
		(at 146.67 125.123 -0)
		(layer "B.SilkS")
	)
	(gr_text "24"
		(at 129.093 125.123 -0)
		(layer "B.SilkS")
	)
	(gr_text "5V"
		(at 164.399 124.971 -0)
		(layer "B.SilkS")
	)
	(gr_text "15"
		(at 151.75 125.0725 -0)
		(layer "B.SilkS")
	)
	(gr_text "20"
		(at 139.253 125.174 -0)
		(layer "B.SilkS")
	)
	(gr_text "21"
		(at 136.6625 125.174 -0)
		(layer "B.SilkS")
	)
	(gr_text "19"
		(at 141.4885 125.174 -0)
		(layer "B.SilkS")
	)
	(gr_text "BAV99"
		(at 129.093 113.1345 0)
		(layer "F.SilkS")
	)
	(gr_text "JasonYANG17 V1.2"
		(at 145.5525 111.966 0)
		(layer "F.SilkS")
	)
	(gr_text "4"
		(at 135.189 125.225 1080)
		(layer "F.SilkS")
	)
	(gr_text "100k"
		(at 123.353 120.348 0)
		(layer "F.SilkS")
	)
	(gr_text "8"
		(at 145.451 125.123 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 157.541 124.92 0)
		(layer "F.SilkS")
	)
	(gr_text "EXT_CHAIN"
		(at 120.0655 110.6895 360)
		(layer "F.SilkS")
	)
	(gr_text "9"
		(at 148.0415 125.0215 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 120.4015 120.557 360)
		(layer "F.SilkS")
	)
	(gr_text "12"
		(at 155.357 125.0725 0)
		(layer "F.SilkS")
	)
	(gr_text "6"
		(at 140.4215 125.174 0)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 130.3125 125.225 1080)
		(layer "F.SilkS")
	)
	(gr_text "EXT_CHAIN"
		(at 162.1295 113.2655 360)
		(layer "F.SilkS")
	)
	(gr_text "5"
		(at 137.831 125.225 1080)
		(layer "F.SilkS")
	)
	(gr_text "3"
		(at 132.751 125.2755 1080)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 166.257 118.445 360)
		(layer "F.SilkS")
	)
	(gr_text "NC"
		(at 166.991 115.83 360)
		(layer "F.SilkS")
	)
	(gr_text "7"
		(at 143.0125 125.174 0)
		(layer "F.SilkS")
	)
	(gr_text "EXT_T"
		(at 160.5385 124.971 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 127.823 125.225 1080)
		(layer "F.SilkS")
	)
	(gr_text "10"
		(at 150.226 125.0725 0)
		(layer "F.SilkS")
	)
	(gr_text "JLCJLCJLCJLC"
		(at 170.87 101.7545 90)
		(layer "F.SilkS")
	)
	(gr_text "11"
		(at 152.9185 125.0215 0)
		(layer "F.SilkS")
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 139.261 102.261978) (xy 139.261 104.921022) (xy 140.066 104.921022) (xy 140.066 102.261978)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 164.661 102.261978) (xy 164.661 104.921022) (xy 165.466 104.921022) (xy 165.466 102.261978)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 168.550177 117.4485) (xy 168.550177 118.241) (xy 170.384664 118.241) (xy 170.384664 117.4485)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 120.6365 82.85) (xy 120.6365 128.7565) (xy 171.319 128.7565) (xy 171.319 82.85)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 126.561 102.261978) (xy 126.561 104.921022) (xy 127.366 104.921022) (xy 127.366 102.261978)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 151.961 83.081978) (xy 151.961 85.741022) (xy 152.766 85.741022) (xy 152.766 83.081978)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 121.046632 117.207) (xy 121.046632 118.062) (xy 123.005368 118.062) (xy 123.005368 117.207)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 169.595 116.404435) (xy 169.595 118.238823) (xy 170.3875 118.238823) (xy 170.3875 116.404435)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 139.261 104.120978) (xy 139.261 106.780022) (xy 140.066 106.780022) (xy 140.066 104.120978)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 126.561 104.120978) (xy 126.561 106.780022) (xy 127.366 106.780022) (xy 127.366 104.120978)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 121.044 117.209632) (xy 121.044 119.168868) (xy 121.899 119.168868) (xy 121.899 117.209632)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 126.561 83.081978) (xy 126.561 85.741022) (xy 127.366 85.741022) (xy 127.366 83.081978)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 164.661 84.940978) (xy 164.661 87.600022) (xy 165.466 87.600022) (xy 165.466 84.940978)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 151.961 102.261978) (xy 151.961 104.921022) (xy 152.766 104.921022) (xy 152.766 102.261978)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 164.661 104.120978) (xy 164.661 106.780022) (xy 165.466 106.780022) (xy 165.466 104.120978)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 126.561 84.940978) (xy 126.561 87.600022) (xy 127.366 87.600022) (xy 127.366 84.940978)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 151.961 84.940978) (xy 151.961 87.600022) (xy 152.766 87.600022) (xy 152.766 84.940978)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 151.961 104.120978) (xy 151.961 106.780022) (xy 152.766 106.780022) (xy 152.766 104.120978)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 169.595 117.450935) (xy 169.595 119.285323) (xy 170.3875 119.285323) (xy 170.3875 117.450935)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 164.661 83.081978) (xy 164.661 85.741022) (xy 165.466 85.741022) (xy 165.466 83.081978)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 118.482 131.2935) (xy 118.482 76.3975) (xy 173.378 76.3975) (xy 173.378 131.2935)
			)
		)
	)
	(zone
		(net 28)
		(net_name "+5V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 162.9095 125.702) (xy 162.9095 129.2735) (xy 165.7535 129.2735) (xy 165.7535 125.702)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "Edge.Cuts")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 120.6525 124.7375) (xy 120.6525 128.7255) (xy 124.6405 128.7255) (xy 124.6405 124.7375)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "Edge.Cuts")
		(hatch edge 0.5)
		(priority 500)
		(connect_pads
			(clearance 0.1015)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 167.0475 124.719) (xy 167.0475 128.707) (xy 171.0355 128.707) (xy 171.0355 124.719)
			)
		)
	)
)