(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "USLetter")
	(title_block
		(title "Pico-Analyzer - A RP2040 Powered Logic Analyzer")
		(date "2024-12-18")
		(rev "1.0")
		(company "Rex McKinnon")
		(comment 1 "- V_{ref} input supports 1.1v - 5.5v")
		(comment 2 "- Selectable 3.3v and 5v logic levels")
		(comment 3 "- 24 Digital Channels")
		(comment 4 "Features:")
	)
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" signal)
		(2 "In2.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.24)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "HAL SnPb")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.038)
		(solder_mask_min_width 0.1)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerbers")
		)
	)
	(net 0 "")
	(net 1 "+5V")
	(net 2 "Net-(D1-DIN)")
	(net 3 "unconnected-(D1-DOUT-Pad2)")
	(net 4 "GND")
	(net 5 "/Level Translation/C4")
	(net 6 "/Level Translation/C5")
	(net 7 "/Level Translation/C2")
	(net 8 "/Level Translation/C3")
	(net 9 "/Level Translation/C1")
	(net 10 "/Level Translation/C0")
	(net 11 "/Level Translation/C10")
	(net 12 "/Level Translation/C11")
	(net 13 "/Level Translation/C9")
	(net 14 "/Level Translation/C8")
	(net 15 "/Level Translation/C7")
	(net 16 "/Level Translation/C6")
	(net 17 "/Level Translation/C13")
	(net 18 "/Level Translation/C17")
	(net 19 "/Level Translation/C12")
	(net 20 "/Level Translation/C15")
	(net 21 "/Level Translation/C14")
	(net 22 "/Level Translation/C16")
	(net 23 "/Level Translation/C23")
	(net 24 "/Level Translation/C21")
	(net 25 "/Level Translation/C18")
	(net 26 "/Level Translation/C22")
	(net 27 "/Level Translation/C19")
	(net 28 "/Level Translation/C20")
	(net 29 "Net-(JP1-A)")
	(net 30 "Net-(JP1-B)")
	(net 31 "+3V3")
	(net 32 "unconnected-(U1-NC-Pad6)")
	(net 33 "/Level Translation/I2")
	(net 34 "unconnected-(U1-NC-Pad9)")
	(net 35 "/Level Translation/I3")
	(net 36 "/Level Translation/I1")
	(net 37 "/Level Translation/I0")
	(net 38 "/Level Translation/I6")
	(net 39 "unconnected-(U2-NC-Pad6)")
	(net 40 "/Level Translation/I4")
	(net 41 "/Level Translation/I5")
	(net 42 "unconnected-(U2-NC-Pad9)")
	(net 43 "/Level Translation/I7")
	(net 44 "/Level Translation/I9")
	(net 45 "unconnected-(U3-NC-Pad6)")
	(net 46 "/Level Translation/I8")
	(net 47 "/Level Translation/I10")
	(net 48 "/Level Translation/I11")
	(net 49 "unconnected-(U3-NC-Pad9)")
	(net 50 "/Level Translation/I15")
	(net 51 "/Level Translation/I13")
	(net 52 "/Level Translation/I12")
	(net 53 "unconnected-(U4-NC-Pad9)")
	(net 54 "unconnected-(U4-NC-Pad6)")
	(net 55 "/Level Translation/I14")
	(net 56 "/Level Translation/I19")
	(net 57 "/Level Translation/I18")
	(net 58 "unconnected-(U5-NC-Pad9)")
	(net 59 "unconnected-(U5-NC-Pad6)")
	(net 60 "/Level Translation/I17")
	(net 61 "/Level Translation/I16")
	(net 62 "unconnected-(U6-NC-Pad9)")
	(net 63 "/Level Translation/I22")
	(net 64 "/Level Translation/I21")
	(net 65 "/Level Translation/I20")
	(net 66 "/Level Translation/I23")
	(net 67 "unconnected-(U6-NC-Pad6)")
	(net 68 "unconnected-(U7-GPIO27-Pad28)")
	(net 69 "unconnected-(U7-BOOTSEL-Pad40)")
	(net 70 "unconnected-(U7-~{RESET}-Pad39)")
	(net 71 "unconnected-(U7-GPIO28-Pad29)")
	(net 72 "Net-(J5-CC2)")
	(net 73 "Net-(J5-CC1)")
	(net 74 "unconnected-(U7-SWCLK-Pad38)")
	(net 75 "unconnected-(U7-VBAT-Pad32)")
	(net 76 "unconnected-(U7-GPIO29-Pad30)")
	(net 77 "unconnected-(U7-SWDIO-Pad37)")
	(net 78 "Net-(U7-USB_D+)")
	(net 79 "Net-(U7-USB_D-)")
	(net 80 "unconnected-(J5-SBU2-PadB8)")
	(net 81 "unconnected-(J5-SBU1-PadA8)")
	(net 82 "V_{ref}")
	(net 83 "V_{in}")
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 135.369 99.822 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_Small"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Translation")
		(sheetfile "pico-analyzer-translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kibuzzard-676315DE"
		(layer "F.Cu")
		(at 143.383 115.824)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiWyIsICJDYXBSaWdodENob2ljZSI6ICJdIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIkdORCIsICJQYWRkaW5nQm90dG9tQ3RybCI6IDEuMCwgIlBhZGRpbmdMZWZ0Q3RybCI6IDMuMCwgIlBhZGRpbmdSaWdodEN0cmwiOiAzLjAsICJQYWRkaW5nVG9wQ3RybCI6IDEuMCwgIldpZHRoQ3RybCI6IDAuMCwgImFkdmFuY2VkQ2hlY2tib3giOiBmYWxzZSwgImlubGluZUZvcm1hdFRleHRib3giOiBmYWxzZSwgImxpbmVvdmVyU3R5bGVDaG9pY2UiOiAiU3F1YXJlIiwgImxpbmVvdmVyVGhpY2tuZXNzQ3RybCI6IDF9")
		(property "Reference" "kibuzzard-676315DE"
			(at 0 -3.704435 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.704435 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "kibuzzard-676317F6"
		(layer "F.Cu")
		(at 94.234 115.824)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjQiLCAiUGFkZGluZ0JvdHRvbUN0cmwiOiAxLjAsICJQYWRkaW5nTGVmdEN0cmwiOiAyLjUsICJQYWRkaW5nUmlnaHRDdHJsIjogMi41LCAiUGFkZGluZ1RvcEN0cmwiOiAxLjAsICJXaWR0aEN0cmwiOiAwLjAsICJhZHZhbmNlZENoZWNrYm94IjogZmFsc2UsICJpbmxpbmVGb3JtYXRUZXh0Ym94IjogZmFsc2UsICJsaW5lb3ZlclN0eWxlQ2hvaWNlIjogIlNxdWFyZSIsICJsaW5lb3ZlclRoaWNrbmVzc0N0cmwiOiAxfQ==")
		(property "Reference" "kibuzzard-676317F6"
			(at 0 -3.682626 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.682626 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "kibuzzard-67631765"
		(layer "F.Cu")
		(at 106.426 117.602)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjkiLCAiUGFkZGluZ0JvdHRvbUN0cmwiOiAxLjAsICJQYWRkaW5nTGVmdEN0cmwiOiAyLjUsICJQYWRkaW5nUmlnaHRDdHJsIjogMi41LCAiUGFkZGluZ1RvcEN0cmwiOiAxLjAsICJXaWR0aEN0cmwiOiAwLjAsICJhZHZhbmNlZENoZWNrYm94IjogZmFsc2UsICJpbmxpbmVGb3JtYXRUZXh0Ym94IjogZmFsc2UsICJsaW5lb3ZlclN0eWxlQ2hvaWNlIjogIlNxdWFyZSIsICJsaW5lb3ZlclRoaWNrbmVzc0N0cmwiOiAxfQ==")
		(property "Reference" "kibuzzard-67631765"
			(at 0 -3.697165 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.697165 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "kibuzzard-6763120A"
		(layer "F.Cu")
		(at 121.666 115.824)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjE0IiwgIlBhZGRpbmdCb3R0b21DdHJsIjogMS4wLCAiUGFkZGluZ0xlZnRDdHJsIjogMC4wLCAiUGFkZGluZ1JpZ2h0Q3RybCI6IDAuMCwgIlBhZGRpbmdUb3BDdHJsIjogMS4wLCAiV2lkdGhDdHJsIjogMC4wLCAiYWR2YW5jZWRDaGVja2JveCI6IGZhbHNlLCAiaW5saW5lRm9ybWF0VGV4dGJveCI6IGZhbHNlLCAibGluZW92ZXJTdHlsZUNob2ljZSI6ICJTcXVhcmUiLCAibGluZW92ZXJUaGlja25lc3NDdHJsIjogMX0=")
		(property "Reference" "kibuzzard-6763120A"
			(at 0 -3.682626 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.682626 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "kibuzzard-6763155B"
		(layer "F.Cu")
		(at 133.858 115.824)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjE4IiwgIlBhZGRpbmdCb3R0b21DdHJsIjogMS4wLCAiUGFkZGluZ0xlZnRDdHJsIjogMC4wLCAiUGFkZGluZ1JpZ2h0Q3RybCI6IDAuMCwgIlBhZGRpbmdUb3BDdHJsIjogMS4wLCAiV2lkdGhDdHJsIjogMC4wLCAiYWR2YW5jZWRDaGVja2JveCI6IGZhbHNlLCAiaW5saW5lRm9ybWF0VGV4dGJveCI6IGZhbHNlLCAibGluZW92ZXJTdHlsZUNob2ljZSI6ICJTcXVhcmUiLCAibGluZW92ZXJUaGlja25lc3NDdHJsIjogMX0=")
		(property "Reference" "kibuzzard-6763155B"
			(at 0 -3.705243 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.705243 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "pico-analyzer:USB_C_Receptacle_GCT_USB4215-xx-A_16P"
		(layer "F.Cu")
		(at 115.57 54.0512 180)
		(descr "USB 2.0 Type C Receptacle, GCT, 16P, top mounted, horizontal, 5A: https://gct.co/files/drawings/usb4105.pdf")
		(tags "USB C Type-C Receptacle SMD USB 2.0 16P 16C USB4105-15-A USB4105-15-A-060 USB4105-15-A-120 USB4105-GF-A USB4105-GF-A-060 USB4105-GF-A-120")
		(property "Reference" "J5"
			(at 0 -5.5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USB_C_Receptacle_USB2.0_16P"
			(at 0 4.445 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "pico-analyzer:USB_C_Receptacle_GCT_USB4215-xx-A_16P"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "USB 2.0-only 16P Type-C Receptacle connector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "USB*C*Receptacle*")
		(sheetname "Root")
		(sheetfile "pico-analyzer.kicad_sch")
		(attr smd)
		(fp_text user "PCB Edge"
			(at 0 2.54 180)
			(unlocked yes)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "A1" smd roundrect
			(at -3.2 -3.425 180)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "A4" smd roundrect
			(at -2.4 -3.425 180)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "A5" smd roundrect
			(at -1.25 -3.425 180)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 73 "Net-(J5-CC1)")
			(pinfunction "CC1")
			(pintype "bidirectional")
		)
		(pad "A6" smd roundrect
			(at -0.25 -3.425 180)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 78 "Net-(U7-USB_D+)")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "A7" smd roundrect
			(at 0.25 -3.425 180)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 79 "Net-(U7-USB_D-)")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "A8" smd roundrect
			(at 1.25 -3.425 180)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 81 "unconnected-(J5-SBU1-PadA8)")
			(pinfunction "SBU1")
			(pintype "bidirectional+no_connect")
		)
		(pad "A9" smd roundrect
			(at 2.4 -3.425 180)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "A12" smd roundrect
			(at 3.2 -3.425 180)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "B1" smd roundrect
			(at 3.2 -3.425 180)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "B4" smd roundrect
			(at 2.4 -3.425 180)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "B5" smd roundrect
			(at 1.75 -3.425 180)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 72 "Net-(J5-CC2)")
			(pinfunction "CC2")
			(pintype "bidirectional")
		)
		(pad "B6" smd roundrect
			(at 0.75 -3.425 180)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 78 "Net-(U7-USB_D+)")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "B7" smd roundrect
			(at -0.75 -3.425 180)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 79 "Net-(U7-USB_D-)")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "B8" smd roundrect
			(at -1.75 -3.425 180)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 80 "unconnected-(J5-SBU2-PadB8)")
			(pinfunction "SBU2")
			(pintype "bidirectional+no_connect")
		)
		(pad "B9" smd roundrect
			(at -2.4 -3.425 180)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "B12" smd roundrect
			(at -3.2 -3.425 180)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at -4.32 -2.85 180)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at -4.32 1.15 180)
			(size 1 2.2)
			(drill oval 0.6 1.8)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at 4.32 -2.85 180)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at 4.32 1.15 180)
			(size 1 2.2)
			(drill oval 0.6 1.8)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_GCT_USB4105-xx-A_16P_TopMnt_Horizontal.wrl"
			(offset
				(xyz 0 -0.25 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kibuzzard-6763127F"
		(layer "F.Cu")
		(at 121.666 117.602)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjE1IiwgIlBhZGRpbmdCb3R0b21DdHJsIjogMS4wLCAiUGFkZGluZ0xlZnRDdHJsIjogMC4wLCAiUGFkZGluZ1JpZ2h0Q3RybCI6IDAuMCwgIlBhZGRpbmdUb3BDdHJsIjogMS4wLCAiV2lkdGhDdHJsIjogMC4wLCAiYWR2YW5jZWRDaGVja2JveCI6IGZhbHNlLCAiaW5saW5lRm9ybWF0VGV4dGJveCI6IGZhbHNlLCAibGluZW92ZXJTdHlsZUNob2ljZSI6ICJTcXVhcmUiLCAibGluZW92ZXJUaGlja25lc3NDdHJsIjogMX0=")
		(property "Reference" "kibuzzard-6763127F"
			(at 0 -3.693127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.693127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "kibuzzard-67631565"
		(layer "F.Cu")
		(at 133.858 117.602)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjE5IiwgIlBhZGRpbmdCb3R0b21DdHJsIjogMS4wLCAiUGFkZGluZ0xlZnRDdHJsIjogMC4wLCAiUGFkZGluZ1JpZ2h0Q3RybCI6IDAuMCwgIlBhZGRpbmdUb3BDdHJsIjogMS4wLCAiV2lkdGhDdHJsIjogMC4wLCAiYWR2YW5jZWRDaGVja2JveCI6IGZhbHNlLCAiaW5saW5lRm9ybWF0VGV4dGJveCI6IGZhbHNlLCAibGluZW92ZXJTdHlsZUNob2ljZSI6ICJTcXVhcmUiLCAibGluZW92ZXJUaGlja25lc3NDdHJsIjogMX0=")
		(property "Reference" "kibuzzard-67631565"
			(at 0 -3.697165 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.697165 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 126.479 101.092 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_Small"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Translation")
		(sheetfile "pico-analyzer-translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 95.999 101.092 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at -0.013 1.778 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_Small"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Translation")
		(sheetfile "pico-analyzer-translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kibuzzard-67631277"
		(layer "F.Cu")
		(at 118.618 117.602)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjEzIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogMS4wLCAiUGFkZGluZ0xlZnRDdHJsIjogMC4wLCAiUGFkZGluZ1JpZ2h0Q3RybCI6IDAuMCwgIlBhZGRpbmdUb3BDdHJsIjogMS4wLCAiV2lkdGhDdHJsIjogMC4wLCAiYWR2YW5jZWRDaGVja2JveCI6IGZhbHNlLCAiaW5saW5lRm9ybWF0VGV4dGJveCI6IGZhbHNlLCAibGluZW92ZXJTdHlsZUNob2ljZSI6ICJTcXVhcmUiLCAibGluZW92ZXJUaGlja25lc3NDdHJsIjogMX0=")
		(property "Reference" "kibuzzard-67631277"
			(at 0 -3.704435 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.704435 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "kibuzzard-6763201C"
		(layer "F.Cu")
		(at 135.2804 64.008 90)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDIuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjNWMyIsICJQYWRkaW5nQm90dG9tQ3RybCI6IDIuMCwgIlBhZGRpbmdMZWZ0Q3RybCI6IDAuMCwgIlBhZGRpbmdSaWdodEN0cmwiOiAwLjAsICJQYWRkaW5nVG9wQ3RybCI6IDIuMCwgIldpZHRoQ3RybCI6IDAuMCwgImFkdmFuY2VkQ2hlY2tib3giOiBmYWxzZSwgImlubGluZUZvcm1hdFRleHRib3giOiBmYWxzZSwgImxpbmVvdmVyU3R5bGVDaG9pY2UiOiAiU3F1YXJlIiwgImxpbmVvdmVyVGhpY2tuZXNzQ3RybCI6IDF9")
		(property "Reference" "kibuzzard-6763201C"
			(at 0 -4.630122 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 4.630122 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 122.301 56.642 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -1.651 90)
			(layer "F.SilkS")
		)
		(property "Value" "5K1"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pico-analyzer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 73 "Net-(J5-CC1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kibuzzard-67631771"
		(layer "F.Cu")
		(at 103.378 117.602)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjciLCAiUGFkZGluZ0JvdHRvbUN0cmwiOiAxLjAsICJQYWRkaW5nTGVmdEN0cmwiOiAyLjUsICJQYWRkaW5nUmlnaHRDdHJsIjogMi41LCAiUGFkZGluZ1RvcEN0cmwiOiAxLjAsICJXaWR0aEN0cmwiOiAwLjAsICJhZHZhbmNlZENoZWNrYm94IjogZmFsc2UsICJpbmxpbmVGb3JtYXRUZXh0Ym94IjogZmFsc2UsICJsaW5lb3ZlclN0eWxlQ2hvaWNlIjogIlNxdWFyZSIsICJsaW5lb3ZlclRoaWNrbmVzc0N0cmwiOiAxfQ==")
		(property "Reference" "kibuzzard-67631771"
			(at 0 -3.682626 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.682626 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "pico-analyzer:PinHeader_2x04_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 88.89 120.396 -90)
		(descr "Through hole angled pin header, 2x04, 2.54mm pitch, 6mm pin length, double rows")
		(tags "Through hole angled pin header THT 2x04 2.54mm double row")
		(property "Reference" "J1"
			(at 1.27 2.56 90)
			(layer "F.SilkS")
		)
		(property "Value" "Channels 0-5"
			(at 5.655 2.27 90)
			(layer "F.Fab")
		)
		(property "Footprint" "pico-analyzer:PinHeader_2x04_P2.54mm_Horizontal"
			(at 0 -7.62 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 -7.62 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x04, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 -7.62 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "pico-analyzer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.31 -3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/Level Translation/C0")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/Level Translation/C1")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/Level Translation/C2")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/Level Translation/C3")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/Level Translation/C4")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/Level Translation/C5")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.54 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "V_{in}")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 7.62 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kibuzzard-6763156D"
		(layer "F.Cu")
		(at 136.906 115.824)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjIwIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogMS4wLCAiUGFkZGluZ0xlZnRDdHJsIjogMC4wLCAiUGFkZGluZ1JpZ2h0Q3RybCI6IDAuMCwgIlBhZGRpbmdUb3BDdHJsIjogMS4wLCAiV2lkdGhDdHJsIjogMC4wLCAiYWR2YW5jZWRDaGVja2JveCI6IGZhbHNlLCAiaW5saW5lRm9ybWF0VGV4dGJveCI6IGZhbHNlLCAibGluZW92ZXJTdHlsZUNob2ljZSI6ICJTcXVhcmUiLCAibGluZW92ZXJUaGlja25lc3NDdHJsIjogMX0=")
		(property "Reference" "kibuzzard-6763156D"
			(at 0 -3.704435 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.704435 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm"
		(layer "F.Cu")
		(at 87.96 63.5 -90)
		(descr "5.0mm x 5.0mm Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
		(tags "LED RGB NeoPixel PLCC-4 5050")
		(property "Reference" "D1"
			(at 2.286 -3.683 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WS2812B"
			(at 0 4 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*PLCC*5.0x5.0mm*P3.2mm*")
		(sheetname "Root")
		(sheetfile "pico-analyzer.kicad_sch")
		(attr smd)
		(fp_text user "1"
			(at -4.15 -1.6 90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.45 -1.65 270)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 1 "+5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.45 1.65 270)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 3 "unconnected-(D1-DOUT-Pad2)")
			(pinfunction "DOUT")
			(pintype "output+no_connect")
		)
		(pad "3" smd roundrect
			(at 2.45 1.65 270)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 4 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at 2.45 -1.65 270)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1)
			(net 2 "Net-(D1-DIN)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kibuzzard-67631586"
		(layer "F.Cu")
		(at 139.954 117.602)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjIzIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogMS4wLCAiUGFkZGluZ0xlZnRDdHJsIjogMC4wLCAiUGFkZGluZ1JpZ2h0Q3RybCI6IDAuMCwgIlBhZGRpbmdUb3BDdHJsIjogMS4wLCAiV2lkdGhDdHJsIjogMC4wLCAiYWR2YW5jZWRDaGVja2JveCI6IGZhbHNlLCAiaW5saW5lRm9ybWF0VGV4dGJveCI6IGZhbHNlLCAibGluZW92ZXJTdHlsZUNob2ljZSI6ICJTcXVhcmUiLCAibGluZW92ZXJUaGlja25lc3NDdHJsIjogMX0=")
		(property "Reference" "kibuzzard-67631586"
			(at 0 -3.704435 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.704435 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
		(layer "F.Cu")
		(at 121.95 104.902 90)
		(descr "TSSOP, 14 Pin (JEDEC MO-153 Var AB-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U4"
			(at 0 -3.45 90)
			(layer "F.SilkS")
		)
		(property "Value" "TXU0104PW"
			(at 0 3.45 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txu0104.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4-Bit Unidirectional Voltage-Level Translator, 1.1 - 5.5V A/BPort, TSSOP-14"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*14*5mm*P0.65mm*")
		(sheetname "Level Translation")
		(sheetfile "pico-analyzer-translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 82 "V_{ref}")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.8625 -1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "/Level Translation/C12")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.8625 -0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "/Level Translation/C13")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.8625 0 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "/Level Translation/C14")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.8625 0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "/Level Translation/C15")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.8625 1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 54 "unconnected-(U4-NC-Pad6)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "7" smd roundrect
			(at -2.8625 1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at 2.8625 1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "+3V3")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at 2.8625 1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 53 "unconnected-(U4-NC-Pad9)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "10" smd roundrect
			(at 2.8625 0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 50 "/Level Translation/I15")
			(pinfunction "B4")
			(pintype "output")
		)
		(pad "11" smd roundrect
			(at 2.8625 0 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 55 "/Level Translation/I14")
			(pinfunction "B3")
			(pintype "output")
		)
		(pad "12" smd roundrect
			(at 2.8625 -0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 51 "/Level Translation/I13")
			(pinfunction "B2")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at 2.8625 -1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 52 "/Level Translation/I12")
			(pinfunction "B1")
			(pintype "output")
		)
		(pad "14" smd roundrect
			(at 2.8625 -1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "+3V3")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2_DIN965"
		(layer "F.Cu")
		(at 149.86 114.3)
		(descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
		(tags "mounting hole 2.2mm no annular m2 din965")
		(property "Reference" "MH"
			(at 0 -2.9 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.2mm_M2_DIN965"
			(at 0 2.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_2.2mm_M2_DIN965"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 104.889 102.362 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_Small"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Translation")
		(sheetfile "pico-analyzer-translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 108.839 56.642 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 1.524 90)
			(layer "F.SilkS")
		)
		(property "Value" "5K1"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "pico-analyzer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 72 "Net-(J5-CC2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 87.109 104.902 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.778 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_Small"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Translation")
		(sheetfile "pico-analyzer-translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 82 "V_{ref}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2_DIN965"
		(layer "F.Cu")
		(at 81.28 63.5)
		(descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
		(tags "mounting hole 2.2mm no annular m2 din965")
		(property "Reference" "MH"
			(at 0 -2.9 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.2mm_M2_DIN965"
			(at 0 2.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_2.2mm_M2_DIN965"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "pico-analyzer:PinHeader_2x04_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 134.61 120.396 -90)
		(descr "Through hole angled pin header, 2x04, 2.54mm pitch, 6mm pin length, double rows")
		(tags "Through hole angled pin header THT 2x04 2.54mm double row")
		(property "Reference" "J4"
			(at 1.27 2.56 90)
			(layer "F.SilkS")
		)
		(property "Value" "Channels 18-23"
			(at 5.655 2.27 90)
			(layer "F.Fab")
		)
		(property "Footprint" "pico-analyzer:PinHeader_2x04_P2.54mm_Horizontal"
			(at 0 -7.62 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 -7.62 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x04, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 -7.62 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "pico-analyzer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.31 -3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/Level Translation/C18")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/Level Translation/C19")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/Level Translation/C20")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/Level Translation/C21")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/Level Translation/C22")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/Level Translation/C23")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.54 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "V_{in}")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 7.62 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pico-analyzer:PinHeader_2x04_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 104.13 120.396 -90)
		(descr "Through hole angled pin header, 2x04, 2.54mm pitch, 6mm pin length, double rows")
		(tags "Through hole angled pin header THT 2x04 2.54mm double row")
		(property "Reference" "J2"
			(at 1.27 2.56 90)
			(layer "F.SilkS")
		)
		(property "Value" "Channels 6-11"
			(at 5.655 2.27 90)
			(layer "F.Fab")
		)
		(property "Footprint" "pico-analyzer:PinHeader_2x04_P2.54mm_Horizontal"
			(at 0 -7.62 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 -7.62 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x04, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 -7.62 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "pico-analyzer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.31 -3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/Level Translation/C6")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/Level Translation/C7")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/Level Translation/C8")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/Level Translation/C9")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/Level Translation/C10")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/Level Translation/C11")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.54 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "V_{in}")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 7.62 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pico-analyzer:RP2xxx_Stamp_SMD"
		(layer "F.Cu")
		(at 115.57 76.962)
		(property "Reference" "U7"
			(at 12 13.4 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RP2040_Stamp"
			(at 0 14.15 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "pico-analyzer:RP2xxx_Stamp_SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "RP2xxx_Stamp*")
		(sheetname "Root")
		(sheetfile "pico-analyzer.kicad_sch")
		(attr through_hole)
		(fp_text user "G"
			(at 11.4 -11.2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "20"
			(at 11.2 11.4 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "0"
			(at -11.2 -11.2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "10"
			(at -11.4 11.2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -11.65 -9)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 29 "Net-(JP1-A)")
			(pinfunction "GPIO0")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -11.65 -7)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 30 "Net-(JP1-B)")
			(pinfunction "GPIO1")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -11.65 -5)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 2 "Net-(D1-DIN)")
			(pinfunction "GPIO2")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -11.65 -3)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 37 "/Level Translation/I0")
			(pinfunction "GPIO3")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -11.65 -1)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 36 "/Level Translation/I1")
			(pinfunction "GPIO4")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -11.65 1)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 33 "/Level Translation/I2")
			(pinfunction "GPIO5")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -11.65 3)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 35 "/Level Translation/I3")
			(pinfunction "GPIO6")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at -11.65 5)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 40 "/Level Translation/I4")
			(pinfunction "GPIO7")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at -11.65 7)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 41 "/Level Translation/I5")
			(pinfunction "GPIO8")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at -11.65 9)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 38 "/Level Translation/I6")
			(pinfunction "GPIO9")
			(pintype "bidirectional")
		)
		(pad "11" smd rect
			(at -9 11.65 270)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 43 "/Level Translation/I7")
			(pinfunction "GPIO10")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at -7 11.65 270)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 46 "/Level Translation/I8")
			(pinfunction "GPIO11")
			(pintype "bidirectional")
		)
		(pad "13" smd rect
			(at -5 11.65 270)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 44 "/Level Translation/I9")
			(pinfunction "GPIO12")
			(pintype "bidirectional")
		)
		(pad "14" smd rect
			(at -3 11.65 270)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 47 "/Level Translation/I10")
			(pinfunction "GPIO13")
			(pintype "bidirectional")
		)
		(pad "15" smd rect
			(at -1 11.65 270)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 48 "/Level Translation/I11")
			(pinfunction "GPIO14")
			(pintype "bidirectional")
		)
		(pad "16" smd rect
			(at 1 11.65 270)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 52 "/Level Translation/I12")
			(pinfunction "GPIO15")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at 3 11.65 270)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 51 "/Level Translation/I13")
			(pinfunction "GPIO16")
			(pintype "bidirectional")
		)
		(pad "18" smd rect
			(at 5 11.65 270)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 55 "/Level Translation/I14")
			(pinfunction "GPIO17")
			(pintype "bidirectional")
		)
		(pad "19" smd rect
			(at 7 11.65 270)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 50 "/Level Translation/I15")
			(pinfunction "GPIO18")
			(pintype "bidirectional")
		)
		(pad "20" smd rect
			(at 9 11.65 270)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 61 "/Level Translation/I16")
			(pinfunction "GPIO19")
			(pintype "bidirectional")
		)
		(pad "21" smd rect
			(at 11.65 9)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 60 "/Level Translation/I17")
			(pinfunction "GPIO20")
			(pintype "bidirectional")
		)
		(pad "22" smd rect
			(at 11.65 7)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 57 "/Level Translation/I18")
			(pinfunction "GPIO21")
			(pintype "bidirectional")
		)
		(pad "23" smd rect
			(at 11.65 5)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 56 "/Level Translation/I19")
			(pinfunction "GPIO22")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at 11.65 3)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 65 "/Level Translation/I20")
			(pinfunction "GPIO23")
			(pintype "bidirectional")
		)
		(pad "25" smd rect
			(at 11.65 1)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 64 "/Level Translation/I21")
			(pinfunction "GPIO24")
			(pintype "bidirectional")
		)
		(pad "26" smd rect
			(at 11.65 -1)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 63 "/Level Translation/I22")
			(pinfunction "GPIO25")
			(pintype "bidirectional")
		)
		(pad "27" smd rect
			(at 11.65 -3)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 66 "/Level Translation/I23")
			(pinfunction "GPIO26")
			(pintype "bidirectional")
		)
		(pad "28" smd rect
			(at 11.65 -5)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 68 "unconnected-(U7-GPIO27-Pad28)")
			(pinfunction "GPIO27")
			(pintype "bidirectional+no_connect")
		)
		(pad "29" smd rect
			(at 11.65 -7)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 71 "unconnected-(U7-GPIO28-Pad29)")
			(pinfunction "GPIO28")
			(pintype "bidirectional+no_connect")
		)
		(pad "30" smd rect
			(at 11.65 -9)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 76 "unconnected-(U7-GPIO29-Pad30)")
			(pinfunction "GPIO29")
			(pintype "bidirectional+no_connect")
		)
		(pad "31" smd rect
			(at 9 -11.65 270)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "32" smd rect
			(at 7 -11.65 270)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 75 "unconnected-(U7-VBAT-Pad32)")
			(pinfunction "VBAT")
			(pintype "power_in+no_connect")
		)
		(pad "33" smd rect
			(at 5 -11.65 270)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 1 "+5V")
			(pinfunction "5V")
			(pintype "power_in")
		)
		(pad "34" smd rect
			(at 3 -11.65 270)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 31 "+3V3")
			(pinfunction "3.3V")
			(pintype "power_out")
		)
		(pad "35" smd rect
			(at 1 -11.65 270)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 79 "Net-(U7-USB_D-)")
			(pinfunction "USB_D-")
			(pintype "bidirectional")
		)
		(pad "36" smd rect
			(at -1 -11.65 270)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 78 "Net-(U7-USB_D+)")
			(pinfunction "USB_D+")
			(pintype "bidirectional")
		)
		(pad "37" smd rect
			(at -3 -11.65 270)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 77 "unconnected-(U7-SWDIO-Pad37)")
			(pinfunction "SWDIO")
			(pintype "bidirectional+no_connect")
		)
		(pad "38" smd rect
			(at -5 -11.65 270)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 74 "unconnected-(U7-SWCLK-Pad38)")
			(pinfunction "SWCLK")
			(pintype "input+no_connect")
		)
		(pad "39" smd rect
			(at -7 -11.65 270)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 70 "unconnected-(U7-~{RESET}-Pad39)")
			(pinfunction "~{RESET}")
			(pintype "bidirectional+no_connect")
		)
		(pad "40" smd rect
			(at -9 -11.65 270)
			(size 2.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 69 "unconnected-(U7-BOOTSEL-Pad40)")
			(pinfunction "BOOTSEL")
			(pintype "input+no_connect")
		)
		(model "${KIPRJMOD}/3d-models/RP2040_Stamp.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kibuzzard-67632017"
		(layer "F.Cu")
		(at 139.2936 64.008 90)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDIuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIlZJTiIsICJQYWRkaW5nQm90dG9tQ3RybCI6IDIuMCwgIlBhZGRpbmdMZWZ0Q3RybCI6IDAuMCwgIlBhZGRpbmdSaWdodEN0cmwiOiAwLjAsICJQYWRkaW5nVG9wQ3RybCI6IDIuMCwgIldpZHRoQ3RybCI6IDAuMCwgImFkdmFuY2VkQ2hlY2tib3giOiBmYWxzZSwgImlubGluZUZvcm1hdFRleHRib3giOiBmYWxzZSwgImxpbmVvdmVyU3R5bGVDaG9pY2UiOiAiU3F1YXJlIiwgImxpbmVvdmVyVGhpY2tuZXNzQ3RybCI6IDF9")
		(property "Reference" "kibuzzard-67632017"
			(at 0 -4.586503 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 4.586503 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 87.109 99.822 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at -0.013 1.778 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_Small"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Translation")
		(sheetfile "pico-analyzer-translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kibuzzard-67632021"
		(layer "F.Cu")
		(at 131.2672 64.008 90)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDIuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjVWIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogMi4wLCAiUGFkZGluZ0xlZnRDdHJsIjogNC4wLCAiUGFkZGluZ1JpZ2h0Q3RybCI6IDEuNSwgIlBhZGRpbmdUb3BDdHJsIjogMi4wLCAiV2lkdGhDdHJsIjogMC4wLCAiYWR2YW5jZWRDaGVja2JveCI6IGZhbHNlLCAiaW5saW5lRm9ybWF0VGV4dGJveCI6IGZhbHNlLCAibGluZW92ZXJTdHlsZUNob2ljZSI6ICJTcXVhcmUiLCAibGluZW92ZXJUaGlja25lc3NDdHJsIjogMX0=")
		(property "Reference" "kibuzzard-67632021"
			(at 0 -4.607505 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 4.607505 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
		(layer "F.Cu")
		(at 91.47 102.362 90)
		(descr "TSSOP, 14 Pin (JEDEC MO-153 Var AB-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U1"
			(at 0 -3.45 90)
			(layer "F.SilkS")
		)
		(property "Value" "TXU0104PW"
			(at 0 3.45 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txu0104.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4-Bit Unidirectional Voltage-Level Translator, 1.1 - 5.5V A/BPort, TSSOP-14"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*14*5mm*P0.65mm*")
		(sheetname "Level Translation")
		(sheetfile "pico-analyzer-translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 82 "V_{ref}")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.8625 -1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "/Level Translation/C0")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.8625 -0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "/Level Translation/C1")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.8625 0 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "/Level Translation/C2")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.8625 0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "/Level Translation/C3")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.8625 1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "unconnected-(U1-NC-Pad6)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "7" smd roundrect
			(at -2.8625 1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at 2.8625 1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "+3V3")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at 2.8625 1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "unconnected-(U1-NC-Pad9)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "10" smd roundrect
			(at 2.8625 0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "/Level Translation/I3")
			(pinfunction "B4")
			(pintype "output")
		)
		(pad "11" smd roundrect
			(at 2.8625 0 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "/Level Translation/I2")
			(pinfunction "B3")
			(pintype "output")
		)
		(pad "12" smd roundrect
			(at 2.8625 -0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "/Level Translation/I1")
			(pinfunction "B2")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at 2.8625 -1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "/Level Translation/I0")
			(pinfunction "B1")
			(pintype "output")
		)
		(pad "14" smd roundrect
			(at 2.8625 -1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "+3V3")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2_DIN965"
		(layer "F.Cu")
		(at 149.86 63.5)
		(descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
		(tags "mounting hole 2.2mm no annular m2 din965")
		(property "Reference" "MH"
			(at 0 -2.9 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.2mm_M2_DIN965"
			(at 0 2.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_2.2mm_M2_DIN965"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 104.889 107.442 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_Small"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Translation")
		(sheetfile "pico-analyzer-translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 82 "V_{ref}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kibuzzard-67631580"
		(layer "F.Cu")
		(at 139.954 115.824)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjIyIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogMS4wLCAiUGFkZGluZ0xlZnRDdHJsIjogMC4wLCAiUGFkZGluZ1JpZ2h0Q3RybCI6IDAuMCwgIlBhZGRpbmdUb3BDdHJsIjogMS4wLCAiV2lkdGhDdHJsIjogMC4wLCAiYWR2YW5jZWRDaGVja2JveCI6IGZhbHNlLCAiaW5saW5lRm9ybWF0VGV4dGJveCI6IGZhbHNlLCAibGluZW92ZXJTdHlsZUNob2ljZSI6ICJTcXVhcmUiLCAibGluZW92ZXJUaGlja25lc3NDdHJsIjogMX0=")
		(property "Reference" "kibuzzard-67631580"
			(at 0 -3.693934 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.693934 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "kibuzzard-67631289"
		(layer "F.Cu")
		(at 124.714 117.602)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjE3IiwgIlBhZGRpbmdCb3R0b21DdHJsIjogMS4wLCAiUGFkZGluZ0xlZnRDdHJsIjogMC4wLCAiUGFkZGluZ1JpZ2h0Q3RybCI6IDAuMCwgIlBhZGRpbmdUb3BDdHJsIjogMS4wLCAiV2lkdGhDdHJsIjogMC4wLCAiYWR2YW5jZWRDaGVja2JveCI6IGZhbHNlLCAiaW5saW5lRm9ybWF0VGV4dGJveCI6IGZhbHNlLCAibGluZW92ZXJTdHlsZUNob2ljZSI6ICJTcXVhcmUiLCAibGluZW92ZXJUaGlja25lc3NDdHJsIjogMX0=")
		(property "Reference" "kibuzzard-67631289"
			(at 0 -3.682626 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.682626 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "kibuzzard-67631748"
		(layer "F.Cu")
		(at 103.378 115.824)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjYiLCAiUGFkZGluZ0JvdHRvbUN0cmwiOiAxLjAsICJQYWRkaW5nTGVmdEN0cmwiOiAyLjUsICJQYWRkaW5nUmlnaHRDdHJsIjogMi41LCAiUGFkZGluZ1RvcEN0cmwiOiAxLjAsICJXaWR0aEN0cmwiOiAwLjAsICJhZHZhbmNlZENoZWNrYm94IjogZmFsc2UsICJpbmxpbmVGb3JtYXRUZXh0Ym94IjogZmFsc2UsICJsaW5lb3ZlclN0eWxlQ2hvaWNlIjogIlNxdWFyZSIsICJsaW5lb3ZlclRoaWNrbmVzc0N0cmwiOiAxfQ==")
		(property "Reference" "kibuzzard-67631748"
			(at 0 -3.696358 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.696358 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "kibuzzard-676315DE"
		(layer "F.Cu")
		(at 112.903 115.824)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiWyIsICJDYXBSaWdodENob2ljZSI6ICJdIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIkdORCIsICJQYWRkaW5nQm90dG9tQ3RybCI6IDEuMCwgIlBhZGRpbmdMZWZ0Q3RybCI6IDMuMCwgIlBhZGRpbmdSaWdodEN0cmwiOiAzLjAsICJQYWRkaW5nVG9wQ3RybCI6IDEuMCwgIldpZHRoQ3RybCI6IDAuMCwgImFkdmFuY2VkQ2hlY2tib3giOiBmYWxzZSwgImlubGluZUZvcm1hdFRleHRib3giOiBmYWxzZSwgImxpbmVvdmVyU3R5bGVDaG9pY2UiOiAiU3F1YXJlIiwgImxpbmVvdmVyVGhpY2tuZXNzQ3RybCI6IDF9")
		(property "Reference" "kibuzzard-676315DE"
			(at 0 -3.704435 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.704435 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "pico-analyzer:PinHeader_2x04_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 119.37 120.396 -90)
		(descr "Through hole angled pin header, 2x04, 2.54mm pitch, 6mm pin length, double rows")
		(tags "Through hole angled pin header THT 2x04 2.54mm double row")
		(property "Reference" "J3"
			(at 1.27 2.56 90)
			(layer "F.SilkS")
		)
		(property "Value" "Channels 12-17"
			(at 5.655 2.27 90)
			(layer "F.Fab")
		)
		(property "Footprint" "pico-analyzer:PinHeader_2x04_P2.54mm_Horizontal"
			(at 0 -7.62 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 -7.62 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x04, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 -7.62 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "pico-analyzer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.31 -3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/Level Translation/C12")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/Level Translation/C13")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/Level Translation/C14")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/Level Translation/C15")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/Level Translation/C16")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/Level Translation/C17")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.54 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "V_{in}")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 7.62 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kibuzzard-676317E9"
		(layer "F.Cu")
		(at 91.186 115.824)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjIiLCAiUGFkZGluZ0JvdHRvbUN0cmwiOiAxLjAsICJQYWRkaW5nTGVmdEN0cmwiOiAyLjUsICJQYWRkaW5nUmlnaHRDdHJsIjogMi41LCAiUGFkZGluZ1RvcEN0cmwiOiAxLjAsICJXaWR0aEN0cmwiOiAwLjAsICJhZHZhbmNlZENoZWNrYm94IjogZmFsc2UsICJpbmxpbmVGb3JtYXRUZXh0Ym94IjogZmFsc2UsICJsaW5lb3ZlclN0eWxlQ2hvaWNlIjogIlNxdWFyZSIsICJsaW5lb3ZlclRoaWNrbmVzc0N0cmwiOiAxfQ==")
		(property "Reference" "kibuzzard-676317E9"
			(at 0 -3.693934 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.693934 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 135.369 104.902 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_Small"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Translation")
		(sheetfile "pico-analyzer-translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 82 "V_{ref}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 117.589 107.442 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_Small"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Translation")
		(sheetfile "pico-analyzer-translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 82 "V_{ref}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 92.075 62.103 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -1.651 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "pico-analyzer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kibuzzard-67631217"
		(layer "F.Cu")
		(at 124.714 115.824)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjE2IiwgIlBhZGRpbmdCb3R0b21DdHJsIjogMS4wLCAiUGFkZGluZ0xlZnRDdHJsIjogMC4wLCAiUGFkZGluZ1JpZ2h0Q3RybCI6IDAuMCwgIlBhZGRpbmdUb3BDdHJsIjogMS4wLCAiV2lkdGhDdHJsIjogMC4wLCAiYWR2YW5jZWRDaGVja2JveCI6IGZhbHNlLCAiaW5saW5lRm9ybWF0VGV4dGJveCI6IGZhbHNlLCAibGluZW92ZXJTdHlsZUNob2ljZSI6ICJTcXVhcmUiLCAibGluZW92ZXJUaGlja25lc3NDdHJsIjogMX0=")
		(property "Reference" "kibuzzard-67631217"
			(at 0 -3.696358 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.696358 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
		(layer "F.Cu")
		(at 139.73 102.362 90)
		(descr "TSSOP, 14 Pin (JEDEC MO-153 Var AB-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U6"
			(at 0 -3.45 90)
			(layer "F.SilkS")
		)
		(property "Value" "TXU0104PW"
			(at 0 3.45 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txu0104.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4-Bit Unidirectional Voltage-Level Translator, 1.1 - 5.5V A/BPort, TSSOP-14"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*14*5mm*P0.65mm*")
		(sheetname "Level Translation")
		(sheetfile "pico-analyzer-translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 82 "V_{ref}")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.8625 -1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 28 "/Level Translation/C20")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.8625 -0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "/Level Translation/C21")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.8625 0 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 26 "/Level Translation/C22")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.8625 0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/Level Translation/C23")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.8625 1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 67 "unconnected-(U6-NC-Pad6)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "7" smd roundrect
			(at -2.8625 1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at 2.8625 1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "+3V3")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at 2.8625 1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 62 "unconnected-(U6-NC-Pad9)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "10" smd roundrect
			(at 2.8625 0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 66 "/Level Translation/I23")
			(pinfunction "B4")
			(pintype "output")
		)
		(pad "11" smd roundrect
			(at 2.8625 0 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 63 "/Level Translation/I22")
			(pinfunction "B3")
			(pintype "output")
		)
		(pad "12" smd roundrect
			(at 2.8625 -0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "/Level Translation/I21")
			(pinfunction "B2")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at 2.8625 -1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "/Level Translation/I20")
			(pinfunction "B1")
			(pintype "output")
		)
		(pad "14" smd roundrect
			(at 2.8625 -1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "+3V3")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2_DIN965"
		(layer "F.Cu")
		(at 81.28 114.3)
		(descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
		(tags "mounting hole 2.2mm no annular m2 din965")
		(property "Reference" "MH"
			(at 0 -2.9 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.2mm_M2_DIN965"
			(at 0 2.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_2.2mm_M2_DIN965"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 117.589 102.362 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_Small"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Translation")
		(sheetfile "pico-analyzer-translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kibuzzard-67631801"
		(layer "F.Cu")
		(at 94.234 117.602)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjUiLCAiUGFkZGluZ0JvdHRvbUN0cmwiOiAxLjAsICJQYWRkaW5nTGVmdEN0cmwiOiAyLjUsICJQYWRkaW5nUmlnaHRDdHJsIjogMi41LCAiUGFkZGluZ1RvcEN0cmwiOiAxLjAsICJXaWR0aEN0cmwiOiAwLjAsICJhZHZhbmNlZENoZWNrYm94IjogZmFsc2UsICJpbmxpbmVGb3JtYXRUZXh0Ym94IjogZmFsc2UsICJsaW5lb3ZlclN0eWxlQ2hvaWNlIjogIlNxdWFyZSIsICJsaW5lb3ZlclRoaWNrbmVzc0N0cmwiOiAxfQ==")
		(property "Reference" "kibuzzard-67631801"
			(at 0 -3.693127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.693127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "kibuzzard-67631203"
		(layer "F.Cu")
		(at 118.618 115.824)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjEyIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogMS4wLCAiUGFkZGluZ0xlZnRDdHJsIjogMC4wLCAiUGFkZGluZ1JpZ2h0Q3RybCI6IDAuMCwgIlBhZGRpbmdUb3BDdHJsIjogMS4wLCAiV2lkdGhDdHJsIjogMC4wLCAiYWR2YW5jZWRDaGVja2JveCI6IGZhbHNlLCAiaW5saW5lRm9ybWF0VGV4dGJveCI6IGZhbHNlLCAibGluZW92ZXJTdHlsZUNob2ljZSI6ICJTcXVhcmUiLCAibGluZW92ZXJUaGlja25lc3NDdHJsIjogMX0=")
		(property "Reference" "kibuzzard-67631203"
			(at 0 -3.693934 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.693934 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "kibuzzard-6763175E"
		(layer "F.Cu")
		(at 106.426 115.824)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjgiLCAiUGFkZGluZ0JvdHRvbUN0cmwiOiAxLjAsICJQYWRkaW5nTGVmdEN0cmwiOiAyLjUsICJQYWRkaW5nUmlnaHRDdHJsIjogMi41LCAiUGFkZGluZ1RvcEN0cmwiOiAxLjAsICJXaWR0aEN0cmwiOiAwLjAsICJhZHZhbmNlZENoZWNrYm94IjogZmFsc2UsICJpbmxpbmVGb3JtYXRUZXh0Ym94IjogZmFsc2UsICJsaW5lb3ZlclN0eWxlQ2hvaWNlIjogIlNxdWFyZSIsICJsaW5lb3ZlclRoaWNrbmVzc0N0cmwiOiAxfQ==")
		(property "Reference" "kibuzzard-6763175E"
			(at 0 -3.705243 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.705243 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "pico-analyzer:EG2315A"
		(layer "F.Cu")
		(at 139.255 54.95 180)
		(descr "EG2315A")
		(tags "Switch")
		(property "Reference" "SW1"
			(at 12.128 -1.298 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_DP3T"
			(at 4 1.75 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "pico-analyzer:EG2315A"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Switch, three position, dual pole triple throw, 3 position switch, SP3T"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SW* DP3T*")
		(sheetname "Root")
		(sheetfile "pico-analyzer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 4 -1.171 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "V_{in}")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4 0 180)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "V_{ref}")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 6 0 180)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "+3V3")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 8 0 180)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 -2.5 180)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "V_{in}")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 4 -2.5 180)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "V_{ref}")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 6 -2.5 180)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "+3V3")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 8 -2.5 180)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "MH1" thru_hole circle
			(at -2.1 -1.25 180)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "MH2" thru_hole circle
			(at 10.1 -1.25 180)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(model "/home/rex/EG2315A/3D/EG2315A.stp"
			(offset
				(xyz 3.99999994 1.249999981 0.159999994)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "kibuzzard-676317ED"
		(layer "F.Cu")
		(at 91.186 117.602)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjMiLCAiUGFkZGluZ0JvdHRvbUN0cmwiOiAxLjAsICJQYWRkaW5nTGVmdEN0cmwiOiAyLjUsICJQYWRkaW5nUmlnaHRDdHJsIjogMi41LCAiUGFkZGluZ1RvcEN0cmwiOiAxLjAsICJXaWR0aEN0cmwiOiAwLjAsICJhZHZhbmNlZENoZWNrYm94IjogZmFsc2UsICJpbmxpbmVGb3JtYXRUZXh0Ym94IjogZmFsc2UsICJsaW5lb3ZlclN0eWxlQ2hvaWNlIjogIlNxdWFyZSIsICJsaW5lb3ZlclRoaWNrbmVzc0N0cmwiOiAxfQ==")
		(property "Reference" "kibuzzard-676317ED"
			(at 0 -3.704435 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.704435 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "kibuzzard-676317E0"
		(layer "F.Cu")
		(at 88.138 115.824)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjAiLCAiUGFkZGluZ0JvdHRvbUN0cmwiOiAxLjAsICJQYWRkaW5nTGVmdEN0cmwiOiAyLjUsICJQYWRkaW5nUmlnaHRDdHJsIjogMi41LCAiUGFkZGluZ1RvcEN0cmwiOiAxLjAsICJXaWR0aEN0cmwiOiAwLjAsICJhZHZhbmNlZENoZWNrYm94IjogZmFsc2UsICJpbmxpbmVGb3JtYXRUZXh0Ym94IjogZmFsc2UsICJsaW5lb3ZlclN0eWxlQ2hvaWNlIjogIlNxdWFyZSIsICJsaW5lb3ZlclRoaWNrbmVzc0N0cmwiOiAxfQ==")
		(property "Reference" "kibuzzard-676317E0"
			(at 0 -3.704435 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.704435 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 126.479 106.172 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_Small"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Translation")
		(sheetfile "pico-analyzer-translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 82 "V_{ref}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kibuzzard-6763170A"
		(layer "F.Cu")
		(at 109.474 117.602)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjExIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogMS4wLCAiUGFkZGluZ0xlZnRDdHJsIjogMC4wLCAiUGFkZGluZ1JpZ2h0Q3RybCI6IDAuMCwgIlBhZGRpbmdUb3BDdHJsIjogMS4wLCAiV2lkdGhDdHJsIjogMC4wLCAiYWR2YW5jZWRDaGVja2JveCI6IGZhbHNlLCAiaW5saW5lRm9ybWF0VGV4dGJveCI6IGZhbHNlLCAibGluZW92ZXJTdHlsZUNob2ljZSI6ICJTcXVhcmUiLCAibGluZW92ZXJUaGlja25lc3NDdHJsIjogMX0=")
		(property "Reference" "kibuzzard-6763170A"
			(at 0 -3.682626 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.682626 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "kibuzzard-67631617"
		(layer "F.Cu")
		(at 143.383 117.602)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiPiIsICJDYXBSaWdodENob2ljZSI6ICI8IiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIlZJTiIsICJQYWRkaW5nQm90dG9tQ3RybCI6IDEuMCwgIlBhZGRpbmdMZWZ0Q3RybCI6IDAuMCwgIlBhZGRpbmdSaWdodEN0cmwiOiAxLjAsICJQYWRkaW5nVG9wQ3RybCI6IDEuMCwgIldpZHRoQ3RybCI6IDAuMCwgImFkdmFuY2VkQ2hlY2tib3giOiBmYWxzZSwgImlubGluZUZvcm1hdFRleHRib3giOiBmYWxzZSwgImxpbmVvdmVyU3R5bGVDaG9pY2UiOiAiU3F1YXJlIiwgImxpbmVvdmVyVGhpY2tuZXNzQ3RybCI6IDF9")
		(property "Reference" "kibuzzard-67631617"
			(at 0 -3.682626 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.682626 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
		(layer "F.Cu")
		(at 130.81 103.632 90)
		(descr "TSSOP, 14 Pin (JEDEC MO-153 Var AB-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U5"
			(at 0 -3.45 90)
			(layer "F.SilkS")
		)
		(property "Value" "TXU0104PW"
			(at 0 3.45 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txu0104.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4-Bit Unidirectional Voltage-Level Translator, 1.1 - 5.5V A/BPort, TSSOP-14"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*14*5mm*P0.65mm*")
		(sheetname "Level Translation")
		(sheetfile "pico-analyzer-translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 82 "V_{ref}")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.8625 -1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "/Level Translation/C16")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.8625 -0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "/Level Translation/C17")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.8625 0 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "/Level Translation/C18")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.8625 0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "/Level Translation/C19")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.8625 1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 59 "unconnected-(U5-NC-Pad6)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "7" smd roundrect
			(at -2.8625 1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at 2.8625 1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "+3V3")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at 2.8625 1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 58 "unconnected-(U5-NC-Pad9)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "10" smd roundrect
			(at 2.8625 0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "/Level Translation/I19")
			(pinfunction "B4")
			(pintype "output")
		)
		(pad "11" smd roundrect
			(at 2.8625 0 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 57 "/Level Translation/I18")
			(pinfunction "B3")
			(pintype "output")
		)
		(pad "12" smd roundrect
			(at 2.8625 -0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 60 "/Level Translation/I17")
			(pinfunction "B2")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at 2.8625 -1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 61 "/Level Translation/I16")
			(pinfunction "B1")
			(pintype "output")
		)
		(pad "14" smd roundrect
			(at 2.8625 -1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "+3V3")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kibuzzard-67631703"
		(layer "F.Cu")
		(at 109.474 115.824)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjEwIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogMS4wLCAiUGFkZGluZ0xlZnRDdHJsIjogMC4wLCAiUGFkZGluZ1JpZ2h0Q3RybCI6IDAuMCwgIlBhZGRpbmdUb3BDdHJsIjogMS4wLCAiV2lkdGhDdHJsIjogMC4wLCAiYWR2YW5jZWRDaGVja2JveCI6IGZhbHNlLCAiaW5saW5lRm9ybWF0VGV4dGJveCI6IGZhbHNlLCAibGluZW92ZXJTdHlsZUNob2ljZSI6ICJTcXVhcmUiLCAibGluZW92ZXJUaGlja25lc3NDdHJsIjogMX0=")
		(property "Reference" "kibuzzard-67631703"
			(at 0 -3.704435 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.704435 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "kibuzzard-67631617"
		(layer "F.Cu")
		(at 128.143 117.602)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiPiIsICJDYXBSaWdodENob2ljZSI6ICI8IiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIlZJTiIsICJQYWRkaW5nQm90dG9tQ3RybCI6IDEuMCwgIlBhZGRpbmdMZWZ0Q3RybCI6IDAuMCwgIlBhZGRpbmdSaWdodEN0cmwiOiAxLjAsICJQYWRkaW5nVG9wQ3RybCI6IDEuMCwgIldpZHRoQ3RybCI6IDAuMCwgImFkdmFuY2VkQ2hlY2tib3giOiBmYWxzZSwgImlubGluZUZvcm1hdFRleHRib3giOiBmYWxzZSwgImxpbmVvdmVyU3R5bGVDaG9pY2UiOiAiU3F1YXJlIiwgImxpbmVvdmVyVGhpY2tuZXNzQ3RybCI6IDF9")
		(property "Reference" "kibuzzard-67631617"
			(at 0 -3.682626 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.682626 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
		(layer "F.Cu")
		(at 109.25 104.902 90)
		(descr "TSSOP, 14 Pin (JEDEC MO-153 Var AB-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U3"
			(at 0 -3.45 90)
			(layer "F.SilkS")
		)
		(property "Value" "TXU0104PW"
			(at 0 3.45 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txu0104.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4-Bit Unidirectional Voltage-Level Translator, 1.1 - 5.5V A/BPort, TSSOP-14"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*14*5mm*P0.65mm*")
		(sheetname "Level Translation")
		(sheetfile "pico-analyzer-translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 82 "V_{ref}")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.8625 -1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "/Level Translation/C8")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.8625 -0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "/Level Translation/C9")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.8625 0 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "/Level Translation/C10")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.8625 0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "/Level Translation/C11")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.8625 1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "unconnected-(U3-NC-Pad6)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "7" smd roundrect
			(at -2.8625 1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at 2.8625 1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "+3V3")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at 2.8625 1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 49 "unconnected-(U3-NC-Pad9)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "10" smd roundrect
			(at 2.8625 0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 48 "/Level Translation/I11")
			(pinfunction "B4")
			(pintype "output")
		)
		(pad "11" smd roundrect
			(at 2.8625 0 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "/Level Translation/I10")
			(pinfunction "B3")
			(pintype "output")
		)
		(pad "12" smd roundrect
			(at 2.8625 -0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "/Level Translation/I9")
			(pinfunction "B2")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at 2.8625 -1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "/Level Translation/I8")
			(pinfunction "B1")
			(pintype "output")
		)
		(pad "14" smd roundrect
			(at 2.8625 -1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "+3V3")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
		(layer "F.Cu")
		(at 100.33 103.632 90)
		(descr "TSSOP, 14 Pin (JEDEC MO-153 Var AB-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U2"
			(at 0 -3.45 90)
			(layer "F.SilkS")
		)
		(property "Value" "TXU0104PW"
			(at 0 3.45 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txu0104.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4-Bit Unidirectional Voltage-Level Translator, 1.1 - 5.5V A/BPort, TSSOP-14"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*14*5mm*P0.65mm*")
		(sheetname "Level Translation")
		(sheetfile "pico-analyzer-translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 82 "V_{ref}")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.8625 -1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "/Level Translation/C4")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.8625 -0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "/Level Translation/C5")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.8625 0 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "/Level Translation/C6")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.8625 0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "/Level Translation/C7")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.8625 1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "unconnected-(U2-NC-Pad6)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "7" smd roundrect
			(at -2.8625 1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at 2.8625 1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "+3V3")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at 2.8625 1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 42 "unconnected-(U2-NC-Pad9)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "10" smd roundrect
			(at 2.8625 0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "/Level Translation/I7")
			(pinfunction "B4")
			(pintype "output")
		)
		(pad "11" smd roundrect
			(at 2.8625 0 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/Level Translation/I6")
			(pinfunction "B3")
			(pintype "output")
		)
		(pad "12" smd roundrect
			(at 2.8625 -0.65 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "/Level Translation/I5")
			(pinfunction "B2")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at 2.8625 -1.3 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "/Level Translation/I4")
			(pinfunction "B1")
			(pintype "output")
		)
		(pad "14" smd roundrect
			(at 2.8625 -1.95 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "+3V3")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kibuzzard-676315DE"
		(layer "F.Cu")
		(at 97.663 115.824)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiWyIsICJDYXBSaWdodENob2ljZSI6ICJdIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIkdORCIsICJQYWRkaW5nQm90dG9tQ3RybCI6IDEuMCwgIlBhZGRpbmdMZWZ0Q3RybCI6IDMuMCwgIlBhZGRpbmdSaWdodEN0cmwiOiAzLjAsICJQYWRkaW5nVG9wQ3RybCI6IDEuMCwgIldpZHRoQ3RybCI6IDAuMCwgImFkdmFuY2VkQ2hlY2tib3giOiBmYWxzZSwgImlubGluZUZvcm1hdFRleHRib3giOiBmYWxzZSwgImxpbmVvdmVyU3R5bGVDaG9pY2UiOiAiU3F1YXJlIiwgImxpbmVvdmVyVGhpY2tuZXNzQ3RybCI6IDF9")
		(property "Reference" "kibuzzard-676315DE"
			(at 0 -3.704435 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.704435 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "kibuzzard-67631578"
		(layer "F.Cu")
		(at 136.906 117.602)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjIxIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogMS4wLCAiUGFkZGluZ0xlZnRDdHJsIjogMC4wLCAiUGFkZGluZ1JpZ2h0Q3RybCI6IDAuMCwgIlBhZGRpbmdUb3BDdHJsIjogMS4wLCAiV2lkdGhDdHJsIjogMC4wLCAiYWR2YW5jZWRDaGVja2JveCI6IGZhbHNlLCAiaW5saW5lRm9ybWF0VGV4dGJveCI6IGZhbHNlLCAibGluZW92ZXJTdHlsZUNob2ljZSI6ICJTcXVhcmUiLCAibGluZW92ZXJUaGlja25lc3NDdHJsIjogMX0=")
		(property "Reference" "kibuzzard-67631578"
			(at 0 -3.693934 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.693934 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 100.584 68.961 -90)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP1"
			(at 0 2.159 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SolderJumper_2_Bridged"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, closed/bridged"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged*")
		(sheetname "Root")
		(sheetfile "pico-analyzer.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom)
		(net_tie_pad_groups "1, 2")
		(pad "1" smd custom
			(at -0.65 0 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 29 "Net-(JP1-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 30 "Net-(JP1-B)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "kibuzzard-676315DE"
		(layer "F.Cu")
		(at 128.143 115.824)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiWyIsICJDYXBSaWdodENob2ljZSI6ICJdIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIkdORCIsICJQYWRkaW5nQm90dG9tQ3RybCI6IDEuMCwgIlBhZGRpbmdMZWZ0Q3RybCI6IDMuMCwgIlBhZGRpbmdSaWdodEN0cmwiOiAzLjAsICJQYWRkaW5nVG9wQ3RybCI6IDEuMCwgIldpZHRoQ3RybCI6IDAuMCwgImFkdmFuY2VkQ2hlY2tib3giOiBmYWxzZSwgImlubGluZUZvcm1hdFRleHRib3giOiBmYWxzZSwgImxpbmVvdmVyU3R5bGVDaG9pY2UiOiAiU3F1YXJlIiwgImxpbmVvdmVyVGhpY2tuZXNzQ3RybCI6IDF9")
		(property "Reference" "kibuzzard-676315DE"
			(at 0 -3.704435 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.704435 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "kibuzzard-67631617"
		(layer "F.Cu")
		(at 97.663 117.602)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiPiIsICJDYXBSaWdodENob2ljZSI6ICI8IiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIlZJTiIsICJQYWRkaW5nQm90dG9tQ3RybCI6IDEuMCwgIlBhZGRpbmdMZWZ0Q3RybCI6IDAuMCwgIlBhZGRpbmdSaWdodEN0cmwiOiAxLjAsICJQYWRkaW5nVG9wQ3RybCI6IDEuMCwgIldpZHRoQ3RybCI6IDAuMCwgImFkdmFuY2VkQ2hlY2tib3giOiBmYWxzZSwgImlubGluZUZvcm1hdFRleHRib3giOiBmYWxzZSwgImxpbmVvdmVyU3R5bGVDaG9pY2UiOiAiU3F1YXJlIiwgImxpbmVvdmVyVGhpY2tuZXNzQ3RybCI6IDF9")
		(property "Reference" "kibuzzard-67631617"
			(at 0 -3.682626 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.682626 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "kibuzzard-676317E5"
		(layer "F.Cu")
		(at 88.138 117.602)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIjEiLCAiUGFkZGluZ0JvdHRvbUN0cmwiOiAxLjAsICJQYWRkaW5nTGVmdEN0cmwiOiAyLjUsICJQYWRkaW5nUmlnaHRDdHJsIjogMi41LCAiUGFkZGluZ1RvcEN0cmwiOiAxLjAsICJXaWR0aEN0cmwiOiAwLjAsICJhZHZhbmNlZENoZWNrYm94IjogZmFsc2UsICJpbmxpbmVGb3JtYXRUZXh0Ym94IjogZmFsc2UsICJsaW5lb3ZlclN0eWxlQ2hvaWNlIjogIlNxdWFyZSIsICJsaW5lb3ZlclRoaWNrbmVzc0N0cmwiOiAxfQ==")
		(property "Reference" "kibuzzard-676317E5"
			(at 0 -3.682626 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.682626 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 95.999 106.172 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 -1.778 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_Small"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Level Translation")
		(sheetfile "pico-analyzer-translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 82 "V_{ref}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kibuzzard-67631617"
		(layer "F.Cu")
		(at 112.903 117.602)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiPiIsICJDYXBSaWdodENob2ljZSI6ICI8IiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6IDEuMCwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJMaW5lU3BhY2luZ0N0cmwiOiAxLjAsICJNdWx0aUxpbmVUZXh0IjogIlZJTiIsICJQYWRkaW5nQm90dG9tQ3RybCI6IDEuMCwgIlBhZGRpbmdMZWZ0Q3RybCI6IDAuMCwgIlBhZGRpbmdSaWdodEN0cmwiOiAxLjAsICJQYWRkaW5nVG9wQ3RybCI6IDEuMCwgIldpZHRoQ3RybCI6IDAuMCwgImFkdmFuY2VkQ2hlY2tib3giOiBmYWxzZSwgImlubGluZUZvcm1hdFRleHRib3giOiBmYWxzZSwgImxpbmVvdmVyU3R5bGVDaG9pY2UiOiAiU3F1YXJlIiwgImxpbmVvdmVyVGhpY2tuZXNzQ3RybCI6IDF9")
		(property "Reference" "kibuzzard-67631617"
			(at 0 -3.682626 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 3.682626 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(gr_arc
		(start 85.725 127)
		(mid 78.989808 124.210192)
		(end 76.2 117.475)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 76.2 60.325)
		(mid 78.989808 53.589808)
		(end 85.725 50.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145.415 127)
		(end 85.725 127)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 154.94 117.475)
		(mid 152.150192 124.210192)
		(end 145.415 127)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 85.725 50.8)
		(end 145.415 50.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 76.2 117.475)
		(end 76.2 60.325)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.94 60.325)
		(end 154.94 117.475)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 145.415 50.8)
		(mid 152.150192 53.589808)
		(end 154.94 60.325)
		(layer "Edge.Cuts")
	)
	(gr_text "pico-analyzer"
		(at 146.685 88.9 90)
		(layer "F.SilkS")
	)
	(gr_text "Place stamp\nhere.\nPost Office\nwill not\ndeliver mail\nwithout postage."
		(at 115.57 76.962 0)
		(layer "F.SilkS")
	)
	(gr_text "v1.0"
		(at 152.4 72.898 90)
		(layer "F.SilkS")
	)
	(gr_text "2024-12-18"
		(at 152.4 104.902 90)
		(layer "F.SilkS")
	)
	(dimension
		(type aligned)
		(layer "Eco1.User")
		(pts
			(xy 81.28 114.3) (xy 81.28 63.5)
		)
		(height -10.16)
		(gr_text "50.8 mm"
			(at 69.97 88.9 90)
			(layer "Eco1.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4) suppress_zeroes)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Eco1.User")
		(pts
			(xy 76.2 60.325) (xy 154.94 60.325)
		)
		(height -24.765)
		(gr_text "78.74 mm"
			(at 115.57 34.41 0)
			(layer "Eco1.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4) suppress_zeroes)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Eco1.User")
		(pts
			(xy 85.725 50.8) (xy 85.725 127)
		)
		(height 24.765)
		(gr_text "76.2 mm"
			(at 59.81 88.9 90)
			(layer "Eco1.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4) suppress_zeroes)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Eco1.User")
		(pts
			(xy 81.28 114.3) (xy 81.28 127)
		)
		(height 10.16)
		(gr_text "12.7 mm"
			(at 69.97 120.65 90)
			(layer "Eco1.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4) suppress_zeroes)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Eco1.User")
		(pts
			(xy 81.28 114.3) (xy 149.86 114.3)
		)
		(height 22.86)
		(gr_text "68.58 mm"
			(at 115.57 136.01 0)
			(layer "Eco1.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4) suppress_zeroes)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Eco1.User")
		(pts
			(xy 154.94 114.3) (xy 149.86 114.3)
		)
		(height -22.86)
		(gr_text "5.08 mm"
			(at 159.004 137.16 0)
			(layer "Eco1.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4) suppress_zeroes)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 2)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Eco2.User")
		(pts
			(xy 87.96 63.5) (xy 87.96 50.8)
		)
		(height -16.84)
		(gr_text "12.7 mm"
			(at 69.97 57.15 90)
			(layer "Eco2.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4) suppress_zeroes)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Eco2.User")
		(pts
			(xy 134.62 122.936) (xy 134.62 127)
		)
		(height 2.286)
		(gr_text "4.064 mm"
			(at 131.184 122.936 90)
			(layer "Eco2.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4) suppress_zeroes)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 2)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Eco2.User")
		(pts
			(xy 92.71 118.596) (xy 107.95 118.596)
		)
		(height 23.644)
		(gr_text "15.24 mm"
			(at 100.33 141.09 0)
			(layer "Eco2.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4) suppress_zeroes)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Eco2.User")
		(pts
			(xy 115.57 54.0512) (xy 154.94 54.0512)
		)
		(height -13.4112)
		(gr_text "39.37 mm"
			(at 135.255 39.49 0)
			(layer "Eco2.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4) suppress_zeroes)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Eco2.User")
		(pts
			(xy 87.96 63.5) (xy 76.2 63.5)
		)
		(height 17.78)
		(gr_text "11.76 mm"
			(at 82.08 44.57 0)
			(layer "Eco2.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4) suppress_zeroes)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Eco2.User")
		(pts
			(xy 92.71 118.469) (xy 76.2 118.469)
		)
		(height -23.771)
		(gr_text "16.51 mm"
			(at 84.455 141.09 0)
			(layer "Eco2.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4) suppress_zeroes)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Eco2.User")
		(pts
			(xy 138.43 121.666) (xy 138.43 127.036)
		)
		(height -21.59)
		(gr_text "5.37 mm"
			(at 160.02 117.602 90)
			(layer "Eco2.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4) suppress_zeroes)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 2)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Eco2.User")
		(pts
			(xy 135.255 52.8) (xy 154.94 52.8)
		)
		(height -7.08)
		(gr_text "19.685 mm"
			(at 145.0975 44.57 0)
			(layer "Eco2.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4) suppress_zeroes)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "User.3")
		(pts
			(xy 85.725 127) (xy 85.725 133.0198)
		)
		(height 14.605)
		(gr_text "6.02 mm"
			(at 71.12 136.906 90)
			(layer "User.3")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
			(override_value "6.02")
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 2)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "User.3")
		(pts
			(xy 71.12 50.8) (xy 71.12 49.1998)
		)
		(height 0)
		(gr_text "1.6 mm"
			(at 71.12 45.72 90)
			(layer "User.3")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
			(override_value "1.6")
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 2)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "User.3")
		(pts
			(xy 73.66 49.2) (xy 157.48 49.2)
		)
		(height -18.72)
		(gr_text "83.82 mm"
			(at 115.57 29.33 0)
			(layer "User.3")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4) suppress_zeroes)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "User.3")
		(pts
			(xy 74.6 49.2) (xy 74.6 133.02)
		)
		(height 18.72)
		(gr_text "83.82 mm"
			(at 54.73 91.11 90)
			(layer "User.3")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4) suppress_zeroes)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "User.3")
		(pts
			(xy 81.28 114.3) (xy 81.28 133.0198)
		)
		(height 15.24)
		(gr_text "18.72 mm"
			(at 64.89 121.158 90)
			(layer "User.3")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
			(override_value "18.72")
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 2)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "User.4")
		(pts
			(xy 87.96 63.5) (xy 73.66 63.5)
		)
		(height 22.86)
		(gr_text "14.3 mm"
			(at 80.81 39.49 0)
			(layer "User.4")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4) suppress_zeroes)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "User.4")
		(pts
			(xy 138.42 127.036) (xy 138.42 133.0198)
		)
		(height -21.6)
		(gr_text "6 mm"
			(at 158.87 130.0279 90)
			(layer "User.4")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
			(override_value "6")
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "User.4")
		(pts
			(xy 87.96 63.5) (xy 87.96 49.1998)
		)
		(height -21.92)
		(gr_text "14.3 mm"
			(at 64.89 56.3499 90)
			(layer "User.4")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
			(override_value "14.3")
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type radial)
		(layer "Eco1.User")
		(pts
			(xy 145.415 60.325) (xy 154.94 60.325)
		)
		(leader_length 4.96269)
		(gr_text "R 9.525 mm"
			(at 167.854347 68.276657 315)
			(layer "Eco1.User")
		)
		(format
			(prefix "R ")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4) suppress_zeroes)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_offset 0.5) keep_text_aligned)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 132.334 107.442) (xy 135.382 107.442) (xy 135.382 103.378) (xy 132.334 103.378)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 116.078 103.886) (xy 116.078 100.838) (xy 117.602 100.838) (xy 117.602 103.886)
			)
		)
	)
	(zone
		(net 1)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 8)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 1.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 118.364 60.325) (xy 118.364 59.69) (xy 116.967 59.69) (xy 116.967 60.325) (xy 116.967 61.595)
				(xy 119.761 61.595) (xy 119.761 66.929) (xy 121.412 66.929) (xy 121.412 60.325)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 92.964 104.14) (xy 96.012 104.14) (xy 96.012 107.696) (xy 92.964 107.696)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 107.569 57.658) (xy 109.982 57.658) (xy 109.982 60.198) (xy 107.569 60.198)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 103.378 103.886) (xy 103.378 105.41) (xy 104.902 105.41) (xy 104.902 103.886)
			)
		)
	)
	(zone
		(net 31)
		(net_name "+3V3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 87.122 98.298) (xy 89.916 98.298) (xy 89.916 100.584) (xy 87.122 100.584)
			)
		)
	)
	(zone
		(net 31)
		(net_name "+3V3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 126.492 99.568) (xy 129.286 99.568) (xy 129.286 101.854) (xy 126.492 101.854)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 103.378 103.886) (xy 103.378 100.838) (xy 104.902 100.838) (xy 104.902 103.886)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 116.078 108.966) (xy 116.078 105.918) (xy 117.602 105.918) (xy 117.602 108.966)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 141.224 104.14) (xy 143.002 104.14) (xy 143.002 106.172) (xy 141.224 106.172)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 123.444 108.712) (xy 126.492 108.712) (xy 126.492 104.648) (xy 123.444 104.648)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 1.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 120.65 60.833) (xy 121.412 60.833) (xy 121.412 63.373) (xy 123.825 63.373) (xy 123.825 66.675)
				(xy 125.349 66.675) (xy 125.349 60.198) (xy 120.65 60.198)
			)
		)
	)
	(zone
		(net 31)
		(net_name "+3V3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 117.602 100.838) (xy 120.396 100.838) (xy 120.396 103.124) (xy 117.602 103.124)
			)
		)
	)
	(zone
		(net 31)
		(net_name "+3V3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 96.012 99.568) (xy 98.806 99.568) (xy 98.806 101.854) (xy 96.012 101.854)
			)
		)
	)
	(zone
		(net 82)
		(net_name "V_{ref}")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 104.902 106.68) (xy 107.696 106.68) (xy 107.696 108.966) (xy 104.902 108.966)
			)
		)
	)
	(zone
		(net 1)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 8)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.6)
		)
		(polygon
			(pts
				(xy 116.967 58.801) (xy 117.602 58.166) (xy 117.602 56.9214) (xy 118.364 56.9214) (xy 118.364 60.325)
				(xy 116.967 60.325)
			)
		)
	)
	(zone
		(net 82)
		(net_name "V_{ref}")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 138.176 106.426) (xy 135.382 106.426) (xy 135.382 104.14) (xy 138.176 104.14)
			)
		)
	)
	(zone
		(net 82)
		(net_name "V_{ref}")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 129.286 107.696) (xy 126.492 107.696) (xy 126.492 105.41) (xy 129.286 105.41)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 133.858 101.346) (xy 133.858 98.298) (xy 135.382 98.298) (xy 135.382 101.346)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 85.598 101.346) (xy 85.598 98.298) (xy 87.122 98.298) (xy 87.122 101.346)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 85.598 101.346) (xy 85.598 103.378) (xy 87.122 103.378) (xy 87.122 101.346)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 124.968 102.616) (xy 124.968 104.648) (xy 126.492 104.648) (xy 126.492 102.616)
			)
		)
	)
	(zone
		(net 31)
		(net_name "+3V3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 104.902 100.838) (xy 107.696 100.838) (xy 107.696 103.124) (xy 104.902 103.124)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 124.968 102.616) (xy 124.968 99.568) (xy 126.492 99.568) (xy 126.492 102.616)
			)
		)
	)
	(zone
		(net 1)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 9)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 88.773 61.976) (xy 92.837 61.976) (xy 92.837 60.071) (xy 88.773 60.071)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 125.349 60.198) (xy 125.349 57.658) (xy 120.65 57.658) (xy 120.65 60.198)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 92.837 62.23) (xy 92.837 64.897) (xy 87.757 64.897) (xy 87.757 67.056) (xy 85.725 67.056) (xy 85.725 62.23)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 94.488 102.616) (xy 94.488 104.14) (xy 96.012 104.14) (xy 96.012 102.616)
			)
		)
	)
	(zone
		(net 82)
		(net_name "V_{ref}")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 96.012 105.41) (xy 98.806 105.41) (xy 98.806 107.696) (xy 96.012 107.696)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 85.598 106.426) (xy 85.598 103.378) (xy 87.122 103.378) (xy 87.122 106.426)
			)
		)
	)
	(zone
		(net 82)
		(net_name "V_{ref}")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 87.122 104.14) (xy 89.916 104.14) (xy 89.916 106.426) (xy 87.122 106.426)
			)
		)
	)
	(zone
		(net 1)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 8)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.6)
		)
		(polygon
			(pts
				(xy 112.776 56.9214) (xy 112.776 60.198) (xy 114.173 60.198) (xy 114.173 58.801) (xy 113.538 58.166)
				(xy 113.538 56.9214)
			)
		)
	)
	(zone
		(net 31)
		(net_name "+3V3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 135.382 98.298) (xy 138.176 98.298) (xy 138.176 100.584) (xy 135.382 100.584)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 116.078 103.886) (xy 116.078 105.918) (xy 117.602 105.918) (xy 117.602 103.886)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 133.858 101.346) (xy 133.858 103.378) (xy 135.382 103.378) (xy 135.382 101.346)
			)
		)
	)
	(zone
		(net 82)
		(net_name "V_{ref}")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 117.602 106.68) (xy 120.396 106.68) (xy 120.396 108.966) (xy 117.602 108.966)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 118.364 57.531) (xy 119.507 56.388) (xy 120.269 56.388) (xy 120.65 56.769) (xy 120.65 60.198)
				(xy 118.364 60.198)
			)
		)
	)
	(zone
		(net 31)
		(net_name "+3V3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 1.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 119.38 66.929) (xy 119.38 61.595) (xy 117.729 61.595) (xy 117.729 66.929)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 110.744 106.68) (xy 112.522 106.68) (xy 112.522 108.712) (xy 110.744 108.712)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 94.488 102.616) (xy 94.488 99.568) (xy 96.012 99.568) (xy 96.012 102.616)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 101.854 105.41) (xy 104.902 105.41) (xy 104.902 108.966) (xy 101.854 108.966)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 112.776 58.390366) (xy 112.776 60.198) (xy 109.982 60.198) (xy 109.982 57.658) (xy 110.49 57.658)
				(xy 111.7092 57.658) (xy 111.76 57.7596) (xy 112.776 57.7596)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GND")
		(layers "In1.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 76.2 50.8) (xy 154.94 50.8) (xy 154.94 127) (xy 76.2 127)
			)
		)
	)
	(zone
		(net 82)
		(net_name "V_{ref}")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 11)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 143.383 78.857237) (xy 134.3914 70.003969) (xy 134.3914 53.848) (xy 136.137264 53.848) (xy 136.106134 68.796134)
				(xy 145.161 77.851) (xy 145.161 109.093) (xy 137.541 109.093) (xy 137.541 107.315) (xy 143.383 107.315)
			)
		)
	)
	(zone
		(net 83)
		(net_name "V_{in}")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 15)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 125.984 121.92) (xy 125.984 124.206) (xy 128.016 124.206) (xy 128.016 121.92)
			)
		)
	)
	(zone
		(net 1)
		(net_name "+5V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 17)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 117.348 61.595) (xy 117.348 59.69) (xy 118.364 59.69) (xy 118.364 60.325) (xy 130.4544 60.325)
				(xy 130.4544 53.848) (xy 132.0546 53.848) (xy 132.0546 61.595) (xy 121.412 61.595) (xy 121.412 63.373)
				(xy 119.761 63.373) (xy 119.761 61.595) (xy 118.364 61.595)
			)
		)
	)
	(zone
		(net 1)
		(net_name "+5V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 13)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 1.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 112.776 59.69) (xy 112.776 60.579) (xy 92.583 60.579) (xy 92.583 60.071) (xy 88.773 60.071)
				(xy 88.773 61.976) (xy 92.583 61.976) (xy 92.583 61.595) (xy 114.173 61.595) (xy 114.173 59.69)
			)
		)
	)
	(zone
		(net 83)
		(net_name "V_{in}")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 14)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 95.504 124.206) (xy 143.256 124.206) (xy 143.256 125.984) (xy 95.504 125.984)
			)
		)
	)
	(zone
		(net 31)
		(net_name "+3V3")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 117.729 63.627) (xy 117.729 61.595) (xy 119.38 61.595) (xy 119.38 63.627) (xy 132.4356 63.627)
				(xy 132.4356 53.848) (xy 134.0612 53.848) (xy 134.0612 65.278) (xy 119.38 65.278) (xy 119.38 66.802)
				(xy 117.729 66.802) (xy 117.729 65.278)
			)
		)
	)
	(zone
		(net 83)
		(net_name "V_{in}")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 15)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 110.744 121.92) (xy 110.744 124.206) (xy 112.776 124.206) (xy 112.776 121.92)
			)
		)
	)
	(zone
		(net 82)
		(net_name "V_{ref}")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 87.122 105.283) (xy 87.122 106.426) (xy 87.122 108.458) (xy 87.122 109.093) (xy 137.541 109.093)
				(xy 137.541 105.283)
			)
		)
	)
	(zone
		(net 83)
		(net_name "V_{in}")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 15)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 141.224 121.92) (xy 141.224 124.206) (xy 143.256 124.206) (xy 143.256 121.92)
			)
		)
	)
	(zone
		(net 83)
		(net_name "V_{in}")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 15)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 95.504 121.92) (xy 95.504 124.206) (xy 97.536 124.206) (xy 97.536 121.92)
			)
		)
	)
	(zone
		(net 31)
		(net_name "+3V3")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 87.122 101.981) (xy 87.122 98.298) (xy 137.541 98.298) (xy 137.541 101.981)
			)
		)
	)
	(zone
		(net 1)
		(net_name "+5V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 12)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.25)
		)
		(polygon
			(pts
				(xy 112.776 58.547) (xy 118.364 58.547) (xy 118.364 61.595) (xy 112.776 61.595)
			)
		)
	)
	(zone
		(net 31)
		(net_name "+3V3")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 117.729 61.595) (xy 119.38 61.595) (xy 119.38 98.298) (xy 120.904 98.298) (xy 120.904 101.981)
				(xy 116.332 101.981) (xy 116.332 98.298) (xy 117.856 98.298)
			)
		)
	)
	(zone
		(net 83)
		(net_name "V_{in}")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 16)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 143.256 121.92) (xy 143.256 125.984) (xy 146.05 125.984) (xy 147.574 124.46) (xy 147.574 74.93)
				(xy 140.081 67.69538) (xy 140.081 53.848) (xy 138.43 53.848) (xy 138.43 68.450772) (xy 145.796 75.946)
				(xy 145.796 120.142) (xy 144.526 121.92)
			)
		)
	)
)
