(kicad_symbol_lib
	(version 20231120)
	(generator "kicad_symbol_editor")
	(generator_version "8.0")
	(symbol "EG2315A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "S"
			(at 21.59 12.7 0)
		)
		(property "Value" "EG2315A"
			(at 21.59 10.16 0)
		)
		(property "Footprint" "EG2315A"
			(at 21.59 -89.84 0)
		)
		(property "Datasheet" "https://configured-product-images.s3.amazonaws.com/2D/specs/EG2315A.pdf"
			(at 21.59 -189.84 0)
		)
		(property "Description" "SLIDE, 200mA, 30VDC DP3T, On-On-On Through Hole, Right Angle"
			(at 0 0 0)
		)
		(property "Height" "4.7"
			(at 21.59 -389.84 0)
		)
		(property "Manufacturer_Name" "E-Switch"
			(at 21.59 -489.84 0)
		)
		(property "Manufacturer_Part_Number" "EG2315A"
			(at 21.59 -589.84 0)
		)
		(property "Mouser Part Number" "612-EG2315A"
			(at 21.59 -689.84 0)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/E-Switch/EG2315A?qs=6C6BR4UgC3PKy3fn0Rxctg%3D%3D"
			(at 21.59 -789.84 0)
		)
		(property "Arrow Part Number" ""
			(at 21.59 -889.84 0)
		)
		(property "Arrow Price/Stock" ""
			(at 21.59 -989.84 0)
		)
		(symbol "EG2315A_1_1"
			(pin passive line
				(at 7.62 -12.7 90)
				(length 5.08)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 10.16 -12.7 90)
				(length 5.08)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 12.7 -12.7 90)
				(length 5.08)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at 15.24 -12.7 90)
				(length 5.08)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at 7.62 12.7 270)
				(length 5.08)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at 10.16 12.7 270)
				(length 5.08)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at 12.7 12.7 270)
				(length 5.08)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at 15.24 12.7 270)
				(length 5.08)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at 0 0 0)
				(length 5.08)
				(name "MH1")
				(number "MH1")
			)
			(pin passive line
				(at 25.4 0 180)
				(length 5.08)
				(name "MH2")
				(number "MH2")
			)
		)
	)
	(symbol "L99VR02J"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "L99VR02J"
			(at -7.62 -13.97 0)
		)
		(property "Footprint" "Package_SO:PowerSSO-16-1EP_3.9x4.9mm_P0.5mm_EP2.5x3.61mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Programmable 0.8V-5V LDO linear regulator, 500ma output, 2.15V-28V input"
			(at 0 0 0)
		)
		(symbol "L99VR02J_1_1"
			(pin power_in line
				(at -8.89 6.35 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -8.89 -2.54 0)
				(length 2.54)
				(name "Wi")
				(number "10")
			)
			(pin output line
				(at 8.89 -10.16 180)
				(length 2.54)
				(name "RST")
				(number "11")
			)
			(pin power_out line
				(at 8.89 6.35 180)
				(length 2.54)
				(name "VOUT")
				(number "12")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54) hide
				(name "PAD")
				(number "13")
			)
			(pin input line
				(at 8.89 0 180)
				(length 2.54)
				(name "SEL1")
				(number "2")
			)
			(pin input line
				(at 8.89 -2.54 180)
				(length 2.54)
				(name "SEL2")
				(number "3")
			)
			(pin input line
				(at 8.89 -5.08 180)
				(length 2.54)
				(name "SEL3")
				(number "4")
			)
			(pin output line
				(at -8.89 2.54 0)
				(length 2.54)
				(name "TW")
				(number "5")
			)
			(pin output line
				(at -8.89 -10.16 0)
				(length 2.54)
				(name "I_{short}")
				(number "6")
			)
			(pin input line
				(at -8.89 0 0)
				(length 2.54)
				(name "EN")
				(number "7")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at -8.89 -7.62 0)
				(length 2.54)
				(name "V_{CW}")
				(number "9")
			)
		)
	)
	(symbol "RP2040_Stamp"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 43.18 0)
		)
		(property "Value" "RP2040_Stamp"
			(at 0 -38.1 0)
		)
		(property "Footprint" "RP2040_Stamp:RP2040_Stamp_SMD"
			(at 0 -40.64 0)
		)
		(property "Datasheet" ""
			(at -33.02 41.91 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RP2xxx_Stamp*"
			(at 0 0 0)
		)
		(symbol "RP2040_Stamp_0_0"
			(text "IN"
				(at -4.445 39.37 0)
			)
			(text "OUT"
				(at -4.445 36.83 0)
			)
			(pin bidirectional line
				(at 12.7 39.37 180)
				(length 2.54)
				(name "GPIO0")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 16.51 180)
				(length 2.54)
				(name "GPIO9")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 13.97 180)
				(length 2.54)
				(name "GPIO10")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 11.43 180)
				(length 2.54)
				(name "GPIO11")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 8.89 180)
				(length 2.54)
				(name "GPIO12")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 6.35 180)
				(length 2.54)
				(name "GPIO13")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 3.81 180)
				(length 2.54)
				(name "GPIO14")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 1.27 180)
				(length 2.54)
				(name "GPIO15")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -1.27 180)
				(length 2.54)
				(name "GPIO16")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 -3.81 180)
				(length 2.54)
				(name "GPIO17")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 -6.35 180)
				(length 2.54)
				(name "GPIO18")
				(number "19")
			)
			(pin bidirectional line
				(at 12.7 36.83 180)
				(length 2.54)
				(name "GPIO1")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 -8.89 180)
				(length 2.54)
				(name "GPIO19")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 -11.43 180)
				(length 2.54)
				(name "GPIO20")
				(number "21")
			)
			(pin bidirectional line
				(at 12.7 -13.97 180)
				(length 2.54)
				(name "GPIO21")
				(number "22")
				(alternate "NEOPIXEL" output line)
			)
			(pin bidirectional line
				(at 12.7 -16.51 180)
				(length 2.54)
				(name "GPIO22")
				(number "23")
			)
			(pin bidirectional line
				(at 12.7 -19.05 180)
				(length 2.54)
				(name "GPIO23")
				(number "24")
			)
			(pin bidirectional line
				(at 12.7 -21.59 180)
				(length 2.54)
				(name "GPIO24")
				(number "25")
			)
			(pin bidirectional line
				(at 12.7 -24.13 180)
				(length 2.54)
				(name "GPIO25")
				(number "26")
			)
			(pin bidirectional line
				(at 12.7 -26.67 180)
				(length 2.54)
				(name "GPIO26")
				(number "27")
				(alternate "A0" input line)
			)
			(pin bidirectional line
				(at 12.7 -29.21 180)
				(length 2.54)
				(name "GPIO27")
				(number "28")
				(alternate "A1" input line)
			)
			(pin bidirectional line
				(at 12.7 -31.75 180)
				(length 2.54)
				(name "GPIO28")
				(number "29")
				(alternate "A2" input line)
			)
			(pin bidirectional line
				(at 12.7 34.29 180)
				(length 2.54)
				(name "GPIO2")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 -34.29 180)
				(length 2.54)
				(name "GPIO29")
				(number "30")
				(alternate "A3" input line)
			)
			(pin power_in line
				(at -12.7 -34.29 0)
				(length 2.54)
				(name "GND")
				(number "31")
			)
			(pin power_in line
				(at -12.7 34.29 0)
				(length 2.54)
				(name "VBAT")
				(number "32")
			)
			(pin power_in line
				(at -12.7 39.37 0)
				(length 2.54)
				(name "5V")
				(number "33")
			)
			(pin power_out line
				(at -12.7 36.83 0)
				(length 2.54)
				(name "3.3V")
				(number "34")
			)
			(pin bidirectional line
				(at -12.7 19.05 0)
				(length 2.54)
				(name "USB_D-")
				(number "35")
			)
			(pin bidirectional line
				(at -12.7 16.51 0)
				(length 2.54)
				(name "USB_D+")
				(number "36")
			)
			(pin bidirectional line
				(at -12.7 11.43 0)
				(length 2.54)
				(name "SWDIO")
				(number "37")
			)
			(pin input line
				(at -12.7 8.89 0)
				(length 2.54)
				(name "SWCLK")
				(number "38")
			)
			(pin bidirectional line
				(at -12.7 24.13 0)
				(length 2.54)
				(name "~{RESET}")
				(number "39")
			)
			(pin bidirectional line
				(at 12.7 31.75 180)
				(length 2.54)
				(name "GPIO3")
				(number "4")
			)
			(pin input line
				(at -12.7 29.21 0)
				(length 2.54)
				(name "BOOTSEL")
				(number "40")
			)
			(pin bidirectional line
				(at 12.7 29.21 180)
				(length 2.54)
				(name "GPIO4")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 26.67 180)
				(length 2.54)
				(name "GPIO5")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 24.13 180)
				(length 2.54)
				(name "GPIO6")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 21.59 180)
				(length 2.54)
				(name "GPIO7")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 19.05 180)
				(length 2.54)
				(name "GPIO8")
				(number "9")
			)
		)
		(symbol "RP2040_Stamp_0_1")
	)
	(symbol "SW_DP3T"
		(pin_names
			(offset 0) hide)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 5.08 0)
		)
		(property "Value" "SW_DP3T"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -15.875 4.445 0)
		)
		(property "Datasheet" "~"
			(at -15.875 4.445 0)
		)
		(property "Description" "Switch, three position, dual pole triple throw, 3 position switch, SP3T"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch dp3t ON-ON-ON"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW* DP3T*"
			(at 0 0 0)
		)
		(symbol "SW_DP3T_0_1")
		(symbol "SW_DP3T_1_1"
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "4")
				(number "4")
			)
		)
		(symbol "SW_DP3T_2_1"
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at 0 -6.35 90)
				(length 2.54)
				(name "SHIELD")
				(number "S1")
			)
		)
	)
	(symbol "TXU0104PW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "TXU0104PW"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txu0104.pdf"
			(at 2.794 2.413 0)
		)
		(property "Description" "4-Bit Unidirectional Voltage-Level Translator, 1.1 - 5.5V A/BPort, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*14*5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TXU0104PW_0_1")
		(symbol "TXU0104PW_1_1"
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VCCA")
				(number "1")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B4")
				(number "10")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B3")
				(number "11")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B2")
				(number "12")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "B1")
				(number "13")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VCCB")
				(number "14")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "4")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A4")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 -12.7 0)
				(length 2.54) hide
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin input line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "OE")
				(number "8")
			)
			(pin no_connect line
				(at 7.62 -12.7 180)
				(length 2.54) hide
				(name "NC")
				(number "9")
			)
		)
	)
	(symbol "Vin"
		(power)
		(pin_numbers hide)
		(pin_names
			(offset 0) hide)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -3.81 0)
		)
		(property "Value" "V_{in}"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Power symbol creates a global label with name \"Vin\""
			(at 0 0 0)
		)
		(property "ki_keywords" "global power"
			(at 0 0 0)
		)
		(symbol "Vin_0_1")
		(symbol "Vin_1_1"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(name "~")
				(number "1")
			)
		)
	)
	(symbol "Vref"
		(power)
		(pin_numbers hide)
		(pin_names
			(offset 0) hide)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -3.81 0)
		)
		(property "Value" "V_{ref}"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Power symbol creates a global label with name \"Vref\""
			(at 0 0 0)
		)
		(property "ki_keywords" "global power"
			(at 0 0 0)
		)
		(symbol "Vref_0_1")
		(symbol "Vref_1_1"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(name "~")
				(number "1")
			)
		)
	)
)
