(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (title_block
    (title "PICstick Programming Adapter")
    (date "2022-06-27")
    (rev "1.0")
    (comment 1 "USB programmer that supports PICs low-voltage ICSP protocol.")
    (comment 2 "Designed by Rex McKinnon  -  rexploits.com")
  )
  (lib_symbols
    (symbol "Connector:AVR-ISP-6" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at -6.35 11.43 0))
      (property "Value" "AVR-ISP-6" (id 1) (at 0 11.43 0))
      (property "Footprint" "" (id 2) (at -6.35 1.27 90))
      (property "Datasheet" " ~" (id 3) (at -32.385 -13.97 0))
      (property "ki_keywords" "AVR ISP Connector" (id 4) (at 0 0 0))
      (property "ki_description" "Atmel 6-pin ISP connector" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "IDC?Header*2x03* Pin?Header*2x03*" (id 6) (at 0 0 0))
      (symbol "AVR-ISP-6_0_1"
        (rectangle (start -2.667 -6.858) (end -2.413 -7.62)
          (fill (type none))
        )
        (rectangle (start -2.667 10.16) (end -2.413 9.398)
          (fill (type none))
        )
        (rectangle (start 7.62 -2.413) (end 6.858 -2.667)
          (fill (type none))
        )
        (rectangle (start 7.62 0.127) (end 6.858 -0.127)
          (fill (type none))
        )
        (rectangle (start 7.62 2.667) (end 6.858 2.413)
          (fill (type none))
        )
        (rectangle (start 7.62 5.207) (end 6.858 4.953)
          (fill (type none))
        )
        (rectangle (start 7.62 10.16) (end -7.62 -7.62)
          (fill (type background))
        )
      )
      (symbol "AVR-ISP-6_1_1"
        (pin passive line (at 10.16 5.08 180) (length 2.54)
          (name "MISO")
          (number "1")
        )
        (pin passive line (at -2.54 12.7 270) (length 2.54)
          (name "VCC")
          (number "2")
        )
        (pin passive line (at 10.16 0 180) (length 2.54)
          (name "SCK")
          (number "3")
        )
        (pin passive line (at 10.16 2.54 180) (length 2.54)
          (name "MOSI")
          (number "4")
        )
        (pin passive line (at 10.16 -2.54 180) (length 2.54)
          (name "~{RST}")
          (number "5")
        )
        (pin passive line (at -2.54 -10.16 90) (length 2.54)
          (name "GND")
          (number "6")
        )
      )
    )
    (symbol "Connector:Conn_01x03_Male" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 5.08 0))
      (property "Value" "Conn_01x03_Male" (id 1) (at 0 -5.08 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_01x03_Male_1_1"
        (polyline
          (pts
            (xy 1.27 -2.54)
            (xy 0.8636 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy 0.8636 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 2.54)
            (xy 0.8636 2.54)
          )
          (fill (type none))
        )
        (rectangle (start 0.8636 -2.413) (end 0 -2.667)
          (fill (type outline))
        )
        (rectangle (start 0.8636 0.127) (end 0 -0.127)
          (fill (type outline))
        )
        (rectangle (start 0.8636 2.667) (end 0 2.413)
          (fill (type outline))
        )
        (pin passive line (at 5.08 2.54 180) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 5.08 0 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at 5.08 -2.54 180) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
      )
    )
    (symbol "Connector:USB_A" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at -5.08 11.43 0))
      (property "Value" "USB_A" (id 1) (at -5.08 8.89 0))
      (property "Footprint" "" (id 2) (at 3.81 -1.27 0))
      (property "Datasheet" " ~" (id 3) (at 3.81 -1.27 0))
      (property "ki_keywords" "connector USB" (id 4) (at 0 0 0))
      (property "ki_description" "USB Type A connector" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "USB*" (id 6) (at 0 0 0))
      (symbol "USB_A_0_1"
        (rectangle (start -5.08 -7.62) (end 5.08 7.62)
          (fill (type background))
        )
        (circle (center -3.81 2.159) (radius 0.635)
          (fill (type outline))
        )
        (rectangle (start -1.524 4.826) (end -4.318 5.334)
          (fill (type outline))
        )
        (rectangle (start -1.27 4.572) (end -4.572 5.842)
          (fill (type none))
        )
        (circle (center -0.635 3.429) (radius 0.381)
          (fill (type outline))
        )
        (rectangle (start -0.127 -7.62) (end 0.127 -6.858)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.175 2.159)
            (xy -2.54 2.159)
            (xy -1.27 3.429)
            (xy -0.635 3.429)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 2.159)
            (xy -1.905 2.159)
            (xy -1.27 0.889)
            (xy 0 0.889)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 2.794)
            (xy 0.635 1.524)
            (xy 1.905 2.159)
            (xy 0.635 2.794)
          )
          (fill (type outline))
        )
        (rectangle (start 0.254 1.27) (end -0.508 0.508)
          (fill (type outline))
        )
        (rectangle (start 5.08 -2.667) (end 4.318 -2.413)
          (fill (type none))
        )
        (rectangle (start 5.08 -0.127) (end 4.318 0.127)
          (fill (type none))
        )
        (rectangle (start 5.08 4.953) (end 4.318 5.207)
          (fill (type none))
        )
      )
      (symbol "USB_A_1_1"
        (polyline
          (pts
            (xy -1.905 2.159)
            (xy 0.635 2.159)
          )
          (fill (type none))
        )
        (pin power_in line (at 7.62 5.08 180) (length 2.54)
          (name "VBUS")
          (number "1")
        )
        (pin bidirectional line (at 7.62 -2.54 180) (length 2.54)
          (name "D-")
          (number "2")
        )
        (pin bidirectional line (at 7.62 0 180) (length 2.54)
          (name "D+")
          (number "3")
        )
        (pin power_in line (at 0 -10.16 90) (length 2.54)
          (name "GND")
          (number "4")
        )
        (pin passive line (at -2.54 -10.16 90) (length 2.54)
          (name "Shield")
          (number "5")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:C_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.254 1.778 0))
      (property "Value" "C_Small" (id 1) (at 0.254 -2.032 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "capacitor cap" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_Small_0_1"
        (polyline
          (pts
            (xy -1.524 -0.508)
            (xy 1.524 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.524 0.508)
            (xy 1.524 0.508)
          )
          (fill (type none))
        )
      )
      (symbol "C_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 2.032)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 2.032)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:Crystal_GND24_Small" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Y" (id 0) (at 1.27 4.445 0))
      (property "Value" "Crystal_GND24_Small" (id 1) (at 1.27 2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "quartz ceramic resonator oscillator" (id 4) (at 0 0 0))
      (property "ki_description" "Four pin crystal, GND on pins 2 and 4, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Crystal*" (id 6) (at 0 0 0))
      (symbol "Crystal_GND24_Small_0_1"
        (rectangle (start -0.762 -1.524) (end 0.762 1.524)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -0.762)
            (xy -1.27 0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -0.762)
            (xy 1.27 0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 -1.905)
            (xy 1.27 -1.905)
            (xy 1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 1.27)
            (xy -1.27 1.905)
            (xy 1.27 1.905)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "Crystal_GND24_Small_1_1"
        (pin passive line (at -2.54 0 0) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 0.635)
          (name "2")
          (number "2")
        )
        (pin passive line (at 2.54 0 180) (length 1.27)
          (name "3")
          (number "3")
        )
        (pin passive line (at 0 2.54 270) (length 0.635)
          (name "4")
          (number "4")
        )
      )
    )
    (symbol "Device:LED" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "LED" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "LED diode" (id 4) (at 0 0 0))
      (property "ki_description" "Light emitting diode" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (id 6) (at 0 0 0))
      (symbol "LED_0_1"
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy -1.27 0)
            (xy 1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.048 -0.762)
            (xy -4.572 -2.286)
            (xy -3.81 -2.286)
            (xy -4.572 -2.286)
            (xy -4.572 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 -0.762)
            (xy -3.302 -2.286)
            (xy -2.54 -2.286)
            (xy -3.302 -2.286)
            (xy -3.302 -1.524)
          )
          (fill (type none))
        )
      )
      (symbol "LED_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:R_US" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.54 0 90))
      (property "Value" "R_US" (id 1) (at -2.54 0 90))
      (property "Footprint" "" (id 2) (at 1.016 -0.254 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor, US symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_US_0_1"
        (polyline
          (pts
            (xy 0 -2.286)
            (xy 0 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.286)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -0.762)
            (xy 1.016 -1.143)
            (xy 0 -1.524)
            (xy -1.016 -1.905)
            (xy 0 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0.762)
            (xy 1.016 0.381)
            (xy 0 0)
            (xy -1.016 -0.381)
            (xy 0 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.286)
            (xy 1.016 1.905)
            (xy 0 1.524)
            (xy -1.016 1.143)
            (xy 0 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "R_US_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Interface_USB:CH340E" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -5.08 13.97 0))
      (property "Value" "CH340E" (id 1) (at 1.27 13.97 0))
      (property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm" (id 2) (at 1.27 -13.97 0))
      (property "Datasheet" "https://www.mpja.com/download/35227cpdata.pdf" (id 3) (at -8.89 20.32 0))
      (property "ki_keywords" "USB UART Serial Converter Interface" (id 4) (at 0 0 0))
      (property "ki_description" "USB serial converter, UART, MSOP-10" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*" (id 6) (at 0 0 0))
      (symbol "CH340E_0_1"
        (rectangle (start -7.62 12.7) (end 7.62 -12.7)
          (fill (type background))
        )
      )
      (symbol "CH340E_1_1"
        (pin bidirectional line (at -10.16 2.54 0) (length 2.54)
          (name "UD+")
          (number "1")
        )
        (pin passive line (at -2.54 15.24 270) (length 2.54)
          (name "V3")
          (number "10")
        )
        (pin bidirectional line (at -10.16 0 0) (length 2.54)
          (name "UD-")
          (number "2")
        )
        (pin power_in line (at 0 -15.24 90) (length 2.54)
          (name "GND")
          (number "3")
        )
        (pin output line (at 10.16 -10.16 180) (length 2.54)
          (name "~{RTS}")
          (number "4")
        )
        (pin input line (at 10.16 2.54 180) (length 2.54)
          (name "~{CTS}")
          (number "5")
        )
        (pin output line (at -10.16 -2.54 0) (length 2.54)
          (name "TNOW")
          (number "6")
        )
        (pin power_in line (at 0 15.24 270) (length 2.54)
          (name "VCC")
          (number "7")
        )
        (pin output line (at 10.16 10.16 180) (length 2.54)
          (name "TXD")
          (number "8")
        )
        (pin input line (at 10.16 7.62 180) (length 2.54)
          (name "RXD")
          (number "9")
        )
      )
    )
    (symbol "MCU_Microchip_ATtiny:ATtiny44V-10M" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -12.7 21.59 0))
      (property "Value" "ATtiny44V-10M" (id 1) (at 2.54 -21.59 0))
      (property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm" (id 2) (at 0 0 0))
      (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "AVR 8bit Microcontroller tinyAVR" (id 4) (at 0 0 0))
      (property "ki_description" "10MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, QFN-20" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*" (id 6) (at 0 0 0))
      (symbol "ATtiny44V-10M_0_1"
        (rectangle (start -12.7 -20.32) (end 12.7 20.32)
          (fill (type background))
        )
      )
      (symbol "ATtiny44V-10M_1_1"
        (pin bidirectional line (at 15.24 5.08 180) (length 2.54)
          (name "PA4")
          (number "1")
        )
        (pin no_connect line (at -12.7 -10.16 0) (length 2.54) hide
          (name "NC")
          (number "10")
        )
        (pin bidirectional line (at 15.24 -7.62 180) (length 2.54)
          (name "XTAL1/PB0")
          (number "11")
        )
        (pin bidirectional line (at 15.24 -10.16 180) (length 2.54)
          (name "XTAL2/PB1")
          (number "12")
        )
        (pin bidirectional line (at 15.24 -15.24 180) (length 2.54)
          (name "~{RESET}/PB3")
          (number "13")
        )
        (pin bidirectional line (at 15.24 -12.7 180) (length 2.54)
          (name "PB2")
          (number "14")
        )
        (pin bidirectional line (at 15.24 -2.54 180) (length 2.54)
          (name "PA7")
          (number "15")
        )
        (pin bidirectional line (at 15.24 0 180) (length 2.54)
          (name "PA6")
          (number "16")
        )
        (pin no_connect line (at -12.7 -12.7 0) (length 2.54) hide
          (name "NC")
          (number "17")
        )
        (pin no_connect line (at -12.7 -15.24 0) (length 2.54) hide
          (name "NC")
          (number "18")
        )
        (pin no_connect line (at -12.7 -17.78 0) (length 2.54) hide
          (name "NC")
          (number "19")
        )
        (pin bidirectional line (at 15.24 7.62 180) (length 2.54)
          (name "PA3")
          (number "2")
        )
        (pin bidirectional line (at 15.24 2.54 180) (length 2.54)
          (name "PA5")
          (number "20")
        )
        (pin passive line (at 0 -22.86 90) (length 2.54) hide
          (name "GND")
          (number "21")
        )
        (pin bidirectional line (at 15.24 10.16 180) (length 2.54)
          (name "PA2")
          (number "3")
        )
        (pin bidirectional line (at 15.24 12.7 180) (length 2.54)
          (name "PA1")
          (number "4")
        )
        (pin bidirectional line (at 15.24 15.24 180) (length 2.54)
          (name "AREF/PA0")
          (number "5")
        )
        (pin no_connect line (at -12.7 -5.08 0) (length 2.54) hide
          (name "NC")
          (number "6")
        )
        (pin no_connect line (at -12.7 -7.62 0) (length 2.54) hide
          (name "NC")
          (number "7")
        )
        (pin power_in line (at 0 -22.86 90) (length 2.54)
          (name "GND")
          (number "8")
        )
        (pin power_in line (at 0 22.86 270) (length 2.54)
          (name "VCC")
          (number "9")
        )
      )
    )
    (symbol "Regulator_Linear:AP2112K-3.3" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -5.08 5.715 0))
      (property "Value" "AP2112K-3.3" (id 1) (at 0 5.715 0))
      (property "Footprint" "Package_TO_SOT_SMD:SOT-23-5" (id 2) (at 0 8.255 0))
      (property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2112.pdf" (id 3) (at 0 2.54 0))
      (property "ki_keywords" "linear regulator ldo fixed positive" (id 4) (at 0 0 0))
      (property "ki_description" "600mA low dropout linear regulator, with enable pin, 3.8V-6V input voltage range, 3.3V fixed positive output, SOT-23-5" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SOT?23?5*" (id 6) (at 0 0 0))
      (symbol "AP2112K-3.3_0_1"
        (rectangle (start -5.08 4.445) (end 5.08 -5.08)
          (fill (type background))
        )
      )
      (symbol "AP2112K-3.3_1_1"
        (pin power_in line (at -7.62 2.54 0) (length 2.54)
          (name "VIN")
          (number "1")
        )
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "GND")
          (number "2")
        )
        (pin input line (at -7.62 0 0) (length 2.54)
          (name "EN")
          (number "3")
        )
        (pin no_connect line (at 5.08 0 180) (length 2.54) hide
          (name "NC")
          (number "4")
        )
        (pin power_out line (at 7.62 2.54 180) (length 2.54)
          (name "VOUT")
          (number "5")
        )
      )
    )
    (symbol "power:+3V3" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+3V3" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+3V3\"" (id 5) (at 0 0 0))
      (symbol "+3V3_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+3V3_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+3V3")
          (number "1")
        )
      )
    )
    (symbol "power:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+5V" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (id 5) (at 0 0 0))
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 186.69 137.16) (diameter 0) (color 0 0 0 0))
  (junction (at 87.63 170.18) (diameter 0) (color 0 0 0 0))
  (junction (at 74.93 157.48) (diameter 0) (color 0 0 0 0))
  (junction (at 173.99 139.7) (diameter 0) (color 0 0 0 0))
  (junction (at 173.99 134.62) (diameter 0) (color 0 0 0 0))
  (junction (at 189.23 140.97) (diameter 0) (color 0 0 0 0))
  (junction (at 142.24 102.87) (diameter 0) (color 0 0 0 0))
  (junction (at 97.79 157.48) (diameter 0) (color 0 0 0 0))
  (junction (at 33.02 124.46) (diameter 0) (color 0 0 0 0))
  (junction (at 77.47 157.48) (diameter 0) (color 0 0 0 0))
  (junction (at 91.44 62.23) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 157.48 125.73) (xy 170.18 125.73)))
  (wire (pts (xy 74.93 157.48) (xy 77.47 157.48)))
  (wire (pts (xy 157.48 118.11) (xy 185.42 118.11)))
  (wire (pts (xy 88.9 62.23) (xy 91.44 62.23)))
  (wire (pts (xy 87.63 170.18) (xy 87.63 172.72)))
  (wire (pts (xy 97.79 167.64) (xy 97.79 170.18)))
  (wire (pts (xy 157.48 128.27) (xy 170.18 128.27)))
  (wire (pts (xy 101.6 90.17) (xy 104.14 90.17)))
  (wire (pts (xy 152.4 102.87) (xy 154.94 102.87)))
  (wire (pts (xy 91.44 59.69) (xy 91.44 62.23)))
  (wire (pts (xy 33.02 124.46) (xy 33.02 127)))
  (wire (pts (xy 87.63 170.18) (xy 97.79 170.18)))
  (wire (pts (xy 101.6 62.23) (xy 104.14 62.23)))
  (wire (pts (xy 101.6 72.39) (xy 104.14 72.39)))
  (wire (pts (xy 157.48 135.89) (xy 166.37 135.89)))
  (wire (pts (xy 97.79 157.48) (xy 97.79 160.02)))
  (wire (pts (xy 163.83 146.05) (xy 163.83 140.97)))
  (wire (pts (xy 157.48 130.81) (xy 170.18 130.81)))
  (wire (pts (xy 142.24 100.33) (xy 142.24 102.87)))
  (wire (pts (xy 243.84 146.05) (xy 241.3 146.05)))
  (wire (pts (xy 80.01 82.55) (xy 81.28 82.55)))
  (wire (pts (xy 142.24 105.41) (xy 142.24 102.87)))
  (wire (pts (xy 74.93 170.18) (xy 87.63 170.18)))
  (polyline (pts (xy 182.245 49.53) (xy 182.245 59.69)))
  (wire (pts (xy 160.02 143.51) (xy 160.02 147.32)))
  (wire (pts (xy 100.33 154.94) (xy 100.33 157.48)))
  (wire (pts (xy 157.48 143.51) (xy 160.02 143.51)))
  (wire (pts (xy 173.99 146.05) (xy 176.53 146.05)))
  (wire (pts (xy 228.6 156.21) (xy 228.6 153.67)))
  (wire (pts (xy 186.69 137.16) (xy 189.23 137.16)))
  (wire (pts (xy 166.37 134.62) (xy 173.99 134.62)))
  (wire (pts (xy 78.74 80.01) (xy 81.28 80.01)))
  (wire (pts (xy 91.44 62.23) (xy 93.98 62.23)))
  (polyline (pts (xy 162.56 59.69) (xy 205.74 59.69)))
  (wire (pts (xy 157.48 140.97) (xy 163.83 140.97)))
  (wire (pts (xy 191.77 140.97) (xy 189.23 140.97)))
  (polyline (pts (xy 194.31 73.66) (xy 264.16 73.66)))
  (wire (pts (xy 184.15 146.05) (xy 189.23 146.05)))
  (wire (pts (xy 186.69 139.7) (xy 186.69 137.16)))
  (wire (pts (xy 40.64 101.6) (xy 40.64 106.68)))
  (wire (pts (xy 72.39 157.48) (xy 74.93 157.48)))
  (wire (pts (xy 166.37 139.7) (xy 173.99 139.7)))
  (wire (pts (xy 101.6 77.47) (xy 104.14 77.47)))
  (wire (pts (xy 186.69 137.16) (xy 186.69 134.62)))
  (wire (pts (xy 157.48 120.65) (xy 185.42 120.65)))
  (wire (pts (xy 157.48 113.03) (xy 170.815 113.03)))
  (wire (pts (xy 243.84 143.51) (xy 241.3 143.51)))
  (wire (pts (xy 228.6 128.27) (xy 228.6 130.81)))
  (wire (pts (xy 173.99 139.7) (xy 179.07 139.7)))
  (wire (pts (xy 189.23 137.16) (xy 189.23 140.97)))
  (polyline (pts (xy 162.56 49.53) (xy 205.74 49.53)))
  (wire (pts (xy 74.93 167.64) (xy 74.93 170.18)))
  (wire (pts (xy 30.48 121.92) (xy 30.48 124.46)))
  (wire (pts (xy 97.79 157.48) (xy 100.33 157.48)))
  (polyline (pts (xy 162.56 54.61) (xy 205.74 54.61)))
  (wire (pts (xy 95.25 157.48) (xy 97.79 157.48)))
  (wire (pts (xy 80.01 160.02) (xy 77.47 160.02)))
  (wire (pts (xy 78.74 77.47) (xy 81.28 77.47)))
  (wire (pts (xy 72.39 154.94) (xy 72.39 157.48)))
  (wire (pts (xy 243.84 138.43) (xy 241.3 138.43)))
  (polyline (pts (xy 194.31 88.9) (xy 264.16 88.9)))
  (wire (pts (xy 77.47 160.02) (xy 77.47 157.48)))
  (wire (pts (xy 33.02 121.92) (xy 33.02 124.46)))
  (wire (pts (xy 74.93 160.02) (xy 74.93 157.48)))
  (wire (pts (xy 87.63 167.64) (xy 87.63 170.18)))
  (wire (pts (xy 157.48 138.43) (xy 166.37 138.43)))
  (wire (pts (xy 166.37 134.62) (xy 166.37 135.89)))
  (wire (pts (xy 40.64 111.76) (xy 48.26 111.76)))
  (wire (pts (xy 101.6 69.85) (xy 104.14 69.85)))
  (polyline (pts (xy 249.555 73.66) (xy 249.555 88.9)))
  (wire (pts (xy 157.48 123.19) (xy 170.18 123.19)))
  (wire (pts (xy 186.69 134.62) (xy 184.15 134.62)))
  (wire (pts (xy 184.15 139.7) (xy 186.69 139.7)))
  (wire (pts (xy 30.48 124.46) (xy 33.02 124.46)))
  (wire (pts (xy 243.84 140.97) (xy 241.3 140.97)))
  (wire (pts (xy 142.24 102.87) (xy 144.78 102.87)))
  (wire (pts (xy 80.01 157.48) (xy 77.47 157.48)))
  (wire (pts (xy 166.37 146.05) (xy 163.83 146.05)))
  (polyline (pts (xy 194.31 78.74) (xy 264.16 78.74)))
  (wire (pts (xy 189.23 140.97) (xy 189.23 146.05)))
  (wire (pts (xy 173.99 134.62) (xy 179.07 134.62)))
  (wire (pts (xy 91.44 95.25) (xy 91.44 97.79)))
  (wire (pts (xy 88.9 64.77) (xy 88.9 62.23)))
  (wire (pts (xy 40.64 114.3) (xy 48.26 114.3)))
  (polyline (pts (xy 194.31 83.82) (xy 264.16 83.82)))
  (wire (pts (xy 157.48 115.57) (xy 185.42 115.57)))
  (wire (pts (xy 91.44 62.23) (xy 91.44 64.77)))
  (wire (pts (xy 166.37 138.43) (xy 166.37 139.7)))
  (text "R1" (at 254 72.39 0))
  (text "150060BS75000" (at 229.87 87.63 180))
  (text "RH100-16.000-8-2020-TR" (at 162.56 58.42 180))
  (text "LED Selection" (at 224.79 66.04 0))
  (text "Blue" (at 241.3 87.63 180))
  (text "RH100-8.000-16-3030-TR-NS1" (at 162.56 53.34 180))
  (text "0Ω" (at 253.365 82.55 0))
  (text "B1931NB--20C006714U1930" (at 229.87 82.55 180))
  (text "*16MHz" (at 172.72 58.42 180))
  (text "*ATtiny44V doesn't officially\nsupport clock speeds over 8MHz"
    (at 163.83 66.04 0)
  )
  (text "60Ω" (at 253.365 77.47 0))
  (text "D1" (at 228.6 72.39 0))
  (text "Blue" (at 241.3 82.55 180))
  (text "8MHz" (at 172.72 53.34 180))
  (text "C4, C5" (at 190.5 48.26 0))
  (text "B1911NG--20D000114U1930" (at 229.87 77.47 180))
  (text "Crystal Selection\n" (at 167.64 41.91 0))
  (text "Y1" (at 167.64 48.26 0))
  (text "Yellow/Green" (at 246.38 77.47 180))
  (text "12pF" (at 193.04 58.42 0))
  (text "0-5Ω" (at 253.365 87.63 0))
  (text "28pF" (at 193.04 53.34 0))
  (label "~{MCLR}" (at 161.925 115.57 0))
  (label "DAT" (at 161.925 120.65 0))
  (label "CLK" (at 161.925 118.11 0))
  (label "MOSI" (at 161.925 128.27 0))
  (label "MISO" (at 161.925 125.73 0))
  (label "SCK" (at 161.925 123.19 0))
  (global_label "U1TX_U2RX" (shape input) (at 170.18 128.27 0) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 183.2974 128.1906 0))
  )
  (global_label "U1RX_U2TX" (shape input) (at 170.18 125.73 0) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 183.2974 125.6506 0))
  )
  (hierarchical_label "RTS" (shape input) (at 104.14 90.17 0))
  (hierarchical_label "CTS" (shape input) (at 170.815 113.03 0))
  (hierarchical_label "D+" (shape input) (at 48.26 111.76 0))
  (hierarchical_label "D-" (shape input) (at 78.74 80.01 180))
  (hierarchical_label "U1RX_U2TX" (shape input) (at 104.14 72.39 0))
  (hierarchical_label "SCK" (shape input) (at 243.84 143.51 0))
  (hierarchical_label "~{RESET}" (shape input) (at 243.84 146.05 0))
  (hierarchical_label "D+" (shape input) (at 78.74 77.47 180))
  (hierarchical_label "~{RESET}" (shape input) (at 160.02 147.32 270))
  (hierarchical_label "TNOW" (shape input) (at 80.01 82.55 180))
  (hierarchical_label "TNOW" (shape input) (at 170.18 130.81 0))
  (hierarchical_label "RTS" (shape input) (at 170.18 123.19 0))
  (hierarchical_label "U1TX_U2RX" (shape input) (at 104.14 69.85 0))
  (hierarchical_label "MISO" (shape input) (at 243.84 138.43 0))
  (hierarchical_label "CTS" (shape input) (at 104.14 77.47 0))
  (hierarchical_label "MOSI" (shape input) (at 243.84 140.97 0))
  (hierarchical_label "D-" (shape input) (at 48.26 114.3 0))
  (symbol (lib_id "Device:C") (at 97.79 163.83 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C2" (id 0) (at 101.6 162.5599 0))
    (property "Value" "1µF" (id 1) (at 101.6 165.0999 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 98.7552 167.64 0))
    (property "Datasheet" "~" (id 3) (at 97.79 163.83 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+3V3") (at 91.44 59.69 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0105" (id 0) (at 91.44 63.5 0))
    (property "Value" "+3V3" (id 1) (at 91.44 54.61 0))
    (property "Footprint" "" (id 2) (at 91.44 59.69 0))
    (property "Datasheet" "" (id 3) (at 91.44 59.69 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 91.44 97.79 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0106" (id 0) (at 91.44 104.14 0))
    (property "Value" "GND" (id 1) (at 91.44 102.87 0))
    (property "Footprint" "" (id 2) (at 91.44 97.79 0))
    (property "Datasheet" "" (id 3) (at 91.44 97.79 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C_Small") (at 181.61 134.62 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C5" (id 0) (at 185.42 133.35 90))
    (property "Value" "TBD" (id 1) (at 182.8862 132.08 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 181.61 134.62 0))
    (property "Datasheet" "~" (id 3) (at 181.61 134.62 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:Conn_01x03_Male") (at 190.5 118.11 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J3" (id 0) (at 191.77 118.1099 0))
    (property "Value" "ICSP" (id 1) (at 191.77 119.3799 0))
    (property "Footprint" "rexploits-kicad:PinHeader_1x03_P2.54mm_Horizontal" (id 2) (at 190.5 118.11 0))
    (property "Datasheet" "~" (id 3) (at 190.5 118.11 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Connector:AVR-ISP-6") (at 231.14 143.51 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J2" (id 0) (at 222.25 142.2399 0))
    (property "Value" "AVR-ISP" (id 1) (at 222.25 143.5099 0))
    (property "Footprint" "rexploits-kicad:PinHeader_2x03_P2.54mm_Vertical" (id 2) (at 224.79 142.24 90))
    (property "Datasheet" " ~" (id 3) (at 198.755 157.48 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
  )
  (symbol (lib_id "Device:Crystal_GND24_Small") (at 173.99 137.16 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Y1" (id 0) (at 173.99 133.35 90))
    (property "Value" "TBD" (id 1) (at 172.3898 124.46 0))
    (property "Footprint" "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm" (id 2) (at 173.99 137.16 0))
    (property "Datasheet" "~" (id 3) (at 173.99 137.16 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "Device:C") (at 97.79 62.23 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C3" (id 0) (at 97.79 54.61 90))
    (property "Value" "0.1µF" (id 1) (at 97.79 57.15 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 101.6 61.2648 0))
    (property "Datasheet" "~" (id 3) (at 97.79 62.23 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 148.59 102.87 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C4" (id 0) (at 148.59 95.25 90))
    (property "Value" "0.1µF" (id 1) (at 148.59 97.79 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 152.4 101.9048 0))
    (property "Datasheet" "~" (id 3) (at 148.59 102.87 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 228.6 156.21 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0116" (id 0) (at 228.6 162.56 0))
    (property "Value" "GND" (id 1) (at 228.6 161.29 0))
    (property "Footprint" "" (id 2) (at 228.6 156.21 0))
    (property "Datasheet" "" (id 3) (at 228.6 156.21 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3V3") (at 228.6 128.27 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR01" (id 0) (at 228.6 132.08 0))
    (property "Value" "+3V3" (id 1) (at 228.6 123.19 0))
    (property "Footprint" "" (id 2) (at 228.6 128.27 0))
    (property "Datasheet" "" (id 3) (at 228.6 128.27 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 191.77 140.97 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0114" (id 0) (at 198.12 140.97 0))
    (property "Value" "GND" (id 1) (at 195.58 140.97 90))
    (property "Footprint" "" (id 2) (at 191.77 140.97 0))
    (property "Datasheet" "" (id 3) (at 191.77 140.97 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 33.02 127 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0101" (id 0) (at 33.02 133.35 0))
    (property "Value" "GND" (id 1) (at 33.02 132.08 0))
    (property "Footprint" "" (id 2) (at 33.02 127 0))
    (property "Datasheet" "" (id 3) (at 33.02 127 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 104.14 62.23 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0107" (id 0) (at 110.49 62.23 0))
    (property "Value" "GND" (id 1) (at 107.95 62.2299 90))
    (property "Footprint" "" (id 2) (at 104.14 62.23 0))
    (property "Datasheet" "" (id 3) (at 104.14 62.23 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 87.63 172.72 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0104" (id 0) (at 87.63 179.07 0))
    (property "Value" "GND" (id 1) (at 87.63 177.8 0))
    (property "Footprint" "" (id 2) (at 87.63 172.72 0))
    (property "Datasheet" "" (id 3) (at 87.63 172.72 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 74.93 163.83 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C1" (id 0) (at 71.12 162.56 0))
    (property "Value" "1µF" (id 1) (at 71.12 165.1 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 75.8952 167.64 0))
    (property "Datasheet" "~" (id 3) (at 74.93 163.83 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Interface_USB:CH340E") (at 91.44 80.01 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U1" (id 0) (at 83.82 64.77 0))
    (property "Value" "CH340E" (id 1) (at 83.82 93.98 0))
    (property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm" (id 2) (at 92.71 93.98 0))
    (property "Datasheet" "https://www.mpja.com/download/35227cpdata.pdf" (id 3) (at 82.55 59.69 0))
    (pin "1")
    (pin "10")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Device:R_US") (at 170.18 146.05 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R1" (id 0) (at 170.18 143.51 90))
    (property "Value" "TBD" (id 1) (at 170.18 142.24 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 170.434 145.034 90))
    (property "Datasheet" "~" (id 3) (at 170.18 146.05 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 176.53 137.16 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0109" (id 0) (at 182.88 137.16 0))
    (property "Value" "GND" (id 1) (at 177.7999 134.62 0))
    (property "Footprint" "" (id 2) (at 176.53 137.16 0))
    (property "Datasheet" "" (id 3) (at 176.53 137.16 0))
    (pin "1")
  )
  (symbol (lib_id "Regulator_Linear:AP2112K-3.3") (at 87.63 160.02 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U3" (id 0) (at 82.55 153.67 0))
    (property "Value" "MCP1801T-3302I{slash}OT" (id 1) (at 87.63 152.4 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-5" (id 2) (at 87.63 151.765 0))
    (property "Datasheet" "" (id 3) (at 87.63 157.48 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Connector:USB_A") (at 33.02 111.76 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J1" (id 0) (at 33.02 99.06 0))
    (property "Value" "USB_A" (id 1) (at 33.02 101.6 0))
    (property "Footprint" "UPL:UP2-AH-1-TH" (id 2) (at 36.83 113.03 0))
    (property "Datasheet" " ~" (id 3) (at 36.83 113.03 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "power:+3V3") (at 100.33 154.94 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0108" (id 0) (at 100.33 158.75 0))
    (property "Value" "+3V3" (id 1) (at 100.33 149.86 0))
    (property "Footprint" "" (id 2) (at 100.33 154.94 0))
    (property "Datasheet" "" (id 3) (at 100.33 154.94 0))
    (pin "1")
  )
  (symbol (lib_id "MCU_Microchip_ATtiny:ATtiny44V-10M") (at 142.24 128.27 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U2" (id 0) (at 129.54 105.41 0))
    (property "Value" "ATtiny44V-10M" (id 1) (at 129.54 149.86 0))
    (property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm" (id 2) (at 142.24 128.27 0))
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf" (id 3) (at 142.24 128.27 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "power:+3V3") (at 142.24 100.33 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0111" (id 0) (at 142.24 104.14 0))
    (property "Value" "+3V3" (id 1) (at 142.24 95.25 0))
    (property "Footprint" "" (id 2) (at 142.24 100.33 0))
    (property "Datasheet" "" (id 3) (at 142.24 100.33 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C_Small") (at 181.61 139.7 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C6" (id 0) (at 185.42 138.43 90))
    (property "Value" "TBD" (id 1) (at 182.88 149.86 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 181.61 139.7 0))
    (property "Datasheet" "~" (id 3) (at 181.61 139.7 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:LED") (at 180.34 146.05 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D1" (id 0) (at 180.34 143.51 0))
    (property "Value" "STATUS" (id 1) (at 185.42 144.78 0))
    (property "Footprint" "LED_SMD:LED_0603_1608Metric" (id 2) (at 180.34 146.05 0))
    (property "Datasheet" "~" (id 3) (at 180.34 146.05 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 142.24 151.13 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0112" (id 0) (at 142.24 157.48 0))
    (property "Value" "GND" (id 1) (at 142.24 156.21 0))
    (property "Footprint" "" (id 2) (at 142.24 151.13 0))
    (property "Datasheet" "" (id 3) (at 142.24 151.13 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5V") (at 40.64 101.6 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0103" (id 0) (at 40.64 105.41 0))
    (property "Value" "+5V" (id 1) (at 40.64 96.52 0))
    (property "Footprint" "" (id 2) (at 40.64 101.6 0))
    (property "Datasheet" "" (id 3) (at 40.64 101.6 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5V") (at 72.39 154.94 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0102" (id 0) (at 72.39 158.75 0))
    (property "Value" "+5V" (id 1) (at 72.39 149.86 0))
    (property "Footprint" "" (id 2) (at 72.39 154.94 0))
    (property "Datasheet" "" (id 3) (at 72.39 154.94 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 171.45 137.16 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0113" (id 0) (at 165.1 137.16 0))
    (property "Value" "GND" (id 1) (at 170.1799 134.62 0))
    (property "Footprint" "" (id 2) (at 171.45 137.16 0))
    (property "Datasheet" "" (id 3) (at 171.45 137.16 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 154.94 102.87 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0110" (id 0) (at 161.29 102.87 0))
    (property "Value" "GND" (id 1) (at 158.75 102.8699 90))
    (property "Footprint" "" (id 2) (at 154.94 102.87 0))
    (property "Datasheet" "" (id 3) (at 154.94 102.87 0))
    (pin "1")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#PWR01") (unit 1) (value "+3V3") (footprint "")
    )
    (path
      (reference "#PWR0101") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0102") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR0103") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR0104") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0105") (unit 1) (value "+3V3") (footprint "")
    )
    (path
      (reference "#PWR0106") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0107") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0108") (unit 1) (value "+3V3") (footprint "")
    )
    (path
      (reference "#PWR0109") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0110") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0111") (unit 1) (value "+3V3") (footprint "")
    )
    (path
      (reference "#PWR0112") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0113") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0114") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0116") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "C1") (unit 1) (value "1µF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C2") (unit 1) (value "1µF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C3") (unit 1) (value "0.1µF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C4") (unit 1) (value "0.1µF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C5") (unit 1) (value "TBD") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C6") (unit 1) (value "TBD") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "D1") (unit 1) (value "STATUS") (footprint "LED_SMD:LED_0603_1608Metric")
    )
    (path
      (reference "J1") (unit 1) (value "USB_A") (footprint "UPL:UP2-AH-1-TH")
    )
    (path
      (reference "J2") (unit 1) (value "AVR-ISP") (footprint "rexploits-kicad:PinHeader_2x03_P2.54mm_Vertical")
    )
    (path
      (reference "J3") (unit 1) (value "ICSP") (footprint "rexploits-kicad:PinHeader_1x03_P2.54mm_Horizontal")
    )
    (path
      (reference "R1") (unit 1) (value "TBD") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "U1") (unit 1) (value "CH340E") (footprint "Package_SO:MSOP-10_3x3mm_P0.5mm")
    )
    (path
      (reference "U2") (unit 1) (value "ATtiny44V-10M") (footprint "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm")
    )
    (path
      (reference "U3") (unit 1) (value "MCP1801T-3302I{slash}OT") (footprint "Package_TO_SOT_SMD:SOT-23-5")
    )
    (path
      (reference "Y1") (unit 1) (value "TBD") (footprint "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm")
    )
  )
)
