(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 0.6)
		(legacy_teardrops no)
	)
	(paper "USLetter")
	(title_block
		(title "PowerPIC Calculator Watch")
		(date "2024-04-26")
		(rev "2.1")
		(comment 1 "Designed by Rex McKinnon <0xff@rexploits.com>")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 0.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(grid_origin 126.46 60.72)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue no)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerbers/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "VCC")
	(net 3 "/SEG22")
	(net 4 "/SEG25")
	(net 5 "/CFLY1")
	(net 6 "/CFLY2")
	(net 7 "/VLCD1")
	(net 8 "/VLCD2")
	(net 9 "/MODE")
	(net 10 "/ADJ")
	(net 11 "/~{MCLR}")
	(net 12 "/VLCD3")
	(net 13 "/BUZZ")
	(net 14 "/SOSCI")
	(net 15 "/SOSCO")
	(net 16 "Net-(D1-A)")
	(net 17 "/ROW3")
	(net 18 "/ROW2")
	(net 19 "/ROW1")
	(net 20 "/ROW0")
	(net 21 "/COL0")
	(net 22 "/COL1")
	(net 23 "/COL2")
	(net 24 "/COL3")
	(net 25 "/COM0")
	(net 26 "/COM1")
	(net 27 "/COM2")
	(net 28 "/COM3")
	(net 29 "/SEG0")
	(net 30 "/SEG1")
	(net 31 "/SEG2")
	(net 32 "/SEG3")
	(net 33 "/SEG4")
	(net 34 "/SEG5")
	(net 35 "/SEG6")
	(net 36 "/SEG7")
	(net 37 "/SEG8")
	(net 38 "/SEG9")
	(net 39 "/SEG10")
	(net 40 "/SEG11")
	(net 41 "/SEG12")
	(net 42 "/SEG13")
	(net 43 "/SEG14")
	(net 44 "/SEG15")
	(net 45 "/SEG16")
	(net 46 "/SEG17")
	(net 47 "/SEG18")
	(net 48 "/SEG19")
	(net 49 "/SEG20")
	(net 50 "/SEG21")
	(net 51 "/SEG23")
	(net 52 "/SEG24")
	(net 53 "/SEG26")
	(net 54 "/SEG27")
	(net 55 "/SEG28")
	(net 56 "/SEG29")
	(net 57 "/SEG30")
	(net 58 "unconnected-(U1-COM5{slash}RH1-Pad25)")
	(net 59 "unconnected-(U1-RA5-Pad27)")
	(net 60 "/DEBUG")
	(net 61 "/LIGHT")
	(net 62 "unconnected-(U1-RA4{slash}SEG14-Pad28)")
	(net 63 "unconnected-(U1-COM4{slash}RH0-Pad26)")
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 122.46 56.5 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 1.6 -0.06 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.27μF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "/VLCD3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "powerpic:ppc-board"
		(locked yes)
		(layer "F.Cu")
		(at 118.015 69.825)
		(descr "PCB Layout for the Casio CA53W")
		(property "Reference" "PPC1"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ppc-board"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ppc-watch:ppc-board"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_line
			(start 0 -25.1)
			(end 0 -2.5)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 2.5 0)
			(end 23.1 0)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 23.1 -27.6)
			(end 2.5 -27.6)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 25 -13.2)
			(end 25.6 -13.9)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 25 -2.5)
			(end 25 -13.2)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 25.6 -13.9)
			(end 25.6 -25.1)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 25.6 -2.5)
			(end 25 -2.5)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 0 -25.1)
			(mid 0.732233 -26.867767)
			(end 2.5 -27.6)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 2.5 0)
			(mid 0.732233 -0.732233)
			(end 0 -2.5)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 23.1 -27.6)
			(mid 24.867767 -26.867767)
			(end 25.6 -25.1)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 25.6 -2.5)
			(mid 24.867767 -0.732233)
			(end 23.1 0)
			(layer "Edge.Cuts")
		)
		(pad "" np_thru_hole circle
			(at 1.6 -13.8)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.3 -27.3)
			(size 1 1)
			(drill 1)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 20.3 -27.3)
			(size 1 1)
			(drill 1)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 23.9 -13.8)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" connect roundrect
			(at 12.9 -25.84)
			(size 8.3 2.75)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.1818181818)
			(net 2 "VCC")
			(pinfunction "VCC")
			(pintype "power_out")
		)
		(pad "2" connect roundrect
			(at 17.3 -16 17)
			(size 6 6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.08333333333)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "3" smd circle
			(at 2.15 -8.8)
			(size 2.2 2.2)
			(layers "B.Cu" "B.Mask")
			(net 13 "/BUZZ")
			(pinfunction "buzz_p")
			(pintype "input")
		)
		(pad "3" smd circle
			(at 6.65 -5.4)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask")
			(net 13 "/BUZZ")
			(pinfunction "buzz_p")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 25.2 -11)
			(size 1.2 2.7)
			(drill oval 0.8 2.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/MODE")
			(pinfunction "MODE")
			(pintype "output")
		)
		(pad "5" thru_hole oval
			(at 25.2 -3.8)
			(size 1.2 2.7)
			(drill oval 0.8 2.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/ADJ")
			(pinfunction "ADJ")
			(pintype "output")
		)
		(pad "6" connect rect
			(at 6.7 -2.6)
			(size 0.985 1.75)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "NC")
			(pintype "unspecified")
		)
		(pad "7" connect rect
			(at 8.2 -2.6)
			(size 0.985 1.75)
			(layers "F.Cu" "F.Mask")
			(net 17 "/ROW3")
			(pinfunction "ROW3")
			(pintype "bidirectional")
		)
		(pad "8" connect rect
			(at 9.7 -2.6)
			(size 0.985 1.75)
			(layers "F.Cu" "F.Mask")
			(net 18 "/ROW2")
			(pinfunction "ROW2")
			(pintype "bidirectional")
		)
		(pad "9" connect rect
			(at 11.2 -2.6)
			(size 0.985 1.75)
			(layers "F.Cu" "F.Mask")
			(net 19 "/ROW1")
			(pinfunction "ROW1")
			(pintype "bidirectional")
		)
		(pad "10" connect rect
			(at 12.7 -2.6)
			(size 0.985 1.75)
			(layers "F.Cu" "F.Mask")
			(net 20 "/ROW0")
			(pinfunction "ROW0")
			(pintype "bidirectional")
		)
		(pad "11" connect rect
			(at 14.2 -2.6)
			(size 0.985 1.75)
			(layers "F.Cu" "F.Mask")
			(net 21 "/COL0")
			(pinfunction "COL0")
			(pintype "bidirectional")
		)
		(pad "12" connect rect
			(at 15.7 -2.6)
			(size 0.985 1.75)
			(layers "F.Cu" "F.Mask")
			(net 22 "/COL1")
			(pinfunction "COL1")
			(pintype "bidirectional")
		)
		(pad "13" connect rect
			(at 17.2 -2.6)
			(size 0.985 1.75)
			(layers "F.Cu" "F.Mask")
			(net 23 "/COL2")
			(pinfunction "COL2")
			(pintype "bidirectional")
		)
		(pad "14" connect rect
			(at 18.7 -2.6)
			(size 0.985 1.75)
			(layers "F.Cu" "F.Mask")
			(net 24 "/COL3")
			(pinfunction "COL3")
			(pintype "bidirectional")
		)
		(pad "15" connect rect
			(at 2.6 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 25 "/COM0")
			(pinfunction "COM0")
			(pintype "input")
		)
		(pad "16" connect rect
			(at 3.2 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 26 "/COM1")
			(pinfunction "COM1")
			(pintype "input")
		)
		(pad "17" connect rect
			(at 3.8 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 27 "/COM2")
			(pinfunction "COM2")
			(pintype "input")
		)
		(pad "18" connect rect
			(at 4.4 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 28 "/COM3")
			(pinfunction "COM3")
			(pintype "input")
		)
		(pad "19" connect rect
			(at 5 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 29 "/SEG0")
			(pinfunction "SEG0")
			(pintype "input")
		)
		(pad "20" connect rect
			(at 5.6 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 30 "/SEG1")
			(pinfunction "SEG1")
			(pintype "input")
		)
		(pad "21" connect rect
			(at 6.2 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 31 "/SEG2")
			(pinfunction "SEG2")
			(pintype "input")
		)
		(pad "22" connect rect
			(at 6.8 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 32 "/SEG3")
			(pinfunction "SEG3")
			(pintype "input")
		)
		(pad "23" connect rect
			(at 7.4 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 33 "/SEG4")
			(pinfunction "SEG4")
			(pintype "input")
		)
		(pad "24" connect rect
			(at 8 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 34 "/SEG5")
			(pinfunction "SEG5")
			(pintype "input")
		)
		(pad "25" connect rect
			(at 8.6 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 35 "/SEG6")
			(pinfunction "SEG6")
			(pintype "input")
		)
		(pad "26" connect rect
			(at 9.2 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 36 "/SEG7")
			(pinfunction "SEG7")
			(pintype "input")
		)
		(pad "27" connect rect
			(at 9.8 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 37 "/SEG8")
			(pinfunction "SEG8")
			(pintype "input")
		)
		(pad "28" connect rect
			(at 10.4 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 38 "/SEG9")
			(pinfunction "SEG9")
			(pintype "input")
		)
		(pad "29" connect rect
			(at 11 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 39 "/SEG10")
			(pinfunction "SEG10")
			(pintype "input")
		)
		(pad "30" connect rect
			(at 11.6 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 40 "/SEG11")
			(pinfunction "SEG11")
			(pintype "input")
		)
		(pad "31" connect rect
			(at 12.2 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 41 "/SEG12")
			(pinfunction "SEG12")
			(pintype "input")
		)
		(pad "32" connect rect
			(at 12.8 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 42 "/SEG13")
			(pinfunction "SEG13")
			(pintype "input")
		)
		(pad "33" connect rect
			(at 13.4 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 43 "/SEG14")
			(pinfunction "SEG14")
			(pintype "input")
		)
		(pad "34" connect rect
			(at 14 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 44 "/SEG15")
			(pinfunction "SEG15")
			(pintype "input")
		)
		(pad "35" connect rect
			(at 14.6 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 45 "/SEG16")
			(pinfunction "SEG16")
			(pintype "input")
		)
		(pad "36" connect rect
			(at 15.2 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 46 "/SEG17")
			(pinfunction "SEG17")
			(pintype "input")
		)
		(pad "37" connect rect
			(at 15.8 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 47 "/SEG18")
			(pinfunction "SEG18")
			(pintype "input")
		)
		(pad "38" connect rect
			(at 16.4 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 48 "/SEG19")
			(pinfunction "SEG19")
			(pintype "input")
		)
		(pad "39" connect rect
			(at 17 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 49 "/SEG20")
			(pinfunction "SEG20")
			(pintype "input")
		)
		(pad "40" connect rect
			(at 17.6 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 50 "/SEG21")
			(pinfunction "SEG21")
			(pintype "input")
		)
		(pad "41" connect rect
			(at 18.2 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 3 "/SEG22")
			(pinfunction "SEG22")
			(pintype "input")
		)
		(pad "42" connect rect
			(at 18.8 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 51 "/SEG23")
			(pinfunction "SEG23")
			(pintype "input")
		)
		(pad "43" connect rect
			(at 19.4 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 52 "/SEG24")
			(pinfunction "SEG24")
			(pintype "input")
		)
		(pad "44" connect rect
			(at 20 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 4 "/SEG25")
			(pinfunction "SEG25")
			(pintype "input")
		)
		(pad "45" connect rect
			(at 20.6 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 53 "/SEG26")
			(pinfunction "SEG26")
			(pintype "input")
		)
		(pad "46" connect rect
			(at 21.2 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 54 "/SEG27")
			(pinfunction "SEG27")
			(pintype "input")
		)
		(pad "47" connect rect
			(at 21.8 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 55 "/SEG28")
			(pinfunction "SEG28")
			(pintype "input")
		)
		(pad "48" connect rect
			(at 22.4 -16.2)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 56 "/SEG29")
			(pinfunction "SEG29")
			(pintype "input")
		)
		(pad "49" connect rect
			(at 23 -16.2 180)
			(size 0.31 1.75)
			(layers "F.Cu" "F.Mask")
			(net 57 "/SEG30")
			(pinfunction "SEG30")
			(pintype "input")
		)
		(pad "50" smd custom
			(at 16.4 -2.15)
			(size 2 2)
			(layers "B.Cu" "B.Mask")
			(net 11 "/~{MCLR}")
			(pinfunction "~{MCLR}")
			(pintype "input")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_rect
					(start 0 -1)
					(end 1.2 1)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "50" smd circle
			(at 19.75 -5.8)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask")
			(net 11 "/~{MCLR}")
			(pinfunction "~{MCLR}")
			(pintype "input")
		)
		(pad "51" smd rect
			(at 18.94 -2.15)
			(size 2.2 2)
			(layers "B.Cu" "B.Mask")
			(net 9 "/MODE")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "52" smd custom
			(at 21.48 -2.15)
			(size 2 2)
			(layers "B.Cu" "B.Mask")
			(net 10 "/ADJ")
			(pinfunction "DAT")
			(pintype "input")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_rect
					(start -1.18 -1)
					(end 0.02 1)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "53" smd circle
			(at 22.25 -6.1)
			(size 2.2 2.2)
			(layers "B.Cu" "B.Mask")
			(net 60 "/DEBUG")
			(pinfunction "DBG")
			(pintype "input")
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 126.620589 60.880589 -45)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at -0.891788 -0.919239 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1μF"
			(at 0 1.16 135)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 315)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 315)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0402_1005Metric"
		(layer "F.Cu")
		(at 142.91 47.65 90)
		(descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at 1.28 -0.39 0)
			(layer "F.SilkS")
		)
		(property "Value" "LCD_LED"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 125.55 63.35 -45)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at -1.718269 -0.502046 0)
			(layer "F.SilkS")
		)
		(property "Value" "TBD"
			(at 0 1.43 135)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 315)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "Net-(D1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 315)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 61 "/LIGHT")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 140.44 60.81 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0.05 -1.28 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1μF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 122.42 60.5 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 1.56 -0.07 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.27μF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "/VLCD1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 121.105 63.69 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 2.165 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "TBD"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "/SOSCI")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 119.89 66.595 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 1.815 -0.95 180)
			(layer "F.SilkS")
		)
		(property "Value" "TBD"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "/SOSCO")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
		(layer "F.Cu")
		(at 133.29 60.09)
		(descr "QFN, 64 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/70593d.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "QFN NoLead")
		(property "Reference" "U1"
			(at -6.11 -2.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "PIC16LF1919x-I/MR"
			(at 0 5.8 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF19195-6-7-Data-Sheet-40001873D.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "8kW FLASH, 1kB RAM, 256B EEPROM, QFN-64"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -2.025 -2.025)
			(size 1.09 1.09)
			(layers "F.Paste")
			(roundrect_rratio 0.229358)
		)
		(pad "" smd roundrect
			(at -2.025 -0.675)
			(size 1.09 1.09)
			(layers "F.Paste")
			(roundrect_rratio 0.229358)
		)
		(pad "" smd roundrect
			(at -2.025 0.675)
			(size 1.09 1.09)
			(layers "F.Paste")
			(roundrect_rratio 0.229358)
		)
		(pad "" smd roundrect
			(at -2.025 2.025)
			(size 1.09 1.09)
			(layers "F.Paste")
			(roundrect_rratio 0.229358)
		)
		(pad "" smd roundrect
			(at -0.675 -2.025)
			(size 1.09 1.09)
			(layers "F.Paste")
			(roundrect_rratio 0.229358)
		)
		(pad "" smd roundrect
			(at -0.675 -0.675)
			(size 1.09 1.09)
			(layers "F.Paste")
			(roundrect_rratio 0.229358)
		)
		(pad "" smd roundrect
			(at -0.675 0.675)
			(size 1.09 1.09)
			(layers "F.Paste")
			(roundrect_rratio 0.229358)
		)
		(pad "" smd roundrect
			(at -0.675 2.025)
			(size 1.09 1.09)
			(layers "F.Paste")
			(roundrect_rratio 0.229358)
		)
		(pad "" smd roundrect
			(at 0.675 -2.025)
			(size 1.09 1.09)
			(layers "F.Paste")
			(roundrect_rratio 0.229358)
		)
		(pad "" smd roundrect
			(at 0.675 -0.675)
			(size 1.09 1.09)
			(layers "F.Paste")
			(roundrect_rratio 0.229358)
		)
		(pad "" smd roundrect
			(at 0.675 0.675)
			(size 1.09 1.09)
			(layers "F.Paste")
			(roundrect_rratio 0.229358)
		)
		(pad "" smd roundrect
			(at 0.675 2.025)
			(size 1.09 1.09)
			(layers "F.Paste")
			(roundrect_rratio 0.229358)
		)
		(pad "" smd roundrect
			(at 2.025 -2.025)
			(size 1.09 1.09)
			(layers "F.Paste")
			(roundrect_rratio 0.229358)
		)
		(pad "" smd roundrect
			(at 2.025 -0.675)
			(size 1.09 1.09)
			(layers "F.Paste")
			(roundrect_rratio 0.229358)
		)
		(pad "" smd roundrect
			(at 2.025 0.675)
			(size 1.09 1.09)
			(layers "F.Paste")
			(roundrect_rratio 0.229358)
		)
		(pad "" smd roundrect
			(at 2.025 2.025)
			(size 1.09 1.09)
			(layers "F.Paste")
			(roundrect_rratio 0.229358)
		)
		(pad "1" smd roundrect
			(at -4.4375 -3.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "/VLCD2")
			(pinfunction "VLCD2/RE1")
			(pintype "bidirectional")
		)
		(pad "2" smd roundrect
			(at -4.4375 -3.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "/VLCD1")
			(pinfunction "VLCD1/RE0")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -4.4375 -2.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "/SEG8")
			(pinfunction "SEG42/RG0")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -4.4375 -2.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "/SEG7")
			(pinfunction "SEG43/RG1")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -4.4375 -1.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "/SEG6")
			(pinfunction "SEG44/RG2")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -4.4375 -1.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "/SEG5")
			(pinfunction "SEG45/RG3")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -4.4375 -0.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "/~{MCLR}")
			(pinfunction "VPP/~{MCLR}/RG5")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -4.4375 -0.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "/SEG4")
			(pinfunction "SEG26/RG4")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -4.4375 0.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "10" smd roundrect
			(at -4.4375 0.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at -4.4375 1.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "/SEG3")
			(pinfunction "SEG25/RF7")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at -4.4375 1.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "/SEG2")
			(pinfunction "SEG24/RF6")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at -4.4375 2.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 30 "/SEG1")
			(pinfunction "SEG23/RF5")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at -4.4375 2.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "/SEG0")
			(pinfunction "SEG22/RF4")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at -4.4375 3.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "/SEG10")
			(pinfunction "SEG21/RF3")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at -4.4375 3.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "/SEG11")
			(pinfunction "SEG20/RF2")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at -3.75 4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/SEG9")
			(pinfunction "SEG19/RF1")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at -3.25 4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "/SEG12")
			(pinfunction "SEG41/RF0")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at -2.75 4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 61 "/LIGHT")
			(pinfunction "COM7/SEG15/RG7")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at -2.25 4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "/BUZZ")
			(pinfunction "COM6/RG6")
			(pintype "bidirectional")
		)
		(pad "21" smd roundrect
			(at -1.75 4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "/ROW3")
			(pinfunction "RA3/SEG35")
			(pintype "bidirectional")
		)
		(pad "22" smd roundrect
			(at -1.25 4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "/ROW2")
			(pinfunction "RA2/SEG34")
			(pintype "bidirectional")
		)
		(pad "23" smd roundrect
			(at -0.75 4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "/ROW1")
			(pinfunction "RA1/SEG18")
			(pintype "bidirectional")
		)
		(pad "24" smd roundrect
			(at -0.25 4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "/ROW0")
			(pinfunction "RA0/SEG33")
			(pintype "bidirectional")
		)
		(pad "25" smd roundrect
			(at 0.25 4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 58 "unconnected-(U1-COM5{slash}RH1-Pad25)")
			(pinfunction "COM5/RH1")
			(pintype "bidirectional+no_connect")
		)
		(pad "26" smd roundrect
			(at 0.75 4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 63 "unconnected-(U1-COM4{slash}RH0-Pad26)")
			(pinfunction "COM4/RH0")
			(pintype "bidirectional+no_connect")
		)
		(pad "27" smd roundrect
			(at 1.25 4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 59 "unconnected-(U1-RA5-Pad27)")
			(pinfunction "RA5")
			(pintype "bidirectional+no_connect")
		)
		(pad "28" smd roundrect
			(at 1.75 4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 62 "unconnected-(U1-RA4{slash}SEG14-Pad28)")
			(pinfunction "RA4/SEG14")
			(pintype "bidirectional+no_connect")
		)
		(pad "29" smd roundrect
			(at 2.25 4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "/SOSCI")
			(pinfunction "RC1")
			(pintype "bidirectional")
		)
		(pad "30" smd roundrect
			(at 2.75 4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "/SOSCO")
			(pinfunction "RC0")
			(pintype "bidirectional")
		)
		(pad "31" smd roundrect
			(at 3.25 4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "/COL0")
			(pinfunction "RC6/SEG27")
			(pintype "bidirectional")
		)
		(pad "32" smd roundrect
			(at 3.75 4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "/COL1")
			(pinfunction "RC7/SEG28")
			(pintype "bidirectional")
		)
		(pad "33" smd roundrect
			(at 4.4375 3.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/COL2")
			(pinfunction "RC2/SEG13")
			(pintype "bidirectional")
		)
		(pad "34" smd roundrect
			(at 4.4375 3.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "/COL3")
			(pinfunction "RC3/SEG17")
			(pintype "bidirectional")
		)
		(pad "35" smd roundrect
			(at 4.4375 2.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 60 "/DEBUG")
			(pinfunction "RC4/SEG16")
			(pintype "bidirectional")
		)
		(pad "36" smd roundrect
			(at 4.4375 2.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 57 "/SEG30")
			(pinfunction "RC5/SEG12")
			(pintype "bidirectional")
		)
		(pad "37" smd roundrect
			(at 4.4375 1.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "/ADJ")
			(pinfunction "RB7/SEG39/ICSPDAT")
			(pintype "bidirectional")
		)
		(pad "38" smd roundrect
			(at 4.4375 1.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "VCC")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "39" smd roundrect
			(at 4.4375 0.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 42 "/SEG13")
			(pinfunction "RA7/SEG37")
			(pintype "bidirectional")
		)
		(pad "40" smd roundrect
			(at 4.4375 0.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "/SEG14")
			(pinfunction "RA6/SEG36")
			(pintype "bidirectional")
		)
		(pad "41" smd roundrect
			(at 4.4375 -0.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "42" smd roundrect
			(at 4.4375 -0.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "/MODE")
			(pinfunction "RB6/SEG38/ICSPCLK")
			(pintype "bidirectional")
		)
		(pad "43" smd roundrect
			(at 4.4375 -1.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "/SEG29")
			(pinfunction "RB5/SEG29")
			(pintype "bidirectional")
		)
		(pad "44" smd roundrect
			(at 4.4375 -1.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 55 "/SEG28")
			(pinfunction "RB4/SEG11")
			(pintype "bidirectional")
		)
		(pad "45" smd roundrect
			(at 4.4375 -2.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 54 "/SEG27")
			(pinfunction "RB3/SEG10")
			(pintype "bidirectional")
		)
		(pad "46" smd roundrect
			(at 4.4375 -2.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 53 "/SEG26")
			(pinfunction "RB2/SEG9")
			(pintype "bidirectional")
		)
		(pad "47" smd roundrect
			(at 4.4375 -3.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/SEG25")
			(pinfunction "RB1/SEG8")
			(pintype "bidirectional")
		)
		(pad "48" smd roundrect
			(at 4.4375 -3.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 52 "/SEG24")
			(pinfunction "RB0/SEG30")
			(pintype "bidirectional")
		)
		(pad "49" smd roundrect
			(at 3.75 -4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 51 "/SEG23")
			(pinfunction "RD7/SEG7")
			(pintype "bidirectional")
		)
		(pad "50" smd roundrect
			(at 3.25 -4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "/SEG22")
			(pinfunction "RD6/SEG6")
			(pintype "bidirectional")
		)
		(pad "51" smd roundrect
			(at 2.75 -4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 50 "/SEG21")
			(pinfunction "RD5/SEG5")
			(pintype "bidirectional")
		)
		(pad "52" smd roundrect
			(at 2.25 -4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 49 "/SEG20")
			(pinfunction "RD4/SEG4")
			(pintype "bidirectional")
		)
		(pad "53" smd roundrect
			(at 1.75 -4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 48 "/SEG19")
			(pinfunction "RD3/SEG3")
			(pintype "bidirectional")
		)
		(pad "54" smd roundrect
			(at 1.25 -4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "/SEG18")
			(pinfunction "RD2/SEG2")
			(pintype "bidirectional")
		)
		(pad "55" smd roundrect
			(at 0.75 -4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "/SEG17")
			(pinfunction "RD1/SEG1")
			(pintype "bidirectional")
		)
		(pad "56" smd roundrect
			(at 0.25 -4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "/CFLY2")
			(pinfunction "CFLY2/SEG40/RH3")
			(pintype "bidirectional")
		)
		(pad "57" smd roundrect
			(at -0.25 -4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "/CFLY1")
			(pinfunction "CFLY1/SEG32/RH2")
			(pintype "bidirectional")
		)
		(pad "58" smd roundrect
			(at -0.75 -4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "/SEG16")
			(pinfunction "RD0/SEG0")
			(pintype "bidirectional")
		)
		(pad "59" smd roundrect
			(at -1.25 -4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "/SEG15")
			(pinfunction "SEG31/RE7")
			(pintype "bidirectional")
		)
		(pad "60" smd roundrect
			(at -1.75 -4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 28 "/COM3")
			(pinfunction "COM3/RE6")
			(pintype "bidirectional")
		)
		(pad "61" smd roundrect
			(at -2.25 -4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "/COM2")
			(pinfunction "COM2/RE5")
			(pintype "bidirectional")
		)
		(pad "62" smd roundrect
			(at -2.75 -4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 26 "/COM1")
			(pinfunction "COM1/RE4")
			(pintype "bidirectional")
		)
		(pad "63" smd roundrect
			(at -3.25 -4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "/COM0")
			(pinfunction "COM0/RE3")
			(pintype "bidirectional")
		)
		(pad "64" smd roundrect
			(at -3.75 -4.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "/VLCD3")
			(pinfunction "VLCD3")
			(pintype "input")
		)
		(pad "65" smd rect
			(at 0 0)
			(size 5.4 5.4)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(zone_connect 2)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 140.45 57.97 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at -0.06 1.28 180)
			(layer "F.SilkS")
		)
		(property "Value" "1μF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "/CFLY1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "/CFLY2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Crystal:Crystal_SMD_MicroCrystal_CC7V-T1A-2Pin_3.2x1.5mm"
		(layer "F.Cu")
		(at 121.87 66.47 -90)
		(descr "SMD Crystal MicroCrystal CC7V-T1A/CM7V-T1A series https://www.microcrystal.com/fileadmin/Media/Products/32kHz/Datasheet/CC7V-T1A.pdf, 3.2x1.5mm^2 package")
		(tags "SMD SMT crystal")
		(property "Reference" "Y1"
			(at -1.65 -2.03 0)
			(layer "F.SilkS")
		)
		(property "Value" "32.768kHz"
			(at 0 1.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Crystal:Crystal_SMD_MicroCrystal_CC7V-T1A-2Pin_3.2x1.5mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Two pin crystal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.25 0 270)
			(size 1 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "/SOSCI")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.25 0 270)
			(size 1 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "/SOSCO")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_MicroCrystal_CC7V-T1A-2Pin_3.2x1.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 122.42 58.5 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 1.56 -0.07 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.27μF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "/VLCD2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kibuzzard-6619F45C"
		(layer "B.Cu")
		(at 122.269 62.5996 143)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJGcmVkZHlTcGFyay1SZWd1bGFyIiwgIkhlaWdodEN0cmwiOiAiMSIsICJMYXllckNvbWJvQm94IjogIkYuU2lsa1MiLCAiTXVsdGlMaW5lVGV4dCI6ICJCVVoiLCAiUGFkZGluZ0JvdHRvbUN0cmwiOiAiMTAiLCAiUGFkZGluZ0xlZnRDdHJsIjogIjE1IiwgIlBhZGRpbmdSaWdodEN0cmwiOiAiMjIiLCAiUGFkZGluZ1RvcEN0cmwiOiAiMTAiLCAiV2lkdGhDdHJsIjogIiJ9")
		(property "Reference" "kibuzzard-6619F45C"
			(at 0 4.274608 143)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 -4.274608 143)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -37)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -37)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -37)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "kibuzzard-6619F682"
		(layer "B.Cu")
		(at 133.9022 49.7218 -163)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJGcmVkZHlTcGFyay1SZWd1bGFyIiwgIkhlaWdodEN0cmwiOiAiMS4yNSIsICJMYXllckNvbWJvQm94IjogIkYuU2lsa1MiLCAiTXVsdGlMaW5lVGV4dCI6ICJHTkQiLCAiUGFkZGluZ0JvdHRvbUN0cmwiOiAiMDUiLCAiUGFkZGluZ0xlZnRDdHJsIjogIjAiLCAiUGFkZGluZ1JpZ2h0Q3RybCI6ICIwIiwgIlBhZGRpbmdUb3BDdHJsIjogIjUiLCAiV2lkdGhDdHJsIjogIiJ9")
		(property "Reference" "kibuzzard-6619F682"
			(at 0 4.177771 -163)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 -4.177771 -163)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 17)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 17)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 17)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "kibuzzard-6619F3FA"
		(layer "B.Cu")
		(at 136.2136 64.022 180)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJGcmVkZHlTcGFyay1SZWd1bGFyIiwgIkhlaWdodEN0cmwiOiAiMSIsICJMYXllckNvbWJvQm94IjogIkYuU2lsa1MiLCAiTXVsdGlMaW5lVGV4dCI6ICJBQyIsICJQYWRkaW5nQm90dG9tQ3RybCI6ICI1IiwgIlBhZGRpbmdMZWZ0Q3RybCI6ICIxNSIsICJQYWRkaW5nUmlnaHRDdHJsIjogIjAiLCAiUGFkZGluZ1RvcEN0cmwiOiAiNSIsICJXaWR0aEN0cmwiOiAiIn0=")
		(property "Reference" "kibuzzard-6619F3FA"
			(at 0 3.95261 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 -3.95261 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "kibuzzard-6619F370"
		(layer "B.Cu")
		(at 140.2522 61.5582 90)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJGcmVkZHlTcGFyay1SZWd1bGFyIiwgIkhlaWdodEN0cmwiOiAiMSIsICJMYXllckNvbWJvQm94IjogIkYuU2lsa1MiLCAiTXVsdGlMaW5lVGV4dCI6ICJEQkciLCAiUGFkZGluZ0JvdHRvbUN0cmwiOiAiMTAiLCAiUGFkZGluZ0xlZnRDdHJsIjogIjIwIiwgIlBhZGRpbmdSaWdodEN0cmwiOiAiMCIsICJQYWRkaW5nVG9wQ3RybCI6ICIxMCIsICJXaWR0aEN0cmwiOiAiIn0=")
		(property "Reference" "kibuzzard-6619F370"
			(at 0 4.282546 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 -4.282546 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "kibuzzard-6619F6E4"
		(layer "B.Cu")
		(at 130.9558 46.6992 180)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJGcmVkZHlTcGFyay1SZWd1bGFyIiwgIkhlaWdodEN0cmwiOiAiMS4yNSIsICJMYXllckNvbWJvQm94IjogIkYuU2lsa1MiLCAiTXVsdGlMaW5lVGV4dCI6ICJWQ0MiLCAiUGFkZGluZ0JvdHRvbUN0cmwiOiAiMDUiLCAiUGFkZGluZ0xlZnRDdHJsIjogIjUiLCAiUGFkZGluZ1JpZ2h0Q3RybCI6ICI1IiwgIlBhZGRpbmdUb3BDdHJsIjogIjUiLCAiV2lkdGhDdHJsIjogIiJ9")
		(property "Reference" "kibuzzard-6619F6E4"
			(at 0 4.179755 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 -4.179755 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "kibuzzard-6619F1C8"
		(layer "B.Cu")
		(at 134.2324 67.6796 180)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiKCIsICJDYXBSaWdodENob2ljZSI6ICIpIiwgIkZvbnRDb21ib0JveCI6ICJGcmVkZHlTcGFyay1SZWd1bGFyIiwgIkhlaWdodEN0cmwiOiAiMS4yNSIsICJMYXllckNvbWJvQm94IjogIkYuU2lsa1MiLCAiTXVsdGlMaW5lVGV4dCI6ICJJQ1NQIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogIjUiLCAiUGFkZGluZ0xlZnRDdHJsIjogIjgwIiwgIlBhZGRpbmdSaWdodEN0cmwiOiAiMCIsICJQYWRkaW5nVG9wQ3RybCI6ICI1IiwgIldpZHRoQ3RybCI6ICIifQ==")
		(property "Reference" "kibuzzard-6619F1C8"
			(at 0 4.176779 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 -4.176779 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(gr_text "v2.1"
		(at 131.73 60.23 0)
		(layer "B.SilkS")
	)
	(gr_text "R"
		(at 134.6134 66.0032 0)
		(layer "B.SilkS")
	)
	(gr_text "D"
		(at 139.033 66.0032 0)
		(layer "B.SilkS")
	)
	(gr_text "REXCM"
		(at 142.3604 45.0736 0)
		(layer "B.SilkS")
	)
	(gr_text "C"
		(at 136.9248 66.0032 0)
		(layer "B.SilkS")
	)
	(gr_text "2416"
		(at 120.1862 45.2768 0)
		(layer "B.SilkS")
	)
	(gr_text "PowerPIC"
		(at 134.1 58.72 0)
		(layer "B.SilkS")
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(pts
			(xy 118.015 44.725) (xy 143.615 44.725)
		)
		(height -6.865)
		(gr_text "25.6000 mm"
			(at 130.815 36.71 0)
			(layer "Cmts.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(pts
			(xy 120.515 69.825) (xy 120.515 42.225)
		)
		(height -6.755)
		(gr_text "27.6000 mm"
			(at 112.61 56.025 90)
			(layer "Cmts.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 2)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.2 68.25) (xy 125.21 68.25) (xy 125.21 66.2) (xy 137.2 66.2)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 2)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.79 54.65) (xy 119.84 54.65) (xy 119.84 52.6) (xy 141.79 52.6)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 2)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125.57 64.26) (xy 124.681077 63.371385) (xy 125.47 63.67)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.508)
		(priority 100)
		(connect_pads
			(clearance 0.1524)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.1524)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 143.71 69.72) (xy 118.01 69.72) (xy 118.02 41.65) (xy 143.72 41.65)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 2)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.31 47.49) (xy 143.22 47.49) (xy 143.14 47.08) (xy 142.74 46.25) (xy 142.04 45.73) (xy 141.26 45.55)
				(xy 141.26 45.23) (xy 143.31 45.23)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 150)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.1524)
			(thermal_bridge_width 0.508)
			(island_removal_mode 2)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.58 59.01) (xy 131.89 59.01) (xy 130.89 49.27) (xy 139.58 49.27)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 2)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 120.37 45.52) (xy 119.96 45.59) (xy 119.54 45.73) (xy 119.19 45.93) (xy 118.83 46.28) (xy 118.53 46.85)
				(xy 118.43 47.49) (xy 117.9 47.49) (xy 117.9 45.43) (xy 120.37 45.43)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 2)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144 45.52) (xy 117.9 45.52) (xy 117.9 41.88) (xy 144 41.88)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.SilkS")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 2)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.64 66.93) (xy 133.64 67.14) (xy 133.55 67.14) (xy 133.53 67.02) (xy 133.63 66.92)
			)
		)
	)
)