(kicad_pcb (version 20220331) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4" portrait)
  (title_block
    (title "PowerPIC Calculator Watch")
    (date "2022-05-02")
    (rev "2.0")
    (comment 1 "Designed by Rex McKinnon <0xff@rexploits.com>")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 126.46 60.72)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "VCC")
  (net 3 "/SEG22")
  (net 4 "/SEG25")
  (net 5 "/CFLY1")
  (net 6 "/CFLY2")
  (net 7 "/VLCD1")
  (net 8 "/VLCD2")
  (net 9 "/MODE")
  (net 10 "/ADJ")
  (net 11 "/~{MCLR}")
  (net 12 "/VLCD3")
  (net 13 "unconnected-(U1-RA5)")
  (net 14 "/BUZZ")
  (net 15 "/SOSCI")
  (net 16 "/SOSCO")
  (net 17 "Net-(D1-A)")
  (net 18 "/ROW3")
  (net 19 "/ROW2")
  (net 20 "/ROW1")
  (net 21 "/ROW0")
  (net 22 "/COL0")
  (net 23 "/COL1")
  (net 24 "/COL2")
  (net 25 "/COL3")
  (net 26 "/COM0")
  (net 27 "/COM1")
  (net 28 "/COM2")
  (net 29 "/COM3")
  (net 30 "/SEG0")
  (net 31 "/SEG1")
  (net 32 "/SEG2")
  (net 33 "/SEG3")
  (net 34 "/SEG4")
  (net 35 "/SEG5")
  (net 36 "/SEG6")
  (net 37 "/SEG7")
  (net 38 "/SEG8")
  (net 39 "/SEG9")
  (net 40 "/SEG10")
  (net 41 "/SEG11")
  (net 42 "/SEG12")
  (net 43 "/SEG13")
  (net 44 "/SEG14")
  (net 45 "/SEG15")
  (net 46 "/SEG16")
  (net 47 "/SEG17")
  (net 48 "/SEG18")
  (net 49 "/SEG19")
  (net 50 "/SEG20")
  (net 51 "/SEG21")
  (net 52 "/SEG23")
  (net 53 "/SEG24")
  (net 54 "/SEG26")
  (net 55 "/SEG27")
  (net 56 "/SEG28")
  (net 57 "/SEG29")
  (net 58 "/SEG30")
  (net 59 "/RH1")
  (net 60 "/RH0")
  (net 61 "/DEBUG")
  (net 62 "/LIGHT")
  (net 63 "unconnected-(U1-RA4/SEG14)")
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 122.46 56.5 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "powerpic.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at 1.6 -0.06) (layer "F.SilkS"))
    (fp_text value "0.27μF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/VLCD3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "powerpic:ppc-board" locked (layer "F.Cu")
    (at 118.015 69.825)
    (descr "PCB Layout for the Casio CA53W")
    (property "Sheetfile" "powerpic.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "PPC1" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "ppc-board" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 1.6 -13.8) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 5.3 -27.3) (size 1 1) (drill 1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 20.3 -27.3) (size 1 1) (drill 1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 23.9 -13.8) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad "1" connect roundrect locked (at 12.9 -25.84) (size 8.3 2.75) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.5)
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_out"))
    (pad "2" connect roundrect locked (at 17.3 -16.4 10) (size 6.4 6) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.1)
      (net 1 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "3" smd circle locked (at 6.75 -5.5) (size 2 2) (layers "B.Cu" "B.Mask")
      (net 14 "/BUZZ") (pinfunction "BUZZ") (pintype "input"))
    (pad "4" thru_hole oval locked (at 25.2 -11) (size 1.2 2.7) (drill oval 0.8 2.3) (layers *.Cu *.Mask)
      (net 9 "/MODE") (pinfunction "MODE") (pintype "output"))
    (pad "5" thru_hole oval locked (at 25.2 -3.8) (size 1.2 2.7) (drill oval 0.8 2.3) (layers *.Cu *.Mask)
      (net 10 "/ADJ") (pinfunction "ADJ") (pintype "output"))
    (pad "6" connect rect locked (at 6.7 -2.6) (size 0.985 1.75) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "NC") (pintype "unspecified"))
    (pad "7" connect rect locked (at 8.2 -2.6) (size 0.985 1.75) (layers "F.Cu" "F.Mask")
      (net 18 "/ROW3") (pinfunction "ROW3") (pintype "bidirectional"))
    (pad "8" connect rect locked (at 9.7 -2.6) (size 0.985 1.75) (layers "F.Cu" "F.Mask")
      (net 19 "/ROW2") (pinfunction "ROW2") (pintype "bidirectional"))
    (pad "9" connect rect locked (at 11.2 -2.6) (size 0.985 1.75) (layers "F.Cu" "F.Mask")
      (net 20 "/ROW1") (pinfunction "ROW1") (pintype "bidirectional"))
    (pad "10" connect rect locked (at 12.7 -2.6) (size 0.985 1.75) (layers "F.Cu" "F.Mask")
      (net 21 "/ROW0") (pinfunction "ROW0") (pintype "bidirectional"))
    (pad "11" connect rect locked (at 14.2 -2.6) (size 0.985 1.75) (layers "F.Cu" "F.Mask")
      (net 22 "/COL0") (pinfunction "COL0") (pintype "bidirectional"))
    (pad "12" connect rect locked (at 15.7 -2.6) (size 0.985 1.75) (layers "F.Cu" "F.Mask")
      (net 23 "/COL1") (pinfunction "COL1") (pintype "bidirectional"))
    (pad "13" connect rect locked (at 17.2 -2.6) (size 0.985 1.75) (layers "F.Cu" "F.Mask")
      (net 24 "/COL2") (pinfunction "COL2") (pintype "bidirectional"))
    (pad "14" connect rect locked (at 18.7 -2.6) (size 0.985 1.75) (layers "F.Cu" "F.Mask")
      (net 25 "/COL3") (pinfunction "COL3") (pintype "bidirectional"))
    (pad "15" connect rect locked (at 2.6 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 26 "/COM0") (pinfunction "COM0") (pintype "input"))
    (pad "16" connect rect locked (at 3.2 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 27 "/COM1") (pinfunction "COM1") (pintype "input"))
    (pad "17" connect rect locked (at 3.8 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 28 "/COM2") (pinfunction "COM2") (pintype "input"))
    (pad "18" connect rect locked (at 4.4 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 29 "/COM3") (pinfunction "COM3") (pintype "input"))
    (pad "19" connect rect locked (at 5 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 30 "/SEG0") (pinfunction "SEG0") (pintype "input"))
    (pad "20" connect rect locked (at 5.6 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 31 "/SEG1") (pinfunction "SEG1") (pintype "input"))
    (pad "21" connect rect locked (at 6.2 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 32 "/SEG2") (pinfunction "SEG2") (pintype "input"))
    (pad "22" connect rect locked (at 6.8 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 33 "/SEG3") (pinfunction "SEG3") (pintype "input"))
    (pad "23" connect rect locked (at 7.4 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 34 "/SEG4") (pinfunction "SEG4") (pintype "input"))
    (pad "24" connect rect locked (at 8 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 35 "/SEG5") (pinfunction "SEG5") (pintype "input"))
    (pad "25" connect rect locked (at 8.6 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 36 "/SEG6") (pinfunction "SEG6") (pintype "input"))
    (pad "26" connect rect locked (at 9.2 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 37 "/SEG7") (pinfunction "SEG7") (pintype "input"))
    (pad "27" connect rect locked (at 9.8 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 38 "/SEG8") (pinfunction "SEG8") (pintype "input"))
    (pad "28" connect rect locked (at 10.4 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 39 "/SEG9") (pinfunction "SEG9") (pintype "input"))
    (pad "29" connect rect locked (at 11 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 40 "/SEG10") (pinfunction "SEG10") (pintype "input"))
    (pad "30" connect rect locked (at 11.6 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 41 "/SEG11") (pinfunction "SEG11") (pintype "input"))
    (pad "31" connect rect locked (at 12.2 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 42 "/SEG12") (pinfunction "SEG12") (pintype "input"))
    (pad "32" connect rect locked (at 12.8 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 43 "/SEG13") (pinfunction "SEG13") (pintype "input"))
    (pad "33" connect rect locked (at 13.4 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 44 "/SEG14") (pinfunction "SEG14") (pintype "input"))
    (pad "34" connect rect locked (at 14 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 45 "/SEG15") (pinfunction "SEG15") (pintype "input"))
    (pad "35" connect rect locked (at 14.6 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 46 "/SEG16") (pinfunction "SEG16") (pintype "input"))
    (pad "36" connect rect locked (at 15.2 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 47 "/SEG17") (pinfunction "SEG17") (pintype "input"))
    (pad "37" connect rect locked (at 15.8 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 48 "/SEG18") (pinfunction "SEG18") (pintype "input"))
    (pad "38" connect rect locked (at 16.4 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 49 "/SEG19") (pinfunction "SEG19") (pintype "input"))
    (pad "39" connect rect locked (at 17 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 50 "/SEG20") (pinfunction "SEG20") (pintype "input"))
    (pad "40" connect rect locked (at 17.6 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 51 "/SEG21") (pinfunction "SEG21") (pintype "input"))
    (pad "41" connect rect locked (at 18.2 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 3 "/SEG22") (pinfunction "SEG22") (pintype "input"))
    (pad "42" connect rect locked (at 18.8 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 52 "/SEG23") (pinfunction "SEG23") (pintype "input"))
    (pad "43" connect rect locked (at 19.4 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 53 "/SEG24") (pinfunction "SEG24") (pintype "input"))
    (pad "44" connect rect locked (at 20 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 4 "/SEG25") (pinfunction "SEG25") (pintype "input"))
    (pad "45" connect rect locked (at 20.6 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 54 "/SEG26") (pinfunction "SEG26") (pintype "input"))
    (pad "46" connect rect locked (at 21.2 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 55 "/SEG27") (pinfunction "SEG27") (pintype "input"))
    (pad "47" connect rect locked (at 21.8 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 56 "/SEG28") (pinfunction "SEG28") (pintype "input"))
    (pad "48" connect rect locked (at 22.4 -16.2) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 57 "/SEG29") (pinfunction "SEG29") (pintype "input"))
    (pad "49" connect rect locked (at 23 -16.2 180) (size 0.31 1.75) (layers "F.Cu" "F.Mask")
      (net 58 "/SEG30") (pinfunction "SEG30") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 126.620589 60.880589 -45)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "powerpic.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at -0.891788 -0.919239) (layer "F.SilkS"))
    (fp_text value "0.1μF" (at 0 1.16 -225) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -225) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.48 0 315) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.48 0 315) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0402_1005Metric" (layer "F.Cu")
    (at 142.91 47.65 90)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "powerpic.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "D1" (at 1.28 -0.39) (layer "F.SilkS"))
    (fp_text value "LCD_LED" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 125.55 63.35 -45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "powerpic.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -1.718269 -0.502046) (layer "F.SilkS"))
    (fp_text value "TBD" (at 0 1.43 135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 315) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(D1-A)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 315) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "/LIGHT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 140.44 60.81 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "powerpic.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 0.05 -1.28) (layer "F.SilkS"))
    (fp_text value "0.1μF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 122.42 60.5 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "powerpic.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C7" (at 1.56 -0.07 180) (layer "F.SilkS"))
    (fp_text value "0.27μF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/VLCD1") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 121.105 63.69 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "powerpic.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 2.165 0) (layer "F.SilkS"))
    (fp_text value "TBD" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/SOSCI") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 119.89 66.595 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "powerpic.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at 1.815 -0.95 180) (layer "F.SilkS"))
    (fp_text value "TBD" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/SOSCO") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm" (layer "F.Cu")
    (at 133.29 60.09)
    (descr "QFN, 64 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/70593d.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (property "Sheetfile" "powerpic.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "8kW FLASH, 1kB RAM, 256B EEPROM, QFN-64")
    (property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller")
    (attr smd)
    (fp_text reference "U1" (at -6.11 -2.5 180) (layer "F.SilkS"))
    (fp_text value "PIC16LF1919x-I/MR" (at 0 5.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd roundrect locked (at -2.025 -2.025) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.2293577982))
    (pad "" smd roundrect locked (at -2.025 -0.675) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.2293577982))
    (pad "" smd roundrect locked (at -2.025 0.675) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.2293577982))
    (pad "" smd roundrect locked (at -2.025 2.025) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.2293577982))
    (pad "" smd roundrect locked (at -0.675 -2.025) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.2293577982))
    (pad "" smd roundrect locked (at -0.675 -0.675) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.2293577982))
    (pad "" smd roundrect locked (at -0.675 0.675) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.2293577982))
    (pad "" smd roundrect locked (at -0.675 2.025) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.2293577982))
    (pad "" smd roundrect locked (at 0.675 -2.025) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.2293577982))
    (pad "" smd roundrect locked (at 0.675 -0.675) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.2293577982))
    (pad "" smd roundrect locked (at 0.675 0.675) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.2293577982))
    (pad "" smd roundrect locked (at 0.675 2.025) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.2293577982))
    (pad "" smd roundrect locked (at 2.025 -2.025) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.2293577982))
    (pad "" smd roundrect locked (at 2.025 -0.675) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.2293577982))
    (pad "" smd roundrect locked (at 2.025 0.675) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.2293577982))
    (pad "" smd roundrect locked (at 2.025 2.025) (size 1.09 1.09) (layers "F.Paste") (roundrect_rratio 0.2293577982))
    (pad "1" smd roundrect locked (at -4.4375 -3.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/VLCD2") (pinfunction "VLCD2/RE1") (pintype "bidirectional"))
    (pad "2" smd roundrect locked (at -4.4375 -3.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/VLCD1") (pinfunction "VLCD1/RE0") (pintype "bidirectional"))
    (pad "3" smd roundrect locked (at -4.4375 -2.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/SEG8") (pinfunction "SEG42/RG0") (pintype "bidirectional"))
    (pad "4" smd roundrect locked (at -4.4375 -2.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "/SEG7") (pinfunction "SEG43/RG1") (pintype "bidirectional"))
    (pad "5" smd roundrect locked (at -4.4375 -1.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/SEG6") (pinfunction "SEG44/RG2") (pintype "bidirectional"))
    (pad "6" smd roundrect locked (at -4.4375 -1.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/SEG5") (pinfunction "SEG45/RG3") (pintype "bidirectional"))
    (pad "7" smd roundrect locked (at -4.4375 -0.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/~{MCLR}") (pinfunction "VPP/~{MCLR}/RG5") (pintype "bidirectional"))
    (pad "8" smd roundrect locked (at -4.4375 -0.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/SEG4") (pinfunction "SEG26/RG4") (pintype "bidirectional"))
    (pad "9" smd roundrect locked (at -4.4375 0.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "10" smd roundrect locked (at -4.4375 0.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "VDD") (pintype "power_in"))
    (pad "11" smd roundrect locked (at -4.4375 1.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/SEG3") (pinfunction "SEG25/RF7") (pintype "bidirectional"))
    (pad "12" smd roundrect locked (at -4.4375 1.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/SEG2") (pinfunction "SEG24/RF6") (pintype "bidirectional"))
    (pad "13" smd roundrect locked (at -4.4375 2.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/SEG1") (pinfunction "SEG23/RF5") (pintype "bidirectional"))
    (pad "14" smd roundrect locked (at -4.4375 2.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/SEG0") (pinfunction "SEG22/RF4") (pintype "bidirectional"))
    (pad "15" smd roundrect locked (at -4.4375 3.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/SEG10") (pinfunction "SEG21/RF3") (pintype "bidirectional"))
    (pad "16" smd roundrect locked (at -4.4375 3.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/SEG11") (pinfunction "SEG20/RF2") (pintype "bidirectional"))
    (pad "17" smd roundrect locked (at -3.75 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/SEG9") (pinfunction "SEG19/RF1") (pintype "bidirectional"))
    (pad "18" smd roundrect locked (at -3.25 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/SEG12") (pinfunction "SEG41/RF0") (pintype "bidirectional"))
    (pad "19" smd roundrect locked (at -2.75 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "/LIGHT") (pinfunction "COM7/SEG15/RG7") (pintype "bidirectional"))
    (pad "20" smd roundrect locked (at -2.25 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/BUZZ") (pinfunction "COM6/RG6") (pintype "bidirectional"))
    (pad "21" smd roundrect locked (at -1.75 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/ROW3") (pinfunction "RA3/SEG35") (pintype "bidirectional"))
    (pad "22" smd roundrect locked (at -1.25 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/ROW2") (pinfunction "RA2/SEG34") (pintype "bidirectional"))
    (pad "23" smd roundrect locked (at -0.75 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/ROW1") (pinfunction "RA1/SEG18") (pintype "bidirectional"))
    (pad "24" smd roundrect locked (at -0.25 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/ROW0") (pinfunction "RA0/SEG33") (pintype "bidirectional"))
    (pad "25" smd roundrect locked (at 0.25 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "/RH1") (pinfunction "COM5/RH1") (pintype "bidirectional"))
    (pad "26" smd roundrect locked (at 0.75 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "/RH0") (pinfunction "COM4/RH0") (pintype "bidirectional"))
    (pad "27" smd roundrect locked (at 1.25 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "unconnected-(U1-RA5)") (pinfunction "RA5") (pintype "bidirectional"))
    (pad "28" smd roundrect locked (at 1.75 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "unconnected-(U1-RA4/SEG14)") (pinfunction "RA4/SEG14") (pintype "bidirectional"))
    (pad "29" smd roundrect locked (at 2.25 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/SOSCI") (pinfunction "RC1") (pintype "bidirectional"))
    (pad "30" smd roundrect locked (at 2.75 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/SOSCO") (pinfunction "RC0") (pintype "bidirectional"))
    (pad "31" smd roundrect locked (at 3.25 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/COL0") (pinfunction "RC6/SEG27") (pintype "bidirectional"))
    (pad "32" smd roundrect locked (at 3.75 4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/COL1") (pinfunction "RC7/SEG28") (pintype "bidirectional"))
    (pad "33" smd roundrect locked (at 4.4375 3.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/COL2") (pinfunction "RC2/SEG13") (pintype "bidirectional"))
    (pad "34" smd roundrect locked (at 4.4375 3.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "/COL3") (pinfunction "RC3/SEG17") (pintype "bidirectional"))
    (pad "35" smd roundrect locked (at 4.4375 2.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/DEBUG") (pinfunction "RC4/SEG16") (pintype "bidirectional"))
    (pad "36" smd roundrect locked (at 4.4375 2.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "/SEG30") (pinfunction "RC5/SEG12") (pintype "bidirectional"))
    (pad "37" smd roundrect locked (at 4.4375 1.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/ADJ") (pinfunction "RB7/SEG39/ICSPDAT") (pintype "bidirectional"))
    (pad "38" smd roundrect locked (at 4.4375 1.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "VDD") (pintype "power_in"))
    (pad "39" smd roundrect locked (at 4.4375 0.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "/SEG13") (pinfunction "RA7/SEG37") (pintype "bidirectional"))
    (pad "40" smd roundrect locked (at 4.4375 0.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "/SEG14") (pinfunction "RA6/SEG36") (pintype "bidirectional"))
    (pad "41" smd roundrect locked (at 4.4375 -0.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "42" smd roundrect locked (at 4.4375 -0.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/MODE") (pinfunction "RB6/SEG38/ICSPCLK") (pintype "bidirectional"))
    (pad "43" smd roundrect locked (at 4.4375 -1.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "/SEG29") (pinfunction "RB5/SEG29") (pintype "bidirectional"))
    (pad "44" smd roundrect locked (at 4.4375 -1.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "/SEG28") (pinfunction "RB4/SEG11") (pintype "bidirectional"))
    (pad "45" smd roundrect locked (at 4.4375 -2.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "/SEG27") (pinfunction "RB3/SEG10") (pintype "bidirectional"))
    (pad "46" smd roundrect locked (at 4.4375 -2.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "/SEG26") (pinfunction "RB2/SEG9") (pintype "bidirectional"))
    (pad "47" smd roundrect locked (at 4.4375 -3.25) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/SEG25") (pinfunction "RB1/SEG8") (pintype "bidirectional"))
    (pad "48" smd roundrect locked (at 4.4375 -3.75) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "/SEG24") (pinfunction "RB0/SEG30") (pintype "bidirectional"))
    (pad "49" smd roundrect locked (at 3.75 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "/SEG23") (pinfunction "RD7/SEG7") (pintype "bidirectional"))
    (pad "50" smd roundrect locked (at 3.25 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/SEG22") (pinfunction "RD6/SEG6") (pintype "bidirectional"))
    (pad "51" smd roundrect locked (at 2.75 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "/SEG21") (pinfunction "RD5/SEG5") (pintype "bidirectional"))
    (pad "52" smd roundrect locked (at 2.25 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "/SEG20") (pinfunction "RD4/SEG4") (pintype "bidirectional"))
    (pad "53" smd roundrect locked (at 1.75 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "/SEG19") (pinfunction "RD3/SEG3") (pintype "bidirectional"))
    (pad "54" smd roundrect locked (at 1.25 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "/SEG18") (pinfunction "RD2/SEG2") (pintype "bidirectional"))
    (pad "55" smd roundrect locked (at 0.75 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "/SEG17") (pinfunction "RD1/SEG1") (pintype "bidirectional"))
    (pad "56" smd roundrect locked (at 0.25 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/CFLY2") (pinfunction "CFLY2/SEG40/RH3") (pintype "bidirectional"))
    (pad "57" smd roundrect locked (at -0.25 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/CFLY1") (pinfunction "CFLY1/SEG32/RH2") (pintype "bidirectional"))
    (pad "58" smd roundrect locked (at -0.75 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "/SEG16") (pinfunction "RD0/SEG0") (pintype "bidirectional"))
    (pad "59" smd roundrect locked (at -1.25 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "/SEG15") (pinfunction "SEG31/RE7") (pintype "bidirectional"))
    (pad "60" smd roundrect locked (at -1.75 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/COM3") (pinfunction "COM3/RE6") (pintype "bidirectional"))
    (pad "61" smd roundrect locked (at -2.25 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/COM2") (pinfunction "COM2/RE5") (pintype "bidirectional"))
    (pad "62" smd roundrect locked (at -2.75 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/COM1") (pinfunction "COM1/RE4") (pintype "bidirectional"))
    (pad "63" smd roundrect locked (at -3.25 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/COM0") (pinfunction "COM0/RE3") (pintype "bidirectional"))
    (pad "64" smd roundrect locked (at -3.75 -4.4375) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/VLCD3") (pinfunction "VLCD3") (pintype "input"))
    (pad "65" smd rect locked (at 0 0) (size 5.4 5.4) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 140.45 57.97 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "powerpic.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C8" (at -0.06 1.28 180) (layer "F.SilkS"))
    (fp_text value "1μF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/CFLY1") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/CFLY2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_SMD_MicroCrystal_CC7V-T1A-2Pin_3.2x1.5mm" (layer "F.Cu")
    (at 121.87 66.47 -90)
    (descr "SMD Crystal MicroCrystal CC7V-T1A/CM7V-T1A series https://www.microcrystal.com/fileadmin/Media/Products/32kHz/Datasheet/CC7V-T1A.pdf, 3.2x1.5mm^2 package")
    (tags "SMD SMT crystal")
    (property "Sheetfile" "powerpic.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Two pin crystal")
    (property "ki_keywords" "quartz ceramic resonator oscillator")
    (attr smd)
    (fp_text reference "Y1" (at -1.65 -2.03) (layer "F.SilkS"))
    (fp_text value "32.768kHz" (at 0 1.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.25 0 270) (size 1 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/SOSCI") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 1.25 0 270) (size 1 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/SOSCO") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_MicroCrystal_CC7V-T1A-2Pin_3.2x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 122.42 58.5 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "powerpic.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C6" (at 1.56 -0.07 180) (layer "F.SilkS"))
    (fp_text value "0.27μF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/VLCD2") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "powerpic:Progo_Pad_D2.0mm" (layer "B.Cu")
    (at 139.865 68.025 180)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "powerpic.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP3" (at 0 1.535) (layer "B.SilkS") hide)
    (fp_text value "Adj" (at 0 -2.05) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2) (layer "B.Fab"))
    (pad "1" smd circle (at 0 0 180) (size 2 2) (property pad_prop_testpoint) (layers "B.Cu" "B.Mask")
      (net 10 "/ADJ") (pinfunction "1") (pintype "passive"))
  )
  (footprint "powerpic:Progo_Pad_D2.0mm" (layer "B.Cu")
    (at 137.325 68.025 180)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "powerpic.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP2" (at -0.065 2.595 90) (layer "B.SilkS") hide)
    (fp_text value "Mode" (at 0 -2.05) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2) (layer "B.Fab"))
    (pad "1" smd circle (at 0 0 180) (size 2 2) (property pad_prop_testpoint) (layers "B.Cu" "B.Mask")
      (net 9 "/MODE") (pinfunction "1") (pintype "passive"))
  )
  (footprint "powerpic:Progo_Pad_D2.0mm" (layer "B.Cu")
    (at 134.785 68.025 180)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "powerpic.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at -0.235 3.135 90) (layer "B.SilkS") hide)
    (fp_text value "~{MCLR}" (at 0 -2.05) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2) (layer "B.Fab"))
    (pad "1" smd circle (at 0 0 180) (size 2 2) (property pad_prop_testpoint) (layers "B.Cu" "B.Mask")
      (net 11 "/~{MCLR}") (pinfunction "1") (pintype "passive"))
  )
  (footprint "powerpic:Progo_Pad_D2.0mm" (layer "B.Cu")
    (at 140.765 64.425 180)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "powerpic.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP4" (at 0.185 1.635 180) (layer "B.SilkS") hide)
    (fp_text value "Debug" (at 0 -2.05) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2) (layer "B.Fab"))
    (pad "1" smd circle (at 0 0 180) (size 2 2) (property pad_prop_testpoint) (layers "B.Cu" "B.Mask")
      (net 61 "/DEBUG") (pinfunction "1") (pintype "passive"))
  )
  (gr_arc (start 120.515 69.825) (mid 118.747233 69.092767) (end 118.015 67.325)
    (layer "Edge.Cuts"))
  (gr_arc (start 118.015 44.725) (mid 118.747233 42.957234) (end 120.515 42.225)
    (layer "Edge.Cuts"))
  (gr_line (start 118.015 44.725) (end 118.015 67.325)
    (layer "Edge.Cuts"))
  (gr_arc (start 143.615 67.325) (mid 142.882767 69.092767) (end 141.115 69.825)
    (layer "Edge.Cuts"))
  (gr_line (start 143.615 44.725) (end 143.615 55.925)
    (layer "Edge.Cuts"))
  (gr_line (start 143.615 67.025) (end 143.615 67.325)
    (layer "Edge.Cuts"))
  (gr_line (start 120.515 69.825) (end 141.115 69.825)
    (layer "Edge.Cuts"))
  (gr_line (start 143.615 55.925) (end 143.015 56.625)
    (layer "Edge.Cuts"))
  (gr_line (start 141.115 42.225) (end 120.515 42.225)
    (layer "Edge.Cuts"))
  (gr_line (start 143.015 56.625) (end 143.015 67.025)
    (layer "Edge.Cuts"))
  (gr_line (start 143.015 67.025) (end 143.615 67.025)
    (layer "Edge.Cuts"))
  (gr_arc (start 141.115 42.225) (mid 142.882767 42.957233) (end 143.615 44.725)
    (layer "Edge.Cuts"))
  (gr_text "Manufactured\nby JLCPCB\nin May 2022" (at 122.79 44.2) (layer "B.Cu"))
  (gr_text "Designed by\nRex McKinnon\nin Oakland CA" (at 139.06 44.19) (layer "B.Cu"))
  (gr_text "2.0" (at 131.73 60.23) (layer "B.SilkS"))
  (gr_text "VIN" (at 130.87 46.52) (layer "B.SilkS" knockout))
  (gr_text "C" (at 136.36 67.06 -45) (layer "B.SilkS" knockout))
  (gr_text "R" (at 133.94 67.01 315) (layer "B.SilkS" knockout))
  (gr_text "BUZ" (at 123.28 64.48) (layer "B.SilkS" knockout))
  (gr_text "GND" (at 134.59 49.3 10) (layer "B.SilkS" knockout))
  (gr_text "ICSP" (at 130.99 68.12) (layer "B.SilkS" knockout))
  (gr_text "GND" (at 121.7 67.34) (layer "B.SilkS" knockout))
  (gr_text "D" (at 138.99 67.01 315) (layer "B.SilkS" knockout))
  (gr_text "DBG" (at 139.29 64.52) (layer "B.SilkS" knockout))
  (gr_text "PowerPIC" (at 134.1 58.72) (layer "B.SilkS"))
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508) (island_removal_mode 2) (island_area_min 10))
    (polygon
      (pts
        (xy 137.2 68.25)
        (xy 125.21 68.25)
        (xy 125.21 66.2)
        (xy 137.2 66.2)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508) (island_removal_mode 2) (island_area_min 10))
    (polygon
      (pts
        (xy 141.79 54.65)
        (xy 119.84 54.65)
        (xy 119.84 52.6)
        (xy 141.79 52.6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508) (island_removal_mode 2) (island_area_min 10))
    (polygon
      (pts
        (xy 125.57 64.26)
        (xy 124.681077 63.371385)
        (xy 125.47 63.67)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (priority 100)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.1524) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 143.71 69.72)
        (xy 118.01 69.72)
        (xy 118.02 41.65)
        (xy 143.72 41.65)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508) (island_removal_mode 2) (island_area_min 10))
    (polygon
      (pts
        (xy 143.31 47.49)
        (xy 143.22 47.49)
        (xy 143.14 47.08)
        (xy 142.74 46.25)
        (xy 142.04 45.73)
        (xy 141.26 45.55)
        (xy 141.26 45.23)
        (xy 143.31 45.23)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 150)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.1524) (thermal_bridge_width 0.508) (island_removal_mode 2) (island_area_min 10))
    (polygon
      (pts
        (xy 140.58 59.01)
        (xy 131.89 59.01)
        (xy 130.89 49.27)
        (xy 139.58 49.27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508) (island_removal_mode 2) (island_area_min 10))
    (polygon
      (pts
        (xy 120.37 45.52)
        (xy 119.96 45.59)
        (xy 119.54 45.73)
        (xy 119.19 45.93)
        (xy 118.83 46.28)
        (xy 118.53 46.85)
        (xy 118.43 47.49)
        (xy 117.9 47.49)
        (xy 117.9 45.43)
        (xy 120.37 45.43)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508) (island_removal_mode 2) (island_area_min 10))
    (polygon
      (pts
        (xy 144 45.52)
        (xy 117.9 45.52)
        (xy 117.9 41.88)
        (xy 144 41.88)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.SilkS") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints not_allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508) (island_removal_mode 2) (island_area_min 10))
    (polygon
      (pts
        (xy 133.64 66.93)
        (xy 133.64 67.14)
        (xy 133.55 67.14)
        (xy 133.53 67.02)
        (xy 133.63 66.92)
      )
    )
  )
)
