(kicad_sch (version 20220404) (generator eeschema)
  (paper "A4" portrait)
  (title_block
    (title "Power PIC Calculator Watch")
    (date "2022-05-12")
    (rev "2.0")
    (comment 1 "Designed by Rex McKinnon <0xff@rexploits.com>")
    (comment 2 "${KICAD_VERSION}")
  )
  (lib_symbols
    (symbol "Connector:TestPoint" (pin_numbers hide) (pin_names (offset 0.762) hide) (in_bom yes) (on_board yes)
      (property "Reference" "TP" (id 0) (at 0 6.858 0))
      (property "Value" "TestPoint" (id 1) (at 0 5.08 0))
      (property "Footprint" "" (id 2) (at 5.08 0 0))
      (property "Datasheet" "~" (id 3) (at 5.08 0 0))
      (property "ki_keywords" "test point tp" (id 4) (at 0 0 0))
      (property "ki_description" "test point" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Pin* Test*" (id 6) (at 0 0 0))
      (symbol "TestPoint_0_1"
        (circle (center 0 3.302) (radius 0.762)
          (fill (type none))
        )
      )
      (symbol "TestPoint_1_1"
        (pin passive line (at 0 0 90) (length 2.54)
          (name "1")
          (number "1")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:Crystal" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Y" (id 0) (at 0 3.81 0))
      (property "Value" "Crystal" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "quartz ceramic resonator oscillator" (id 4) (at 0 0 0))
      (property "ki_description" "Two pin crystal" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Crystal*" (id 6) (at 0 0 0))
      (symbol "Crystal_0_1"
        (rectangle (start -1.143 2.54) (end 1.143 -2.54)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 0)
            (xy -1.905 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.905 -1.27)
            (xy 1.905 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 0)
            (xy 1.905 0)
          )
          (fill (type none))
        )
      )
      (symbol "Crystal_1_1"
        (pin passive line (at -3.81 0 0) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 1.27)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Device:LED" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "LED" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "LED diode" (id 4) (at 0 0 0))
      (property "ki_description" "Light emitting diode" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (id 6) (at 0 0 0))
      (symbol "LED_0_1"
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy -1.27 0)
            (xy 1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.048 -0.762)
            (xy -4.572 -2.286)
            (xy -3.81 -2.286)
            (xy -4.572 -2.286)
            (xy -4.572 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 -0.762)
            (xy -3.302 -2.286)
            (xy -2.54 -2.286)
            (xy -3.302 -2.286)
            (xy -3.302 -1.524)
          )
          (fill (type none))
        )
      )
      (symbol "LED_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
    (symbol "power:VCC" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "VCC" (id 1) (at 0 3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"VCC\"" (id 5) (at 0 0 0))
      (symbol "VCC_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "VCC_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "VCC")
          (number "1")
        )
      )
    )
    (symbol "powerpic:PIC16F1919x-xMR" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -29.845 29.845 0))
      (property "Value" "PIC16F1919x-xMR" (id 1) (at 0 0 0))
      (property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm" (id 2) (at 0 0 0))
      (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF19195-6-7-Data-Sheet-40001873D.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller" (id 4) (at 0 0 0))
      (property "ki_description" "8kW FLASH, 1kB RAM, 256B EEPROM, QFN-64" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "QFN*9x9mm*P0.5mm*" (id 6) (at 0 0 0))
      (symbol "PIC16F1919x-xMR_0_1"
        (polyline
          (pts
            (xy -31.75 25.4)
            (xy -25.4 31.75)
            (xy 31.75 31.75)
            (xy 31.75 -31.75)
            (xy -31.75 -31.75)
            (xy -31.75 25.4)
          )
          (fill (type background))
        )
      )
      (symbol "PIC16F1919x-xMR_1_1"
        (pin bidirectional line (at -34.29 19.05 0) (length 2.54)
          (name "VLCD2/RE1")
          (number "1")
        )
        (pin power_in line (at -34.29 -3.81 0) (length 2.54)
          (name "VDD")
          (number "10")
        )
        (pin bidirectional line (at -34.29 -6.35 0) (length 2.54)
          (name "SEG25/RF7")
          (number "11")
        )
        (pin bidirectional line (at -34.29 -8.89 0) (length 2.54)
          (name "SEG24/RF6")
          (number "12")
        )
        (pin bidirectional line (at -34.29 -11.43 0) (length 2.54)
          (name "SEG23/RF5")
          (number "13")
        )
        (pin bidirectional line (at -34.29 -13.97 0) (length 2.54)
          (name "SEG22/RF4")
          (number "14")
        )
        (pin bidirectional line (at -34.29 -16.51 0) (length 2.54)
          (name "SEG21/RF3")
          (number "15")
        )
        (pin bidirectional line (at -34.29 -19.05 0) (length 2.54)
          (name "SEG20/RF2")
          (number "16")
        )
        (pin bidirectional line (at -19.05 -34.29 90) (length 2.54)
          (name "SEG19/RF1")
          (number "17")
        )
        (pin bidirectional line (at -16.51 -34.29 90) (length 2.54)
          (name "SEG41/RF0")
          (number "18")
        )
        (pin bidirectional line (at -13.97 -34.29 90) (length 2.54)
          (name "COM7/SEG15/RG7")
          (number "19")
        )
        (pin bidirectional line (at -34.29 16.51 0) (length 2.54)
          (name "VLCD1/RE0")
          (number "2")
        )
        (pin bidirectional line (at -11.43 -34.29 90) (length 2.54)
          (name "COM6/RG6")
          (number "20")
        )
        (pin bidirectional line (at -8.89 -34.29 90) (length 2.54)
          (name "RA3/SEG35")
          (number "21")
        )
        (pin bidirectional line (at -6.35 -34.29 90) (length 2.54)
          (name "RA2/SEG34")
          (number "22")
        )
        (pin bidirectional line (at -3.81 -34.29 90) (length 2.54)
          (name "RA1/SEG18")
          (number "23")
        )
        (pin bidirectional line (at -1.27 -34.29 90) (length 2.54)
          (name "RA0/SEG33")
          (number "24")
        )
        (pin bidirectional line (at 1.27 -34.29 90) (length 2.54)
          (name "COM5/RH1")
          (number "25")
        )
        (pin bidirectional line (at 3.81 -34.29 90) (length 2.54)
          (name "COM4/RH0")
          (number "26")
        )
        (pin bidirectional line (at 6.35 -34.29 90) (length 2.54)
          (name "RA5")
          (number "27")
        )
        (pin bidirectional line (at 8.89 -34.29 90) (length 2.54)
          (name "RA4/SEG14")
          (number "28")
        )
        (pin bidirectional line (at 11.43 -34.29 90) (length 2.54)
          (name "RC1")
          (number "29")
        )
        (pin bidirectional line (at -34.29 13.97 0) (length 2.54)
          (name "SEG42/RG0")
          (number "3")
        )
        (pin bidirectional line (at 13.97 -34.29 90) (length 2.54)
          (name "RC0")
          (number "30")
        )
        (pin bidirectional line (at 16.51 -34.29 90) (length 2.54)
          (name "RC6/SEG27")
          (number "31")
        )
        (pin bidirectional line (at 19.05 -34.29 90) (length 2.54)
          (name "RC7/SEG28")
          (number "32")
        )
        (pin bidirectional line (at 34.29 -19.05 180) (length 2.54)
          (name "RC2/SEG13")
          (number "33")
        )
        (pin bidirectional line (at 34.29 -16.51 180) (length 2.54)
          (name "RC3/SEG17")
          (number "34")
        )
        (pin bidirectional line (at 34.29 -13.97 180) (length 2.54)
          (name "RC4/SEG16")
          (number "35")
        )
        (pin bidirectional line (at 34.29 -11.43 180) (length 2.54)
          (name "RC5/SEG12")
          (number "36")
        )
        (pin bidirectional line (at 34.29 -8.89 180) (length 2.54)
          (name "RB7/SEG39/ICSPDAT")
          (number "37")
        )
        (pin power_in line (at 34.29 -6.35 180) (length 2.54)
          (name "VDD")
          (number "38")
        )
        (pin bidirectional line (at 34.29 -3.81 180) (length 2.54)
          (name "RA7/SEG37")
          (number "39")
        )
        (pin bidirectional line (at -34.29 11.43 0) (length 2.54)
          (name "SEG43/RG1")
          (number "4")
        )
        (pin bidirectional line (at 34.29 -1.27 180) (length 2.54)
          (name "RA6/SEG36")
          (number "40")
        )
        (pin power_in line (at 34.29 1.27 180) (length 2.54)
          (name "VSS")
          (number "41")
        )
        (pin bidirectional line (at 34.29 3.81 180) (length 2.54)
          (name "RB6/SEG38/ICSPCLK")
          (number "42")
        )
        (pin bidirectional line (at 34.29 6.35 180) (length 2.54)
          (name "RB5/SEG29")
          (number "43")
        )
        (pin bidirectional line (at 34.29 8.89 180) (length 2.54)
          (name "RB4/SEG11")
          (number "44")
        )
        (pin bidirectional line (at 34.29 11.43 180) (length 2.54)
          (name "RB3/SEG10")
          (number "45")
        )
        (pin bidirectional line (at 34.29 13.97 180) (length 2.54)
          (name "RB2/SEG9")
          (number "46")
        )
        (pin bidirectional line (at 34.29 16.51 180) (length 2.54)
          (name "RB1/SEG8")
          (number "47")
        )
        (pin bidirectional line (at 34.29 19.05 180) (length 2.54)
          (name "RB0/SEG30")
          (number "48")
        )
        (pin bidirectional line (at 19.05 34.29 270) (length 2.54)
          (name "RD7/SEG7")
          (number "49")
        )
        (pin bidirectional line (at -34.29 8.89 0) (length 2.54)
          (name "SEG44/RG2")
          (number "5")
        )
        (pin bidirectional line (at 16.51 34.29 270) (length 2.54)
          (name "RD6/SEG6")
          (number "50")
        )
        (pin bidirectional line (at 13.97 34.29 270) (length 2.54)
          (name "RD5/SEG5")
          (number "51")
        )
        (pin bidirectional line (at 11.43 34.29 270) (length 2.54)
          (name "RD4/SEG4")
          (number "52")
        )
        (pin bidirectional line (at 8.89 34.29 270) (length 2.54)
          (name "RD3/SEG3")
          (number "53")
        )
        (pin bidirectional line (at 6.35 34.29 270) (length 2.54)
          (name "RD2/SEG2")
          (number "54")
        )
        (pin bidirectional line (at 3.81 34.29 270) (length 2.54)
          (name "RD1/SEG1")
          (number "55")
        )
        (pin bidirectional line (at 1.27 34.29 270) (length 2.54)
          (name "CFLY2/SEG40/RH3")
          (number "56")
        )
        (pin bidirectional line (at -1.27 34.29 270) (length 2.54)
          (name "CFLY1/SEG32/RH2")
          (number "57")
        )
        (pin bidirectional line (at -3.81 34.29 270) (length 2.54)
          (name "RD0/SEG0")
          (number "58")
        )
        (pin bidirectional line (at -6.35 34.29 270) (length 2.54)
          (name "SEG31/RE7")
          (number "59")
        )
        (pin bidirectional line (at -34.29 6.35 0) (length 2.54)
          (name "SEG45/RG3")
          (number "6")
        )
        (pin bidirectional line (at -8.89 34.29 270) (length 2.54)
          (name "COM3/RE6")
          (number "60")
        )
        (pin bidirectional line (at -11.43 34.29 270) (length 2.54)
          (name "COM2/RE5")
          (number "61")
        )
        (pin bidirectional line (at -13.97 34.29 270) (length 2.54)
          (name "COM1/RE4")
          (number "62")
        )
        (pin bidirectional line (at -16.51 34.29 270) (length 2.54)
          (name "COM0/RE3")
          (number "63")
        )
        (pin input line (at -19.05 34.29 270) (length 2.54)
          (name "VLCD3")
          (number "64")
        )
        (pin power_in line (at -34.29 -1.27 0) (length 2.54) hide
          (name "VSS")
          (number "65")
        )
        (pin bidirectional line (at -34.29 3.81 0) (length 2.54)
          (name "VPP/~{MCLR}/RG5")
          (number "7")
        )
        (pin bidirectional line (at -34.29 1.27 0) (length 2.54)
          (name "SEG26/RG4")
          (number "8")
        )
        (pin power_in line (at -34.29 -1.27 0) (length 2.54)
          (name "VSS")
          (number "9")
        )
      )
    )
    (symbol "powerpic:ppc-board" (pin_numbers hide) (in_bom yes) (on_board yes)
      (property "Reference" "PPC" (id 0) (at 0 0 0))
      (property "Value" "ppc-board" (id 1) (at 0 0 0))
      (property "Footprint" "ppc-watch:ppc-board" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0.381 0 0))
      (property "ki_locked" "" (id 4) (at 0 0 0))
      (symbol "ppc-board_1_0"
        (circle (center 0 0) (radius 5.08)
          (fill (type background))
        )
        (text "+" (at -3.81 0 900))
        (text "-" (at 3.81 0 900))
        (text "3v" (at 0 1.778 0))
        (text "CR2016" (at 0 -2.032 0))
      )
      (symbol "ppc-board_1_1"
        (polyline
          (pts
            (xy -5.08 0)
            (xy -6.35 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.08 0)
            (xy 6.35 0)
          )
          (fill (type none))
        )
        (pin power_out line (at -6.35 0 0) (length 1.27) hide
          (name "VCC")
          (number "1")
        )
        (pin power_out line (at 6.35 0 180) (length 1.27) hide
          (name "GND")
          (number "2")
        )
      )
      (symbol "ppc-board_2_0"
        (circle (center -0.635 0) (radius 3.175)
          (fill (type background))
        )
      )
      (symbol "ppc-board_2_1"
        (pin input line (at 3.81 0 180) (length 1.27)
          (name "BUZZ")
          (number "3")
        )
      )
      (symbol "ppc-board_3_0"
        (polyline
          (pts
            (xy 4.445 -3.81)
            (xy 4.445 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.445 -1.27)
            (xy 4.445 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.318 1.524)
            (xy 5.08 1.524)
            (xy 5.08 3.556)
            (xy 4.318 3.556)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.445 3.81)
            (xy 4.445 5.08)
            (xy -2.54 5.08)
            (xy -2.54 -5.08)
            (xy 4.445 -5.08)
            (xy 4.445 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.3688 5.0038)
            (xy 4.3688 3.8354)
            (xy 4.0132 3.3528)
            (xy 3.8354 2.8194)
            (xy 3.8608 2.1082)
            (xy 4.1148 1.5494)
            (xy 4.3434 1.2954)
            (xy 4.3434 0.8636)
            (xy 4.3434 -1.27)
            (xy 4.0894 -1.6256)
            (xy 3.8354 -2.54)
            (xy 4.0386 -3.3782)
            (xy 4.3688 -3.8354)
            (xy 4.3688 -4.9784)
            (xy -2.4384 -4.9784)
            (xy -2.4384 5.0292)
            (xy 4.3688 5.0038)
          )
          (fill (type background))
        )
      )
      (symbol "ppc-board_3_1"
        (arc (start 4.4449 -3.81) (mid 7.5111 -2.54) (end 4.4449 -1.27)
          (fill (type none))
        )
        (arc (start 4.4449 1.27) (mid 7.5111 2.54) (end 4.4449 3.81)
          (fill (type none))
        )
        (pin output line (at -3.81 2.54 0) (length 1.27)
          (name "MODE")
          (number "4")
        )
        (pin output line (at -3.81 -2.54 0) (length 1.27)
          (name "ADJ")
          (number "5")
        )
      )
      (symbol "ppc-board_4_0"
        (rectangle (start -5.08 12.7) (end 3.81 -12.7)
          (fill (type none))
        )
        (rectangle (start -2.54 11.43) (end 3.81 -11.43)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 3.81 11.43)
            (xy 3.81 12.7)
            (xy -5.08 12.7)
            (xy -5.08 -12.7)
            (xy 3.81 -12.7)
            (xy 3.81 -11.43)
            (xy -2.54 -11.43)
            (xy -2.54 11.43)
            (xy 3.81 11.43)
          )
          (fill (type outline))
        )
        (rectangle (start 3.81 -8.89) (end -2.54 -11.43)
          (fill (type none))
        )
        (rectangle (start 3.81 -6.35) (end -2.54 -8.89)
          (fill (type none))
        )
        (rectangle (start 3.81 -3.81) (end -2.54 -6.35)
          (fill (type none))
        )
        (rectangle (start 3.81 -1.27) (end -2.54 -3.81)
          (fill (type none))
        )
        (rectangle (start 3.81 1.27) (end -2.54 -1.27)
          (fill (type none))
        )
        (rectangle (start 3.81 3.81) (end -2.54 1.27)
          (fill (type none))
        )
        (rectangle (start 3.81 6.35) (end -2.54 3.81)
          (fill (type none))
        )
        (rectangle (start 3.81 8.89) (end -2.54 6.35)
          (fill (type none))
        )
        (rectangle (start 3.81 11.43) (end -2.54 8.89)
          (fill (type none))
        )
      )
      (symbol "ppc-board_4_1"
        (pin bidirectional line (at 6.35 0 180) (length 2.54)
          (name "ROW0")
          (number "10")
        )
        (pin bidirectional line (at 6.35 -2.54 180) (length 2.54)
          (name "COL0")
          (number "11")
        )
        (pin bidirectional line (at 6.35 -5.08 180) (length 2.54)
          (name "COL1")
          (number "12")
        )
        (pin bidirectional line (at 6.35 -7.62 180) (length 2.54)
          (name "COL2")
          (number "13")
        )
        (pin bidirectional line (at 6.35 -10.16 180) (length 2.54)
          (name "COL3")
          (number "14")
        )
        (pin unspecified line (at 6.35 10.16 180) (length 2.54)
          (name "NC")
          (number "6")
        )
        (pin bidirectional line (at 6.35 7.62 180) (length 2.54)
          (name "ROW3")
          (number "7")
        )
        (pin bidirectional line (at 6.35 5.08 180) (length 2.54)
          (name "ROW2")
          (number "8")
        )
        (pin bidirectional line (at 6.35 2.54 180) (length 2.54)
          (name "ROW1")
          (number "9")
        )
      )
      (symbol "ppc-board_5_0"
        (rectangle (start -3.81 -43.18) (end 3.81 -45.72)
          (fill (type none))
        )
        (rectangle (start -3.81 -40.64) (end 3.81 -43.18)
          (fill (type none))
        )
        (rectangle (start -3.81 -38.1) (end 3.81 -40.64)
          (fill (type none))
        )
        (rectangle (start -3.81 -35.56) (end 3.81 -38.1)
          (fill (type none))
        )
        (rectangle (start -3.81 -33.02) (end 3.81 -35.56)
          (fill (type none))
        )
        (rectangle (start -3.81 -30.48) (end 3.81 -33.02)
          (fill (type none))
        )
        (rectangle (start -3.81 -27.94) (end 3.81 -30.48)
          (fill (type none))
        )
        (rectangle (start -3.81 -25.4) (end 3.81 -27.94)
          (fill (type none))
        )
        (rectangle (start -3.81 -22.86) (end 3.81 -25.4)
          (fill (type none))
        )
        (rectangle (start -3.81 -20.32) (end 3.81 -22.86)
          (fill (type none))
        )
        (rectangle (start -3.81 -17.78) (end 3.81 -20.32)
          (fill (type none))
        )
        (rectangle (start -3.81 -15.24) (end 3.81 -17.78)
          (fill (type none))
        )
        (rectangle (start -3.81 -12.7) (end 3.81 -15.24)
          (fill (type none))
        )
        (rectangle (start -3.81 -10.16) (end 3.81 -12.7)
          (fill (type none))
        )
        (rectangle (start -3.81 -7.62) (end 3.81 -10.16)
          (fill (type none))
        )
        (rectangle (start -3.81 -5.08) (end 3.81 -7.62)
          (fill (type none))
        )
        (rectangle (start -3.81 -2.54) (end 3.81 -5.08)
          (fill (type none))
        )
        (rectangle (start -3.81 0) (end 3.81 -2.54)
          (fill (type none))
        )
        (rectangle (start -3.81 2.54) (end 3.81 0)
          (fill (type none))
        )
        (rectangle (start -3.81 5.08) (end 3.81 2.54)
          (fill (type none))
        )
        (rectangle (start -3.81 7.62) (end 3.81 5.08)
          (fill (type none))
        )
        (rectangle (start -3.81 10.16) (end 3.81 7.62)
          (fill (type none))
        )
        (rectangle (start -3.81 12.7) (end 3.81 10.16)
          (fill (type none))
        )
        (rectangle (start -3.81 15.24) (end 3.81 12.7)
          (fill (type none))
        )
        (rectangle (start -3.81 17.78) (end 3.81 15.24)
          (fill (type none))
        )
        (rectangle (start -3.81 20.32) (end 3.81 17.78)
          (fill (type none))
        )
        (rectangle (start -3.81 22.86) (end 3.81 20.32)
          (fill (type none))
        )
        (rectangle (start -3.81 25.4) (end 3.81 22.86)
          (fill (type none))
        )
        (rectangle (start -3.81 27.94) (end 3.81 25.4)
          (fill (type none))
        )
        (rectangle (start -3.81 30.48) (end 3.81 27.94)
          (fill (type none))
        )
        (rectangle (start -3.81 33.02) (end 3.81 30.48)
          (fill (type none))
        )
        (rectangle (start -3.81 35.56) (end 3.81 33.02)
          (fill (type none))
        )
        (rectangle (start -3.81 38.1) (end 3.81 35.56)
          (fill (type none))
        )
        (rectangle (start -3.81 40.64) (end 3.81 38.1)
          (fill (type none))
        )
        (rectangle (start -3.81 43.18) (end 3.81 -45.72)
          (fill (type background))
        )
        (rectangle (start -3.81 43.18) (end 3.81 40.64)
          (fill (type none))
        )
        (rectangle (start -3.81 44.45) (end 6.35 -46.99)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.81 43.18)
            (xy -3.81 44.45)
            (xy 6.35 44.45)
            (xy 6.35 -46.99)
            (xy -3.81 -46.99)
            (xy -3.81 -45.72)
            (xy 3.81 -45.72)
            (xy 3.81 43.18)
            (xy -3.81 43.18)
          )
          (fill (type outline))
        )
      )
      (symbol "ppc-board_5_1"
        (pin input line (at -6.35 41.91 0) (length 2.54)
          (name "COM0")
          (number "15")
        )
        (pin input line (at -6.35 39.37 0) (length 2.54)
          (name "COM1")
          (number "16")
        )
        (pin input line (at -6.35 36.83 0) (length 2.54)
          (name "COM2")
          (number "17")
        )
        (pin input line (at -6.35 34.29 0) (length 2.54)
          (name "COM3")
          (number "18")
        )
        (pin input line (at -6.35 31.75 0) (length 2.54)
          (name "SEG0")
          (number "19")
        )
        (pin input line (at -6.35 29.21 0) (length 2.54)
          (name "SEG1")
          (number "20")
        )
        (pin input line (at -6.35 26.67 0) (length 2.54)
          (name "SEG2")
          (number "21")
        )
        (pin input line (at -6.35 24.13 0) (length 2.54)
          (name "SEG3")
          (number "22")
        )
        (pin input line (at -6.35 21.59 0) (length 2.54)
          (name "SEG4")
          (number "23")
        )
        (pin input line (at -6.35 19.05 0) (length 2.54)
          (name "SEG5")
          (number "24")
        )
        (pin input line (at -6.35 16.51 0) (length 2.54)
          (name "SEG6")
          (number "25")
        )
        (pin input line (at -6.35 13.97 0) (length 2.54)
          (name "SEG7")
          (number "26")
        )
        (pin input line (at -6.35 11.43 0) (length 2.54)
          (name "SEG8")
          (number "27")
        )
        (pin input line (at -6.35 8.89 0) (length 2.54)
          (name "SEG9")
          (number "28")
        )
        (pin input line (at -6.35 6.35 0) (length 2.54)
          (name "SEG10")
          (number "29")
        )
        (pin input line (at -6.35 3.81 0) (length 2.54)
          (name "SEG11")
          (number "30")
        )
        (pin input line (at -6.35 1.27 0) (length 2.54)
          (name "SEG12")
          (number "31")
        )
        (pin input line (at -6.35 -1.27 0) (length 2.54)
          (name "SEG13")
          (number "32")
        )
        (pin input line (at -6.35 -3.81 0) (length 2.54)
          (name "SEG14")
          (number "33")
        )
        (pin input line (at -6.35 -6.35 0) (length 2.54)
          (name "SEG15")
          (number "34")
        )
        (pin input line (at -6.35 -8.89 0) (length 2.54)
          (name "SEG16")
          (number "35")
        )
        (pin input line (at -6.35 -11.43 0) (length 2.54)
          (name "SEG17")
          (number "36")
        )
        (pin input line (at -6.35 -13.97 0) (length 2.54)
          (name "SEG18")
          (number "37")
        )
        (pin input line (at -6.35 -16.51 0) (length 2.54)
          (name "SEG19")
          (number "38")
        )
        (pin input line (at -6.35 -19.05 0) (length 2.54)
          (name "SEG20")
          (number "39")
        )
        (pin input line (at -6.35 -21.59 0) (length 2.54)
          (name "SEG21")
          (number "40")
        )
        (pin input line (at -6.35 -24.13 0) (length 2.54)
          (name "SEG22")
          (number "41")
        )
        (pin input line (at -6.35 -26.67 0) (length 2.54)
          (name "SEG23")
          (number "42")
        )
        (pin input line (at -6.35 -29.21 0) (length 2.54)
          (name "SEG24")
          (number "43")
        )
        (pin input line (at -6.35 -31.75 0) (length 2.54)
          (name "SEG25")
          (number "44")
        )
        (pin input line (at -6.35 -34.29 0) (length 2.54)
          (name "SEG26")
          (number "45")
        )
        (pin input line (at -6.35 -36.83 0) (length 2.54)
          (name "SEG27")
          (number "46")
        )
        (pin input line (at -6.35 -39.37 0) (length 2.54)
          (name "SEG28")
          (number "47")
        )
        (pin input line (at -6.35 -41.91 0) (length 2.54)
          (name "SEG29")
          (number "48")
        )
        (pin input line (at -6.35 -44.45 0) (length 2.54)
          (name "SEG30")
          (number "49")
        )
      )
    )
  )
  (junction (at 33.02 154.94) (diameter 0) (color 0 0 0 0))
  (junction (at 33.02 167.64) (diameter 0) (color 0 0 0 0))
  (junction (at 45.72 167.64) (diameter 0) (color 0 0 0 0))
  (junction (at 22.86 199.39) (diameter 0) (color 0 0 0 0))
  (junction (at 45.72 173.99) (diameter 0) (color 0 0 0 0))
  (junction (at 38.1 203.2) (diameter 0) (color 0 0 0 0))
  (junction (at 36.83 85.09) (diameter 0) (color 0 0 0 0))
  (junction (at 22.86 207.01) (diameter 0) (color 0 0 0 0))
  (no_connect (at 114.3 195.58))
  (no_connect (at 111.76 195.58))
  (no_connect (at 106.68 195.58))
  (no_connect (at 109.22 195.58))
  (bus_entry (at 143.51 88.9) (size 2.54 -2.54))
  (bus_entry (at 130.81 88.9) (size 2.54 -2.54))
  (bus_entry (at 53.34 156.21) (size 2.54 2.54))
  (bus_entry (at 133.35 88.9) (size 2.54 -2.54))
  (bus_entry (at 53.34 166.37) (size 2.54 2.54))
  (bus_entry (at 87.63 88.9) (size 2.54 -2.54))
  (bus_entry (at 53.34 176.53) (size 2.54 2.54))
  (bus_entry (at 140.97 88.9) (size 2.54 -2.54))
  (bus_entry (at 85.09 88.9) (size 2.54 -2.54))
  (bus_entry (at 138.43 88.9) (size 2.54 -2.54))
  (bus_entry (at 86.36 107.95) (size 2.54 2.54))
  (bus_entry (at 110.49 88.9) (size 2.54 -2.54))
  (bus_entry (at 121.92 107.95) (size 2.54 2.54))
  (bus_entry (at 67.31 88.9) (size 2.54 -2.54))
  (bus_entry (at 62.23 88.9) (size 2.54 -2.54))
  (bus_entry (at 64.77 88.9) (size 2.54 -2.54))
  (bus_entry (at 77.47 88.9) (size 2.54 -2.54))
  (bus_entry (at 80.01 88.9) (size 2.54 -2.54))
  (bus_entry (at 74.93 88.9) (size 2.54 -2.54))
  (bus_entry (at 72.39 88.9) (size 2.54 -2.54))
  (bus_entry (at 69.85 88.9) (size 2.54 -2.54))
  (bus_entry (at 59.69 88.9) (size 2.54 -2.54))
  (bus_entry (at 120.65 88.9) (size 2.54 -2.54))
  (bus_entry (at 96.52 107.95) (size 2.54 2.54))
  (bus_entry (at 53.34 173.99) (size 2.54 2.54))
  (bus_entry (at 100.33 88.9) (size 2.54 -2.54))
  (bus_entry (at 91.44 107.95) (size 2.54 2.54))
  (bus_entry (at 106.68 107.95) (size 2.54 2.54))
  (bus_entry (at 109.22 107.95) (size 2.54 2.54))
  (bus_entry (at 53.34 168.91) (size 2.54 2.54))
  (bus_entry (at 128.27 88.9) (size 2.54 -2.54))
  (bus_entry (at 101.6 228.6) (size 2.54 2.54))
  (bus_entry (at 104.14 228.6) (size 2.54 2.54))
  (bus_entry (at 106.68 228.6) (size 2.54 2.54))
  (bus_entry (at 109.22 228.6) (size 2.54 2.54))
  (bus_entry (at 99.06 228.6) (size 2.54 2.54))
  (bus_entry (at 91.44 228.6) (size 2.54 2.54))
  (bus_entry (at 93.98 228.6) (size 2.54 2.54))
  (bus_entry (at 96.52 228.6) (size 2.54 2.54))
  (bus_entry (at 99.06 107.95) (size 2.54 2.54))
  (bus_entry (at 53.34 146.05) (size 2.54 2.54))
  (bus_entry (at 114.3 107.95) (size 2.54 2.54))
  (bus_entry (at 116.84 107.95) (size 2.54 2.54))
  (bus_entry (at 119.38 107.95) (size 2.54 2.54))
  (bus_entry (at 146.05 88.9) (size 2.54 -2.54))
  (bus_entry (at 135.89 88.9) (size 2.54 -2.54))
  (bus_entry (at 154.94 140.97) (size 2.54 -2.54))
  (bus_entry (at 154.94 163.83) (size 2.54 -2.54))
  (bus_entry (at 154.94 161.29) (size 2.54 -2.54))
  (bus_entry (at 154.94 153.67) (size 2.54 -2.54))
  (bus_entry (at 154.94 151.13) (size 2.54 -2.54))
  (bus_entry (at 154.94 148.59) (size 2.54 -2.54))
  (bus_entry (at 154.94 146.05) (size 2.54 -2.54))
  (bus_entry (at 154.94 143.51) (size 2.54 -2.54))
  (bus_entry (at 154.94 171.45) (size 2.54 -2.54))
  (bus_entry (at 92.71 88.9) (size 2.54 -2.54))
  (bus_entry (at 53.34 148.59) (size 2.54 2.54))
  (bus_entry (at 105.41 88.9) (size 2.54 -2.54))
  (bus_entry (at 123.19 88.9) (size 2.54 -2.54))
  (bus_entry (at 121.92 209.55) (size 2.54 2.54))
  (bus_entry (at 124.46 209.55) (size 2.54 2.54))
  (bus_entry (at 53.34 143.51) (size 2.54 2.54))
  (bus_entry (at 111.76 107.95) (size 2.54 2.54))
  (bus_entry (at 107.95 88.9) (size 2.54 -2.54))
  (bus_entry (at 125.73 88.9) (size 2.54 -2.54))
  (bus_entry (at 93.98 107.95) (size 2.54 2.54))
  (bus_entry (at 53.34 151.13) (size 2.54 2.54))
  (bus_entry (at 96.52 209.55) (size 2.54 2.54))
  (bus_entry (at 99.06 209.55) (size 2.54 2.54))
  (bus_entry (at 101.6 209.55) (size 2.54 2.54))
  (bus_entry (at 104.14 209.55) (size 2.54 2.54))
  (bus_entry (at 154.94 176.53) (size 2.54 2.54))
  (bus_entry (at 154.94 179.07) (size 2.54 2.54))
  (bus_entry (at 82.55 88.9) (size 2.54 -2.54))
  (bus_entry (at 83.82 212.09) (size 2.54 -2.54))
  (bus_entry (at 86.36 212.09) (size 2.54 -2.54))
  (bus_entry (at 97.79 88.9) (size 2.54 -2.54))
  (bus_entry (at 53.34 171.45) (size 2.54 2.54))
  (bus_entry (at 88.9 107.95) (size 2.54 2.54))
  (bus_entry (at 53.34 163.83) (size 2.54 2.54))
  (bus_entry (at 102.87 88.9) (size 2.54 -2.54))
  (bus_entry (at 95.25 88.9) (size 2.54 -2.54))
  (bus_entry (at 90.17 88.9) (size 2.54 -2.54))
  (bus_entry (at 118.11 88.9) (size 2.54 -2.54))
  (bus_entry (at 115.57 88.9) (size 2.54 -2.54))
  (bus_entry (at 113.03 88.9) (size 2.54 -2.54))
  (wire (pts (xy 146.05 82.55) (xy 146.05 86.36)))
  (wire (pts (xy 143.51 82.55) (xy 143.51 86.36)))
  (bus (pts (xy 86.36 107.95) (xy 88.9 107.95)))
  (bus (pts (xy 53.34 151.13) (xy 53.34 156.21)))
  (wire (pts (xy 135.89 82.55) (xy 135.89 86.36)))
  (wire (pts (xy 60.96 265.43) (xy 60.96 267.97)))
  (wire (pts (xy 85.09 82.55) (xy 85.09 86.36)))
  (bus (pts (xy 99.06 107.95) (xy 106.68 107.95)))
  (wire (pts (xy 66.04 137.16) (xy 66.04 143.51)))
  (wire (pts (xy 104.14 125.73) (xy 104.14 118.11)))
  (wire (pts (xy 36.83 85.09) (xy 36.83 87.63)))
  (bus (pts (xy 92.71 88.9) (xy 90.17 88.9)))
  (bus (pts (xy 82.55 88.9) (xy 80.01 88.9)))
  (wire (pts (xy 77.47 82.55) (xy 77.47 86.36)))
  (wire (pts (xy 46.99 71.12) (xy 46.99 74.93)))
  (wire (pts (xy 104.14 194.31) (xy 104.14 209.55)))
  (bus (pts (xy 53.34 107.95) (xy 86.36 107.95)))
  (wire (pts (xy 123.19 82.55) (xy 123.19 86.36)))
  (wire (pts (xy 147.32 168.91) (xy 139.7 168.91)))
  (wire (pts (xy 86.36 125.73) (xy 86.36 123.19)))
  (wire (pts (xy 109.22 110.49) (xy 109.22 125.73)))
  (wire (pts (xy 43.18 173.99) (xy 45.72 173.99)))
  (bus (pts (xy 53.34 143.51) (xy 53.34 107.95)))
  (wire (pts (xy 90.17 82.55) (xy 90.17 86.36)))
  (wire (pts (xy 100.33 82.55) (xy 100.33 86.36)))
  (wire (pts (xy 91.44 110.49) (xy 91.44 125.73)))
  (wire (pts (xy 168.91 157.48) (xy 173.99 157.48)))
  (wire (pts (xy 115.57 82.55) (xy 115.57 86.36)))
  (bus (pts (xy 144.78 92.075) (xy 146.05 92.075)))
  (bus (pts (xy 99.06 107.95) (xy 96.52 107.95)))
  (bus (pts (xy 80.01 88.9) (xy 77.47 88.9)))
  (bus (pts (xy 53.34 156.21) (xy 53.34 163.83)))
  (bus (pts (xy 104.14 228.6) (xy 106.68 228.6)))
  (wire (pts (xy 22.86 199.39) (xy 27.94 199.39)))
  (bus (pts (xy 96.52 107.95) (xy 93.98 107.95)))
  (wire (pts (xy 68.58 132.08) (xy 64.77 132.08)))
  (wire (pts (xy 85.09 234.95) (xy 91.44 234.95)))
  (wire (pts (xy 102.87 82.55) (xy 102.87 86.36)))
  (bus (pts (xy 130.81 88.9) (xy 128.27 88.9)))
  (wire (pts (xy 64.77 134.62) (xy 68.58 134.62)))
  (bus (pts (xy 157.48 138.43) (xy 157.48 140.97)))
  (wire (pts (xy 68.58 140.97) (xy 68.58 134.62)))
  (bus (pts (xy 146.05 88.9) (xy 146.05 92.075)))
  (wire (pts (xy 130.81 82.55) (xy 130.81 86.36)))
  (wire (pts (xy 139.7 148.59) (xy 154.94 148.59)))
  (wire (pts (xy 105.41 82.55) (xy 105.41 86.36)))
  (wire (pts (xy 55.88 176.53) (xy 71.12 176.53)))
  (bus (pts (xy 119.38 107.95) (xy 121.92 107.95)))
  (wire (pts (xy 99.06 110.49) (xy 99.06 125.73)))
  (bus (pts (xy 83.82 212.09) (xy 86.36 212.09)))
  (wire (pts (xy 121.92 110.49) (xy 121.92 125.73)))
  (bus (pts (xy 99.06 228.6) (xy 101.6 228.6)))
  (wire (pts (xy 114.3 195.58) (xy 114.3 194.31)))
  (bus (pts (xy 102.87 88.9) (xy 100.33 88.9)))
  (wire (pts (xy 64.77 163.83) (xy 71.12 163.83)))
  (wire (pts (xy 107.95 82.55) (xy 107.95 86.36)))
  (wire (pts (xy 162.56 76.2) (xy 162.56 81.28)))
  (wire (pts (xy 139.7 153.67) (xy 154.94 153.67)))
  (wire (pts (xy 99.06 231.14) (xy 99.06 234.95)))
  (bus (pts (xy 97.79 88.9) (xy 95.25 88.9)))
  (wire (pts (xy 120.65 82.55) (xy 120.65 86.36)))
  (bus (pts (xy 107.95 88.9) (xy 105.41 88.9)))
  (wire (pts (xy 124.46 194.31) (xy 124.46 209.55)))
  (wire (pts (xy 16.51 199.39) (xy 22.86 199.39)))
  (wire (pts (xy 87.63 82.55) (xy 87.63 86.36)))
  (bus (pts (xy 53.34 148.59) (xy 53.34 146.05)))
  (bus (pts (xy 106.68 212.09) (xy 124.46 212.09)))
  (wire (pts (xy 55.88 146.05) (xy 71.12 146.05)))
  (wire (pts (xy 63.5 156.21) (xy 71.12 156.21)))
  (wire (pts (xy 64.77 137.16) (xy 66.04 137.16)))
  (bus (pts (xy 157.48 148.59) (xy 157.48 151.13)))
  (bus (pts (xy 118.11 88.9) (xy 115.57 88.9)))
  (wire (pts (xy 139.7 166.37) (xy 148.59 166.37)))
  (wire (pts (xy 96.52 110.49) (xy 96.52 125.73)))
  (wire (pts (xy 95.25 82.55) (xy 95.25 86.36)))
  (wire (pts (xy 33.02 147.32) (xy 33.02 154.94)))
  (bus (pts (xy 114.3 107.95) (xy 111.76 107.95)))
  (wire (pts (xy 97.79 82.55) (xy 97.79 86.36)))
  (wire (pts (xy 139.7 171.45) (xy 154.94 171.45)))
  (wire (pts (xy 147.32 173.99) (xy 139.7 173.99)))
  (wire (pts (xy 71.12 140.97) (xy 68.58 140.97)))
  (bus (pts (xy 64.77 88.9) (xy 62.23 88.9)))
  (bus (pts (xy 128.27 88.9) (xy 125.73 88.9)))
  (wire (pts (xy 111.76 195.58) (xy 111.76 194.31)))
  (wire (pts (xy 128.27 82.55) (xy 128.27 86.36)))
  (bus (pts (xy 101.6 228.6) (xy 104.14 228.6)))
  (wire (pts (xy 33.02 154.94) (xy 33.02 167.64)))
  (bus (pts (xy 157.48 179.07) (xy 157.48 181.61)))
  (bus (pts (xy 104.14 212.09) (xy 106.68 212.09)))
  (bus (pts (xy 157.48 107.95) (xy 157.48 138.43)))
  (wire (pts (xy 168.91 162.56) (xy 173.99 162.56)))
  (wire (pts (xy 119.38 194.31) (xy 119.38 201.93)))
  (wire (pts (xy 26.67 82.55) (xy 26.67 85.09)))
  (wire (pts (xy 104.14 231.14) (xy 104.14 234.95)))
  (bus (pts (xy 143.51 88.9) (xy 140.97 88.9)))
  (wire (pts (xy 96.52 231.14) (xy 96.52 234.95)))
  (wire (pts (xy 38.1 203.2) (xy 38.1 199.39)))
  (wire (pts (xy 38.1 199.39) (xy 35.56 199.39)))
  (bus (pts (xy 53.34 166.37) (xy 53.34 163.83)))
  (bus (pts (xy 121.92 107.95) (xy 157.48 107.95)))
  (wire (pts (xy 114.3 110.49) (xy 114.3 125.73)))
  (wire (pts (xy 139.7 179.07) (xy 154.94 179.07)))
  (wire (pts (xy 88.9 110.49) (xy 88.9 125.73)))
  (wire (pts (xy 55.88 148.59) (xy 71.12 148.59)))
  (wire (pts (xy 91.44 194.31) (xy 91.44 201.93)))
  (wire (pts (xy 64.77 161.29) (xy 71.12 161.29)))
  (bus (pts (xy 77.47 88.9) (xy 74.93 88.9)))
  (bus (pts (xy 93.98 107.95) (xy 91.44 107.95)))
  (bus (pts (xy 53.34 212.09) (xy 53.34 176.53)))
  (wire (pts (xy 113.03 82.55) (xy 113.03 86.36)))
  (bus (pts (xy 53.34 171.45) (xy 53.34 173.99)))
  (bus (pts (xy 124.46 212.09) (xy 127 212.09)))
  (wire (pts (xy 69.85 82.55) (xy 69.85 86.36)))
  (wire (pts (xy 67.31 82.55) (xy 67.31 86.36)))
  (wire (pts (xy 62.23 82.55) (xy 62.23 86.36)))
  (wire (pts (xy 101.6 110.49) (xy 101.6 125.73)))
  (bus (pts (xy 157.48 151.13) (xy 157.48 158.75)))
  (bus (pts (xy 93.98 228.6) (xy 96.52 228.6)))
  (bus (pts (xy 53.34 168.91) (xy 53.34 166.37)))
  (wire (pts (xy 139.7 140.97) (xy 154.94 140.97)))
  (bus (pts (xy 157.48 143.51) (xy 157.48 146.05)))
  (wire (pts (xy 109.22 195.58) (xy 109.22 194.31)))
  (bus (pts (xy 67.31 88.9) (xy 64.77 88.9)))
  (wire (pts (xy 116.84 194.31) (xy 116.84 201.93)))
  (bus (pts (xy 109.22 107.95) (xy 111.76 107.95)))
  (wire (pts (xy 36.83 71.12) (xy 36.83 72.39)))
  (wire (pts (xy 110.49 82.55) (xy 110.49 86.36)))
  (wire (pts (xy 16.51 71.12) (xy 16.51 74.93)))
  (bus (pts (xy 62.23 88.9) (xy 59.69 88.9)))
  (wire (pts (xy 86.36 123.19) (xy 68.58 123.19)))
  (bus (pts (xy 53.34 212.09) (xy 83.82 212.09)))
  (wire (pts (xy 93.98 194.31) (xy 93.98 201.93)))
  (bus (pts (xy 106.68 107.95) (xy 109.22 107.95)))
  (bus (pts (xy 53.34 173.99) (xy 53.34 176.53)))
  (wire (pts (xy 92.71 82.55) (xy 92.71 86.36)))
  (wire (pts (xy 139.7 161.29) (xy 154.94 161.29)))
  (bus (pts (xy 88.9 228.6) (xy 91.44 228.6)))
  (wire (pts (xy 125.73 82.55) (xy 125.73 86.36)))
  (bus (pts (xy 95.25 88.9) (xy 92.71 88.9)))
  (wire (pts (xy 43.18 167.64) (xy 45.72 167.64)))
  (wire (pts (xy 133.35 82.55) (xy 133.35 86.36)))
  (wire (pts (xy 140.97 82.55) (xy 140.97 86.36)))
  (wire (pts (xy 88.9 194.31) (xy 88.9 209.55)))
  (wire (pts (xy 33.02 167.64) (xy 33.02 173.99)))
  (bus (pts (xy 99.06 212.09) (xy 101.6 212.09)))
  (wire (pts (xy 36.83 85.09) (xy 46.99 85.09)))
  (wire (pts (xy 96.52 194.31) (xy 96.52 209.55)))
  (wire (pts (xy 55.88 179.07) (xy 71.12 179.07)))
  (wire (pts (xy 16.51 207.01) (xy 22.86 207.01)))
  (wire (pts (xy 111.76 110.49) (xy 111.76 125.73)))
  (wire (pts (xy 33.02 167.64) (xy 35.56 167.64)))
  (wire (pts (xy 86.36 194.31) (xy 86.36 209.55)))
  (wire (pts (xy 72.39 82.55) (xy 72.39 86.36)))
  (bus (pts (xy 90.17 88.9) (xy 87.63 88.9)))
  (wire (pts (xy 190.5 81.28) (xy 190.5 86.36)))
  (bus (pts (xy 123.19 88.9) (xy 120.65 88.9)))
  (wire (pts (xy 93.98 110.49) (xy 93.98 125.73)))
  (bus (pts (xy 91.44 228.6) (xy 93.98 228.6)))
  (wire (pts (xy 68.58 123.19) (xy 68.58 132.08)))
  (wire (pts (xy 101.6 194.31) (xy 101.6 209.55)))
  (wire (pts (xy 106.68 125.73) (xy 106.68 118.11)))
  (wire (pts (xy 50.8 265.43) (xy 50.8 267.97)))
  (bus (pts (xy 87.63 88.9) (xy 85.09 88.9)))
  (wire (pts (xy 33.02 173.99) (xy 35.56 173.99)))
  (wire (pts (xy 101.6 231.14) (xy 101.6 234.95)))
  (bus (pts (xy 157.48 161.29) (xy 157.48 168.91)))
  (wire (pts (xy 80.01 82.55) (xy 80.01 86.36)))
  (wire (pts (xy 106.68 195.58) (xy 106.68 194.31)))
  (wire (pts (xy 64.77 82.55) (xy 64.77 86.36)))
  (bus (pts (xy 69.85 88.9) (xy 67.31 88.9)))
  (wire (pts (xy 118.11 82.55) (xy 118.11 86.36)))
  (wire (pts (xy 46.99 82.55) (xy 46.99 85.09)))
  (wire (pts (xy 55.88 171.45) (xy 71.12 171.45)))
  (wire (pts (xy 106.68 231.14) (xy 106.68 234.95)))
  (bus (pts (xy 146.05 88.9) (xy 143.51 88.9)))
  (wire (pts (xy 38.1 207.01) (xy 38.1 203.2)))
  (bus (pts (xy 88.9 107.95) (xy 91.44 107.95)))
  (wire (pts (xy 71.12 143.51) (xy 66.04 143.51)))
  (bus (pts (xy 133.35 88.9) (xy 130.81 88.9)))
  (wire (pts (xy 16.51 86.36) (xy 16.51 82.55)))
  (wire (pts (xy 55.88 173.99) (xy 71.12 173.99)))
  (bus (pts (xy 72.39 88.9) (xy 69.85 88.9)))
  (bus (pts (xy 138.43 88.9) (xy 135.89 88.9)))
  (wire (pts (xy 36.83 80.01) (xy 36.83 85.09)))
  (wire (pts (xy 55.88 151.13) (xy 71.12 151.13)))
  (wire (pts (xy 55.88 153.67) (xy 71.12 153.67)))
  (bus (pts (xy 127 212.09) (xy 157.48 212.09)))
  (wire (pts (xy 85.09 238.76) (xy 85.09 234.95)))
  (wire (pts (xy 40.64 265.43) (xy 40.64 267.97)))
  (bus (pts (xy 157.48 181.61) (xy 157.48 212.09)))
  (wire (pts (xy 139.7 158.75) (xy 147.32 158.75)))
  (bus (pts (xy 53.34 151.13) (xy 53.34 148.59)))
  (wire (pts (xy 22.86 207.01) (xy 27.94 207.01)))
  (wire (pts (xy 162.56 81.28) (xy 165.1 81.28)))
  (bus (pts (xy 119.38 107.95) (xy 116.84 107.95)))
  (bus (pts (xy 113.03 88.9) (xy 110.49 88.9)))
  (wire (pts (xy 109.22 231.14) (xy 109.22 234.95)))
  (bus (pts (xy 157.48 158.75) (xy 157.48 161.29)))
  (wire (pts (xy 184.15 81.28) (xy 190.5 81.28)))
  (wire (pts (xy 139.7 163.83) (xy 154.94 163.83)))
  (wire (pts (xy 139.7 146.05) (xy 154.94 146.05)))
  (wire (pts (xy 26.67 85.09) (xy 36.83 85.09)))
  (bus (pts (xy 106.68 228.6) (xy 109.22 228.6)))
  (bus (pts (xy 140.97 88.9) (xy 138.43 88.9)))
  (wire (pts (xy 82.55 82.55) (xy 82.55 86.36)))
  (wire (pts (xy 45.72 173.99) (xy 45.72 181.61)))
  (wire (pts (xy 139.7 176.53) (xy 154.94 176.53)))
  (wire (pts (xy 119.38 110.49) (xy 119.38 125.73)))
  (bus (pts (xy 74.93 88.9) (xy 72.39 88.9)))
  (wire (pts (xy 55.88 166.37) (xy 71.12 166.37)))
  (wire (pts (xy 139.7 143.51) (xy 154.94 143.51)))
  (bus (pts (xy 101.6 212.09) (xy 104.14 212.09)))
  (bus (pts (xy 100.33 88.9) (xy 97.79 88.9)))
  (wire (pts (xy 99.06 194.31) (xy 99.06 209.55)))
  (wire (pts (xy 68.58 229.87) (xy 63.5 229.87)))
  (wire (pts (xy 17.78 250.19) (xy 20.32 250.19)))
  (bus (pts (xy 157.48 146.05) (xy 157.48 148.59)))
  (bus (pts (xy 116.84 107.95) (xy 114.3 107.95)))
  (bus (pts (xy 120.65 88.9) (xy 118.11 88.9)))
  (wire (pts (xy 38.1 203.2) (xy 40.64 203.2)))
  (wire (pts (xy 74.93 82.55) (xy 74.93 86.36)))
  (bus (pts (xy 105.41 88.9) (xy 102.87 88.9)))
  (wire (pts (xy 45.72 154.94) (xy 45.72 167.64)))
  (bus (pts (xy 135.89 88.9) (xy 133.35 88.9)))
  (wire (pts (xy 111.76 231.14) (xy 111.76 234.95)))
  (wire (pts (xy 55.88 168.91) (xy 71.12 168.91)))
  (bus (pts (xy 85.09 88.9) (xy 82.55 88.9)))
  (bus (pts (xy 110.49 88.9) (xy 107.95 88.9)))
  (bus (pts (xy 157.48 168.91) (xy 157.48 171.45)))
  (wire (pts (xy 172.72 81.28) (xy 176.53 81.28)))
  (wire (pts (xy 138.43 82.55) (xy 138.43 86.36)))
  (wire (pts (xy 35.56 207.01) (xy 38.1 207.01)))
  (wire (pts (xy 116.84 110.49) (xy 116.84 125.73)))
  (wire (pts (xy 124.46 110.49) (xy 124.46 125.73)))
  (wire (pts (xy 147.32 156.21) (xy 139.7 156.21)))
  (bus (pts (xy 96.52 228.6) (xy 99.06 228.6)))
  (bus (pts (xy 157.48 140.97) (xy 157.48 143.51)))
  (wire (pts (xy 121.92 194.31) (xy 121.92 209.55)))
  (bus (pts (xy 53.34 171.45) (xy 53.34 168.91)))
  (wire (pts (xy 55.88 158.75) (xy 71.12 158.75)))
  (wire (pts (xy 26.67 71.12) (xy 26.67 74.93)))
  (wire (pts (xy 148.59 82.55) (xy 148.59 86.36)))
  (wire (pts (xy 45.72 167.64) (xy 45.72 173.99)))
  (wire (pts (xy 139.7 151.13) (xy 154.94 151.13)))
  (bus (pts (xy 115.57 88.9) (xy 113.03 88.9)))
  (bus (pts (xy 53.34 146.05) (xy 53.34 143.51)))
  (wire (pts (xy 93.98 231.14) (xy 93.98 234.95)))
  (bus (pts (xy 125.73 88.9) (xy 123.19 88.9)))
  (rectangle (start 8.89 62.23) (end 55.88 93.98)
    (fill (type none))
  )
  (rectangle (start 161.29 143.51) (end 187.96 168.91)
    (fill (type none))
  )
  (rectangle (start 29.21 133.35) (end 49.53 187.96)
    (fill (type none))
  )
  (rectangle (start 36.83 251.46) (end 64.77 283.21)
    (fill (type none))
  )
  (rectangle (start 7.62 189.23) (end 49.53 210.82)
    (fill (type none))
  )
  (rectangle (start 81.28 215.9) (end 115.57 250.19)
    (fill (type none))
  )
  (rectangle (start 53.34 215.9) (end 76.2 237.49)
    (fill (type none))
  )
  (rectangle (start 50.8 96.52) (end 160.02 214.63)
    (fill (type none))
  )
  (rectangle (start 58.42 62.23) (end 152.4 93.98)
    (fill (type none))
  )
  (rectangle (start 153.67 62.23) (end 200.66 93.98)
    (fill (type none))
  )
  (text_box "Debug - RC4: UART (RTCC, TMR0, PWM)"
    (at 55.88 245.11 0) (size -40.64 -3.81)
    (fill (type none))
  )
  (text_box "Adj  - RB7: ICSP_DAT\nMode - RB6: ICSP_CLK\nReset - RG5: ICSP_MCLR\n"
    (at 36.83 275.59 0) (size 27.94 7.62)
    (fill (type none))
  )
  (text "DAT" (at 39.37 260.35 0))
  (text "RTC XTAL" (at 16.51 195.58 0))
  (text "Keypad" (at 91.44 222.25 0))
  (text "LCD" (at 71.12 68.58 0))
  (text "Memory -  Flash / RAM\n\n  19195 - 14KB / 1KB\n  19196 - 28KB / 2KB\n  19197 - 56KB / 4KB"
    (at 129.54 124.46 0)
  )
  (text "Power PIC" (at 36.83 48.26 0))
  (text "Buzzer" (at 54.61 222.25 0))
  (text "LCD Backlight" (at 156.21 68.58 0))
  (text "Buttons" (at 163.83 149.86 0))
  (text "(x2) ${0f8e14ae-a999-4c89-a12e-58f0c4205c7e:VALUE}"
    (at 34.29 179.07 0)
  )
  (text "CLK" (at 49.53 260.35 0))
  (text "Charge Pump" (at 12.7 68.58 0))
  (text "ICSP" (at 38.1 256.54 0))
  (text "~{RST}" (at 59.69 260.35 0))
  (text "Note:\nVLCD2 is only needed\nfor 5V LCD mode" (at 13.97 92.71 0))
  (text "PIC Microcontroller" (at 55.88 104.14 0))
  (text "Power" (at 30.48 139.7 0))
  (label "COM1" (at 91.44 119.38 90) (fields_autoplaced))
  (label "ROW1" (at 99.06 231.14 90) (fields_autoplaced))
  (label "SEG22" (at 121.92 119.38 90) (fields_autoplaced))
  (label "SEG25" (at 135.89 86.36 90) (fields_autoplaced))
  (label "SEG8" (at 92.71 86.36 90) (fields_autoplaced))
  (label "COM2" (at 67.31 86.36 90) (fields_autoplaced))
  (label "SEG22" (at 128.27 86.36 90) (fields_autoplaced))
  (label "SEG3" (at 64.77 166.37 0) (fields_autoplaced))
  (label "SEG20" (at 116.84 119.38 90) (fields_autoplaced))
  (label "COL3" (at 146.05 176.53 0) (fields_autoplaced))
  (label "VLCD1" (at 26.67 71.12 90) (fields_autoplaced))
  (label "SEG10" (at 64.77 176.53 0) (fields_autoplaced))
  (label "COM1" (at 64.77 86.36 90) (fields_autoplaced))
  (label "SEG27" (at 147.32 148.59 0) (fields_autoplaced))
  (label "SEG15" (at 99.06 119.38 90) (fields_autoplaced))
  (label "KEY_BUS" (at 138.43 212.09 0) (fields_autoplaced))
  (label "SEG14" (at 107.95 86.36 90) (fields_autoplaced))
  (label "SEG5" (at 64.77 153.67 0) (fields_autoplaced))
  (label "SEG24" (at 147.32 140.97 0) (fields_autoplaced))
  (label "VLCD3" (at 46.99 71.12 90) (fields_autoplaced))
  (label "COL1" (at 106.68 231.14 90) (fields_autoplaced))
  (label "SEG12" (at 88.9 200.66 90) (fields_autoplaced))
  (label "LCD_BUS" (at 144.78 92.075 0) (fields_autoplaced))
  (label "COL2" (at 109.22 231.14 90) (fields_autoplaced))
  (label "SEG29" (at 146.05 86.36 90) (fields_autoplaced))
  (label "CFLY2" (at 16.51 86.36 90) (fields_autoplaced))
  (label "COM0" (at 88.9 119.38 90) (fields_autoplaced))
  (label "COM3" (at 96.52 119.38 90) (fields_autoplaced))
  (label "COL0" (at 121.92 200.66 90) (fields_autoplaced))
  (label "SEG23" (at 130.81 86.36 90) (fields_autoplaced))
  (label "SEG12" (at 102.87 86.36 90) (fields_autoplaced))
  (label "SEG24" (at 133.35 86.36 90) (fields_autoplaced))
  (label "SEG13" (at 105.41 86.36 90) (fields_autoplaced))
  (label "SEG0" (at 64.77 173.99 0) (fields_autoplaced))
  (label "COM0" (at 62.23 86.36 90) (fields_autoplaced))
  (label "SEG6" (at 64.77 151.13 0) (fields_autoplaced))
  (label "SEG26" (at 138.43 86.36 90) (fields_autoplaced))
  (label "SEG1" (at 64.77 171.45 0) (fields_autoplaced))
  (label "COL3" (at 111.76 231.14 90) (fields_autoplaced))
  (label "SEG16" (at 113.03 86.36 90) (fields_autoplaced))
  (label "COL1" (at 124.46 200.66 90) (fields_autoplaced))
  (label "SEG1" (at 74.93 86.36 90) (fields_autoplaced))
  (label "SEG7" (at 90.17 86.36 90) (fields_autoplaced))
  (label "SEG4" (at 64.77 158.75 0) (fields_autoplaced))
  (label "COL0" (at 104.14 231.14 90) (fields_autoplaced))
  (label "SEG25" (at 147.32 143.51 0) (fields_autoplaced))
  (label "SEG18" (at 118.11 86.36 90) (fields_autoplaced))
  (label "SEG27" (at 140.97 86.36 90) (fields_autoplaced))
  (label "SEG15" (at 110.49 86.36 90) (fields_autoplaced))
  (label "ROW2" (at 99.06 200.66 90) (fields_autoplaced))
  (label "SEG2" (at 64.77 168.91 0) (fields_autoplaced))
  (label "SEG5" (at 85.09 86.36 90) (fields_autoplaced))
  (label "SEG19" (at 114.3 119.38 90) (fields_autoplaced))
  (label "ROW0" (at 104.14 200.66 90) (fields_autoplaced))
  (label "ROW3" (at 96.52 200.66 90) (fields_autoplaced))
  (label "KEY_BUS" (at 89.535 228.6 0) (fields_autoplaced))
  (label "SEG23" (at 124.46 119.38 90) (fields_autoplaced))
  (label "SEG16" (at 101.6 119.38 90) (fields_autoplaced))
  (label "SEG3" (at 80.01 86.36 90) (fields_autoplaced))
  (label "SEG29" (at 147.32 153.67 0) (fields_autoplaced))
  (label "ROW1" (at 101.6 200.66 90) (fields_autoplaced))
  (label "SEG11" (at 64.77 179.07 0) (fields_autoplaced))
  (label "SEG8" (at 64.77 146.05 0) (fields_autoplaced))
  (label "SEG9" (at 86.36 200.66 90) (fields_autoplaced))
  (label "SEG20" (at 123.19 86.36 90) (fields_autoplaced))
  (label "SEG21" (at 119.38 119.38 90) (fields_autoplaced))
  (label "ROW3" (at 93.98 231.14 90) (fields_autoplaced))
  (label "SEG30" (at 146.05 171.45 0) (fields_autoplaced))
  (label "COL2" (at 146.05 179.07 0) (fields_autoplaced))
  (label "ROW2" (at 96.52 231.14 90) (fields_autoplaced))
  (label "COM2" (at 93.98 119.38 90) (fields_autoplaced))
  (label "SEG9" (at 95.25 86.36 90) (fields_autoplaced))
  (label "LCD_BUS" (at 53.34 109.22 90) (fields_autoplaced))
  (label "ROW0" (at 101.6 231.14 90) (fields_autoplaced))
  (label "SEG14" (at 147.32 161.29 0) (fields_autoplaced))
  (label "SEG17" (at 115.57 86.36 90) (fields_autoplaced))
  (label "SEG7" (at 64.77 148.59 0) (fields_autoplaced))
  (label "SEG28" (at 143.51 86.36 90) (fields_autoplaced))
  (label "SEG26" (at 147.32 146.05 0) (fields_autoplaced))
  (label "SEG2" (at 77.47 86.36 90) (fields_autoplaced))
  (label "CFLY1" (at 16.51 71.12 90) (fields_autoplaced))
  (label "SEG30" (at 148.59 86.36 90) (fields_autoplaced))
  (label "SEG6" (at 87.63 86.36 90) (fields_autoplaced))
  (label "SEG19" (at 120.65 86.36 90) (fields_autoplaced))
  (label "SEG17" (at 109.22 119.38 90) (fields_autoplaced))
  (label "VLCD2" (at 36.83 71.12 0) (fields_autoplaced))
  (label "SEG18" (at 111.76 119.38 90) (fields_autoplaced))
  (label "SEG11" (at 100.33 86.36 90) (fields_autoplaced))
  (label "SEG28" (at 147.32 151.13 0) (fields_autoplaced))
  (label "SEG10" (at 97.79 86.36 90) (fields_autoplaced))
  (label "COM3" (at 69.85 86.36 90) (fields_autoplaced))
  (label "SEG0" (at 72.39 86.36 90) (fields_autoplaced))
  (label "SEG21" (at 125.73 86.36 90) (fields_autoplaced))
  (label "SEG4" (at 82.55 86.36 90) (fields_autoplaced))
  (label "SEG13" (at 147.32 163.83 0) (fields_autoplaced))
  (hierarchical_label "SOSCI" (shape input) (at 116.84 201.93 270) (fields_autoplaced))
  (hierarchical_label "VLCD3" (shape input) (at 64.77 132.08 180) (fields_autoplaced))
  (hierarchical_label "SOSCI" (shape input) (at 16.51 207.01 180) (fields_autoplaced))
  (hierarchical_label "BUZZ" (shape input) (at 93.98 201.93 270) (fields_autoplaced))
  (hierarchical_label "VLCD1" (shape input) (at 64.77 137.16 180) (fields_autoplaced))
  (hierarchical_label "MODE" (shape input) (at 50.8 267.97 270) (fields_autoplaced))
  (hierarchical_label "CFLY2" (shape input) (at 106.68 118.11 90) (fields_autoplaced))
  (hierarchical_label "SOSCO" (shape input) (at 16.51 199.39 180) (fields_autoplaced))
  (hierarchical_label "CFLY1" (shape input) (at 104.14 118.11 90) (fields_autoplaced))
  (hierarchical_label "SOSCO" (shape input) (at 119.38 201.93 270) (fields_autoplaced))
  (hierarchical_label "DEBUG" (shape input) (at 20.32 250.19 0) (fields_autoplaced))
  (hierarchical_label "VLCD2" (shape input) (at 64.77 134.62 180) (fields_autoplaced))
  (hierarchical_label "LIGHT" (shape input) (at 162.56 76.2 90) (fields_autoplaced))
  (hierarchical_label "ADJ" (shape input) (at 40.64 267.97 270) (fields_autoplaced))
  (hierarchical_label "MODE" (shape input) (at 147.32 156.21 0) (fields_autoplaced))
  (hierarchical_label "~{MCLR}" (shape input) (at 60.96 267.97 270) (fields_autoplaced))
  (hierarchical_label "DEBUG" (shape input) (at 147.32 173.99 0) (fields_autoplaced))
  (hierarchical_label "~{MCLR}" (shape input) (at 63.5 156.21 180) (fields_autoplaced))
  (hierarchical_label "ADJ" (shape input) (at 168.91 162.56 180) (fields_autoplaced))
  (hierarchical_label "LIGHT" (shape input) (at 91.44 201.93 270) (fields_autoplaced))
  (hierarchical_label "ADJ" (shape input) (at 147.32 168.91 0) (fields_autoplaced))
  (hierarchical_label "BUZZ" (shape input) (at 68.58 229.87 0) (fields_autoplaced))
  (hierarchical_label "MODE" (shape input) (at 168.91 157.48 180) (fields_autoplaced))
  (symbol (lib_id "Device:C") (at 46.99 78.74 0) (unit 1)
    (in_bom yes) (on_board yes)
    (default_instance (reference "U") (unit 1) (value "") (footprint ""))
    (property "Reference" "U" (id 0) (at 48.26 76.2 0))
    (property "Value" "" (id 1) (at 48.26 81.28 0))
    (property "Footprint" "" (id 2) (at 47.9552 82.55 0))
    (property "Datasheet" "~" (id 3) (at 46.99 78.74 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 39.37 173.99 270) (unit 1)
    (in_bom yes) (on_board yes)
    (default_instance (reference "U") (unit 1) (value "") (footprint ""))
    (property "Reference" "U" (id 0) (at 34.29 172.72 90))
    (property "Value" "" (id 1) (at 46.99 175.26 90))
    (property "Footprint" "" (id 2) (at 35.56 174.9552 0))
    (property "Datasheet" "~" (id 3) (at 39.37 173.99 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 31.75 199.39 90) (unit 1)
    (in_bom yes) (on_board yes)
    (default_instance (reference "C") (unit 1) (value "C") (footprint ""))
    (property "Reference" "C" (id 0) (at 29.21 198.12 90))
    (property "Value" "C" (id 1) (at 33.655 195.58 0))
    (property "Footprint" "" (id 2) (at 35.56 198.4248 0))
    (property "Datasheet" "~" (id 3) (at 31.75 199.39 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 190.5 86.36 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (default_instance (reference "#PWR") (unit 1) (value "GND") (footprint ""))
    (property "Reference" "#PWR" (id 0) (at 190.5 92.71 0))
    (property "Value" "GND" (id 1) (at 190.5 90.17 0))
    (property "Footprint" "" (id 2) (at 190.5 86.36 0))
    (property "Datasheet" "" (id 3) (at 190.5 86.36 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 147.32 158.75 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (default_instance (reference "U") (unit 1) (value "") (footprint ""))
    (property "Reference" "U" (id 0) (at 153.67 158.75 0))
    (property "Value" "" (id 1) (at 151.13 158.75 90))
    (property "Footprint" "" (id 2) (at 147.32 158.75 0))
    (property "Datasheet" "" (id 3) (at 147.32 158.75 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 168.91 81.28 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (default_instance (reference "R") (unit 1) (value "R") (footprint ""))
    (property "Reference" "R" (id 0) (at 168.91 78.74 90))
    (property "Value" "R" (id 1) (at 168.91 80.01 90))
    (property "Footprint" "" (id 2) (at 168.91 83.058 90))
    (property "Datasheet" "~" (id 3) (at 168.91 81.28 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "powerpic:ppc-board") (at 177.8 160.02 0) (unit 1)
    (in_bom yes) (on_board yes)
    (default_instance (reference "U") (unit 1) (value "") (footprint ""))
    (property "Reference" "U" (id 0) (at 175.26 153.67 0))
    (property "Value" "" (id 1) (at 175.26 166.37 0))
    (property "Footprint" "" (id 2) (at 177.8 160.02 0))
    (property "Datasheet" "" (id 3) (at 178.181 160.02 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "33")
    (pin "34")
    (pin "35")
    (pin "36")
    (pin "37")
    (pin "38")
    (pin "39")
    (pin "40")
    (pin "41")
    (pin "42")
    (pin "43")
    (pin "44")
    (pin "45")
    (pin "46")
    (pin "47")
    (pin "48")
    (pin "49")
  )
  (symbol (lib_id "power:VCC") (at 148.59 166.37 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (default_instance (reference "U") (unit 1) (value "") (footprint ""))
    (property "Reference" "U" (id 0) (at 144.78 166.37 0))
    (property "Value" "" (id 1) (at 152.4 166.37 90))
    (property "Footprint" "" (id 2) (at 148.59 166.37 0))
    (property "Datasheet" "" (id 3) (at 148.59 166.37 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 36.83 87.63 0) (unit 1)
    (in_bom yes) (on_board yes)
    (default_instance (reference "U") (unit 1) (value "") (footprint ""))
    (property "Reference" "U" (id 0) (at 36.83 93.98 0))
    (property "Value" "" (id 1) (at 36.83 91.44 0))
    (property "Footprint" "" (id 2) (at 36.83 87.63 0))
    (property "Datasheet" "" (id 3) (at 36.83 87.63 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 31.75 207.01 90) (unit 1)
    (in_bom yes) (on_board yes)
    (default_instance (reference "C") (unit 1) (value "C") (footprint ""))
    (property "Reference" "C" (id 0) (at 29.21 205.74 90))
    (property "Value" "C" (id 1) (at 33.655 203.2 0))
    (property "Footprint" "" (id 2) (at 35.56 206.0448 0))
    (property "Datasheet" "~" (id 3) (at 31.75 207.01 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 45.72 181.61 0) (unit 1)
    (in_bom yes) (on_board yes)
    (default_instance (reference "U") (unit 1) (value "") (footprint ""))
    (property "Reference" "U" (id 0) (at 45.72 187.96 0))
    (property "Value" "" (id 1) (at 45.72 185.42 0))
    (property "Footprint" "" (id 2) (at 45.72 181.61 0))
    (property "Datasheet" "" (id 3) (at 45.72 181.61 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 16.51 78.74 0) (unit 1)
    (in_bom yes) (on_board yes)
    (default_instance (reference "U") (unit 1) (value "") (footprint ""))
    (property "Reference" "U" (id 0) (at 17.78 76.2 0))
    (property "Value" "" (id 1) (at 17.78 81.28 0))
    (property "Footprint" "" (id 2) (at 17.4752 82.55 0))
    (property "Datasheet" "~" (id 3) (at 16.51 78.74 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 40.64 203.2 90) (unit 1)
    (in_bom yes) (on_board yes)
    (default_instance (reference "#PWR") (unit 1) (value "GND") (footprint ""))
    (property "Reference" "#PWR" (id 0) (at 46.99 203.2 0))
    (property "Value" "GND" (id 1) (at 44.45 203.2 90))
    (property "Footprint" "" (id 2) (at 40.64 203.2 0))
    (property "Datasheet" "" (id 3) (at 40.64 203.2 0))
    (pin "1")
  )
  (symbol (lib_id "powerpic:PIC16F1919x-xMR") (at 105.41 160.02 0) (unit 1)
    (in_bom yes) (on_board yes)
    (default_instance (reference "U") (unit 1) (value "") (footprint ""))
    (property "Reference" "U" (id 0) (at 105.41 160.02 0))
    (property "Value" "" (id 1) (at 105.41 165.1 0))
    (property "Footprint" "" (id 2) (at 105.41 160.02 0))
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF19195-6-7-Data-Sheet-40001873D.pdf" (id 3) (at 105.41 160.02 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "33")
    (pin "34")
    (pin "35")
    (pin "36")
    (pin "37")
    (pin "38")
    (pin "39")
    (pin "4")
    (pin "40")
    (pin "41")
    (pin "42")
    (pin "43")
    (pin "44")
    (pin "45")
    (pin "46")
    (pin "47")
    (pin "48")
    (pin "49")
    (pin "5")
    (pin "50")
    (pin "51")
    (pin "52")
    (pin "53")
    (pin "54")
    (pin "55")
    (pin "56")
    (pin "57")
    (pin "58")
    (pin "59")
    (pin "6")
    (pin "60")
    (pin "61")
    (pin "62")
    (pin "63")
    (pin "64")
    (pin "65")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "power:VCC") (at 33.02 147.32 0) (unit 1)
    (in_bom yes) (on_board yes)
    (default_instance (reference "U") (unit 1) (value "") (footprint ""))
    (property "Reference" "U" (id 0) (at 33.02 151.13 0))
    (property "Value" "" (id 1) (at 33.02 143.51 0))
    (property "Footprint" "" (id 2) (at 33.02 147.32 0))
    (property "Datasheet" "" (id 3) (at 33.02 147.32 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 64.77 161.29 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (default_instance (reference "U") (unit 1) (value "") (footprint ""))
    (property "Reference" "U" (id 0) (at 58.42 161.29 0))
    (property "Value" "" (id 1) (at 60.96 161.29 90))
    (property "Footprint" "" (id 2) (at 64.77 161.29 0))
    (property "Datasheet" "" (id 3) (at 64.77 161.29 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 36.83 76.2 0) (unit 1)
    (in_bom yes) (on_board yes)
    (default_instance (reference "U") (unit 1) (value "") (footprint ""))
    (property "Reference" "U" (id 0) (at 38.1 73.66 0))
    (property "Value" "" (id 1) (at 38.1 78.74 0))
    (property "Footprint" "" (id 2) (at 37.7952 80.01 0))
    (property "Datasheet" "~" (id 3) (at 36.83 76.2 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "powerpic:ppc-board") (at 104.14 76.2 90) (unit 1)
    (in_bom yes) (on_board yes)
    (default_instance (reference "U") (unit 1) (value "") (footprint ""))
    (property "Reference" "U" (id 0) (at 59.69 68.58 90))
    (property "Value" "" (id 1) (at 151.13 68.58 90))
    (property "Footprint" "" (id 2) (at 104.14 76.2 0))
    (property "Datasheet" "" (id 3) (at 104.14 75.819 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "33")
    (pin "34")
    (pin "35")
    (pin "36")
    (pin "37")
    (pin "38")
    (pin "39")
    (pin "40")
    (pin "41")
    (pin "42")
    (pin "43")
    (pin "44")
    (pin "45")
    (pin "46")
    (pin "47")
    (pin "48")
    (pin "49")
  )
  (symbol (lib_id "Connector:TestPoint") (at 60.96 265.43 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (default_instance (reference "TP") (unit 1) (value "TestPoint") (footprint ""))
    (property "Reference" "TP" (id 0) (at 63.5 261.493 0))
    (property "Value" "TestPoint" (id 1) (at 63.5 264.033 0))
    (property "Footprint" "" (id 2) (at 66.04 265.43 0))
    (property "Datasheet" "~" (id 3) (at 66.04 265.43 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint") (at 17.78 250.19 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (default_instance (reference "TP") (unit 1) (value "TestPoint") (footprint ""))
    (property "Reference" "TP" (id 0) (at 13.843 252.73 0))
    (property "Value" "TestPoint" (id 1) (at 16.383 252.73 0))
    (property "Footprint" "" (id 2) (at 17.78 255.27 0))
    (property "Datasheet" "~" (id 3) (at 17.78 255.27 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint") (at 40.64 265.43 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (default_instance (reference "TP") (unit 1) (value "TestPoint") (footprint ""))
    (property "Reference" "TP" (id 0) (at 43.18 261.493 0))
    (property "Value" "TestPoint" (id 1) (at 43.18 264.033 0))
    (property "Footprint" "" (id 2) (at 45.72 265.43 0))
    (property "Datasheet" "~" (id 3) (at 45.72 265.43 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 26.67 78.74 0) (unit 1)
    (in_bom yes) (on_board yes)
    (default_instance (reference "U") (unit 1) (value "") (footprint ""))
    (property "Reference" "U" (id 0) (at 27.94 76.2 0))
    (property "Value" "" (id 1) (at 27.94 81.28 0))
    (property "Footprint" "" (id 2) (at 27.6352 82.55 0))
    (property "Datasheet" "~" (id 3) (at 26.67 78.74 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint") (at 50.8 265.43 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (default_instance (reference "TP") (unit 1) (value "TestPoint") (footprint ""))
    (property "Reference" "TP" (id 0) (at 53.34 261.493 0))
    (property "Value" "TestPoint" (id 1) (at 53.34 264.033 0))
    (property "Footprint" "" (id 2) (at 55.88 265.43 0))
    (property "Datasheet" "~" (id 3) (at 55.88 265.43 0))
    (pin "1")
  )
  (symbol (lib_id "power:VCC") (at 64.77 163.83 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (default_instance (reference "U") (unit 1) (value "") (footprint ""))
    (property "Reference" "U" (id 0) (at 68.58 163.83 0))
    (property "Value" "" (id 1) (at 60.96 163.83 90))
    (property "Footprint" "" (id 2) (at 64.77 163.83 0))
    (property "Datasheet" "" (id 3) (at 64.77 163.83 0))
    (pin "1")
  )
  (symbol (lib_id "powerpic:ppc-board") (at 101.6 241.3 90) (unit 1)
    (in_bom yes) (on_board yes)
    (default_instance (reference "U") (unit 1) (value "") (footprint ""))
    (property "Reference" "U" (id 0) (at 88.9 247.65 90))
    (property "Value" "" (id 1) (at 114.3 247.65 90))
    (property "Footprint" "" (id 2) (at 101.6 241.3 0))
    (property "Datasheet" "" (id 3) (at 101.6 240.919 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "33")
    (pin "34")
    (pin "35")
    (pin "36")
    (pin "37")
    (pin "38")
    (pin "39")
    (pin "40")
    (pin "41")
    (pin "42")
    (pin "43")
    (pin "44")
    (pin "45")
    (pin "46")
    (pin "47")
    (pin "48")
    (pin "49")
  )
  (symbol (lib_id "Device:C") (at 39.37 167.64 270) (unit 1)
    (in_bom yes) (on_board yes)
    (default_instance (reference "U") (unit 1) (value "") (footprint ""))
    (property "Reference" "U" (id 0) (at 34.29 166.37 90))
    (property "Value" "" (id 1) (at 46.99 168.91 90))
    (property "Footprint" "" (id 2) (at 35.56 168.6052 0))
    (property "Datasheet" "~" (id 3) (at 39.37 167.64 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:LED") (at 180.34 81.28 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (default_instance (reference "D") (unit 1) (value "LED") (footprint ""))
    (property "Reference" "D" (id 0) (at 181.61 78.74 0))
    (property "Value" "LED" (id 1) (at 181.61 85.09 0))
    (property "Footprint" "" (id 2) (at 180.34 81.28 0))
    (property "Datasheet" "~" (id 3) (at 180.34 81.28 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "powerpic:ppc-board") (at 39.37 154.94 0) (unit 1)
    (in_bom yes) (on_board yes)
    (default_instance (reference "U") (unit 1) (value "") (footprint ""))
    (property "Reference" "U" (id 0) (at 39.37 148.59 0))
    (property "Value" "" (id 1) (at 39.37 161.29 0))
    (property "Footprint" "" (id 2) (at 39.37 154.94 0))
    (property "Datasheet" "" (id 3) (at 39.751 154.94 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "33")
    (pin "34")
    (pin "35")
    (pin "36")
    (pin "37")
    (pin "38")
    (pin "39")
    (pin "40")
    (pin "41")
    (pin "42")
    (pin "43")
    (pin "44")
    (pin "45")
    (pin "46")
    (pin "47")
    (pin "48")
    (pin "49")
  )
  (symbol (lib_id "powerpic:ppc-board") (at 59.69 229.87 0) (unit 1)
    (in_bom yes) (on_board yes)
    (default_instance (reference "U") (unit 1) (value "") (footprint ""))
    (property "Reference" "U" (id 0) (at 55.88 226.06 0))
    (property "Value" "" (id 1) (at 55.88 233.68 0))
    (property "Footprint" "" (id 2) (at 59.69 229.87 0))
    (property "Datasheet" "" (id 3) (at 60.071 229.87 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "33")
    (pin "34")
    (pin "35")
    (pin "36")
    (pin "37")
    (pin "38")
    (pin "39")
    (pin "40")
    (pin "41")
    (pin "42")
    (pin "43")
    (pin "44")
    (pin "45")
    (pin "46")
    (pin "47")
    (pin "48")
    (pin "49")
  )
  (symbol (lib_id "Device:Crystal") (at 22.86 203.2 90) (unit 1)
    (in_bom yes) (on_board yes)
    (default_instance (reference "Y") (unit 1) (value "Crystal") (footprint ""))
    (property "Reference" "Y" (id 0) (at 19.05 203.2 90))
    (property "Value" "Crystal" (id 1) (at 22.86 208.28 90))
    (property "Footprint" "" (id 2) (at 22.86 203.2 0))
    (property "Datasheet" "~" (id 3) (at 22.86 203.2 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 85.09 238.76 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (default_instance (reference "#PWR") (unit 1) (value "GND") (footprint ""))
    (property "Reference" "#PWR" (id 0) (at 85.09 245.11 0))
    (property "Value" "GND" (id 1) (at 85.09 243.84 0))
    (property "Footprint" "" (id 2) (at 85.09 238.76 0))
    (property "Datasheet" "" (id 3) (at 85.09 238.76 0))
    (pin "1")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#PWR01") (unit 1) (value "VCC") (footprint "")
    )
    (path
      (reference "#PWR02") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR03") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR04") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR05") (unit 1) (value "VCC") (footprint "")
    )
    (path
      (reference "#PWR0102") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0103") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0104") (unit 1) (value "VCC") (footprint "")
    )
    (path
      (reference "#PWR0106") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "C1") (unit 1) (value "0.1μF") (footprint "Capacitor_SMD:C_0402_1005Metric")
    )
    (path
      (reference "C2") (unit 1) (value "0.1μF") (footprint "Capacitor_SMD:C_0402_1005Metric")
    )
    (path
      (reference "C3") (unit 1) (value "TBD") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C4") (unit 1) (value "TBD") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C5") (unit 1) (value "0.27μF") (footprint "Capacitor_SMD:C_0402_1005Metric")
    )
    (path
      (reference "C6") (unit 1) (value "0.27μF") (footprint "Capacitor_SMD:C_0402_1005Metric")
    )
    (path
      (reference "C7") (unit 1) (value "0.27μF") (footprint "Capacitor_SMD:C_0402_1005Metric")
    )
    (path
      (reference "C8") (unit 1) (value "1μF") (footprint "Capacitor_SMD:C_0402_1005Metric")
    )
    (path
      (reference "D1") (unit 1) (value "LCD_LED") (footprint "LED_SMD:LED_0402_1005Metric")
    )
    (path
      (reference "PPC1") (unit 1) (value "ppc-board") (footprint "powerpic:ppc-board")
    )
    (path
      (reference "PPC1") (unit 2) (value "ppc-board") (footprint "powerpic:ppc-board")
    )
    (path
      (reference "PPC1") (unit 3) (value "ppc-board") (footprint "powerpic:ppc-board")
    )
    (path
      (reference "PPC1") (unit 4) (value "ppc-board") (footprint "powerpic:ppc-board")
    )
    (path
      (reference "PPC1") (unit 5) (value "ppc-board") (footprint "powerpic:ppc-board")
    )
    (path
      (reference "R1") (unit 1) (value "TBD") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "TP1") (unit 1) (value "~{MCLR}") (footprint "powerpic:Progo_Pad_D2.0mm")
    )
    (path
      (reference "TP2") (unit 1) (value "Mode") (footprint "powerpic:Progo_Pad_D2.0mm")
    )
    (path
      (reference "TP3") (unit 1) (value "Adj") (footprint "powerpic:Progo_Pad_D2.0mm")
    )
    (path
      (reference "TP4") (unit 1) (value "Debug") (footprint "powerpic:Progo_Pad_D2.0mm")
    )
    (path
      (reference "U1") (unit 1) (value "PIC16LF1919x-I/MR") (footprint "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm")
    )
    (path
      (reference "Y1") (unit 1) (value "32.768kHz") (footprint "Crystal:Crystal_SMD_MicroCrystal_CC7V-T1A-2Pin_3.2x1.5mm")
    )
  )
)
