(kicad_symbol_lib
	(version 20231120)
	(generator "kicad_symbol_editor")
	(generator_version "8.0")
	(symbol "PIC16F1919x-xMR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.845 29.845 0)
		)
		(property "Value" "PIC16F1919x-xMR"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF19195-6-7-Data-Sheet-40001873D.pdf"
			(at 0 0 0)
		)
		(property "Description" "8kW FLASH, 1kB RAM, 256B EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F1919x-xMR_0_1")
		(symbol "PIC16F1919x-xMR_1_1"
			(pin bidirectional line
				(at -34.29 19.05 0)
				(length 2.54)
				(name "VLCD2/RE1")
				(number "1")
			)
			(pin power_in line
				(at -34.29 -3.81 0)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin bidirectional line
				(at -34.29 -6.35 0)
				(length 2.54)
				(name "SEG25/RF7")
				(number "11")
			)
			(pin bidirectional line
				(at -34.29 -8.89 0)
				(length 2.54)
				(name "SEG24/RF6")
				(number "12")
			)
			(pin bidirectional line
				(at -34.29 -11.43 0)
				(length 2.54)
				(name "SEG23/RF5")
				(number "13")
			)
			(pin bidirectional line
				(at -34.29 -13.97 0)
				(length 2.54)
				(name "SEG22/RF4")
				(number "14")
			)
			(pin bidirectional line
				(at -34.29 -16.51 0)
				(length 2.54)
				(name "SEG21/RF3")
				(number "15")
			)
			(pin bidirectional line
				(at -34.29 -19.05 0)
				(length 2.54)
				(name "SEG20/RF2")
				(number "16")
			)
			(pin bidirectional line
				(at -19.05 -34.29 90)
				(length 2.54)
				(name "SEG19/RF1")
				(number "17")
			)
			(pin bidirectional line
				(at -16.51 -34.29 90)
				(length 2.54)
				(name "SEG41/RF0")
				(number "18")
			)
			(pin bidirectional line
				(at -13.97 -34.29 90)
				(length 2.54)
				(name "COM7/SEG15/RG7")
				(number "19")
			)
			(pin bidirectional line
				(at -34.29 16.51 0)
				(length 2.54)
				(name "VLCD1/RE0")
				(number "2")
			)
			(pin bidirectional line
				(at -11.43 -34.29 90)
				(length 2.54)
				(name "COM6/RG6")
				(number "20")
			)
			(pin bidirectional line
				(at -8.89 -34.29 90)
				(length 2.54)
				(name "RA3/SEG35")
				(number "21")
			)
			(pin bidirectional line
				(at -6.35 -34.29 90)
				(length 2.54)
				(name "RA2/SEG34")
				(number "22")
			)
			(pin bidirectional line
				(at -3.81 -34.29 90)
				(length 2.54)
				(name "RA1/SEG18")
				(number "23")
			)
			(pin bidirectional line
				(at -1.27 -34.29 90)
				(length 2.54)
				(name "RA0/SEG33")
				(number "24")
			)
			(pin bidirectional line
				(at 1.27 -34.29 90)
				(length 2.54)
				(name "COM5/RH1")
				(number "25")
			)
			(pin bidirectional line
				(at 3.81 -34.29 90)
				(length 2.54)
				(name "COM4/RH0")
				(number "26")
			)
			(pin bidirectional line
				(at 6.35 -34.29 90)
				(length 2.54)
				(name "RA5")
				(number "27")
			)
			(pin bidirectional line
				(at 8.89 -34.29 90)
				(length 2.54)
				(name "RA4/SEG14")
				(number "28")
			)
			(pin bidirectional line
				(at 11.43 -34.29 90)
				(length 2.54)
				(name "RC1")
				(number "29")
			)
			(pin bidirectional line
				(at -34.29 13.97 0)
				(length 2.54)
				(name "SEG42/RG0")
				(number "3")
			)
			(pin bidirectional line
				(at 13.97 -34.29 90)
				(length 2.54)
				(name "RC0")
				(number "30")
			)
			(pin bidirectional line
				(at 16.51 -34.29 90)
				(length 2.54)
				(name "RC6/SEG27")
				(number "31")
			)
			(pin bidirectional line
				(at 19.05 -34.29 90)
				(length 2.54)
				(name "RC7/SEG28")
				(number "32")
			)
			(pin bidirectional line
				(at 34.29 -19.05 180)
				(length 2.54)
				(name "RC2/SEG13")
				(number "33")
			)
			(pin bidirectional line
				(at 34.29 -16.51 180)
				(length 2.54)
				(name "RC3/SEG17")
				(number "34")
			)
			(pin bidirectional line
				(at 34.29 -13.97 180)
				(length 2.54)
				(name "RC4/SEG16")
				(number "35")
			)
			(pin bidirectional line
				(at 34.29 -11.43 180)
				(length 2.54)
				(name "RC5/SEG12")
				(number "36")
			)
			(pin bidirectional line
				(at 34.29 -8.89 180)
				(length 2.54)
				(name "RB7/SEG39/ICSPDAT")
				(number "37")
			)
			(pin power_in line
				(at 34.29 -6.35 180)
				(length 2.54)
				(name "VDD")
				(number "38")
			)
			(pin bidirectional line
				(at 34.29 -3.81 180)
				(length 2.54)
				(name "RA7/SEG37")
				(number "39")
			)
			(pin bidirectional line
				(at -34.29 11.43 0)
				(length 2.54)
				(name "SEG43/RG1")
				(number "4")
			)
			(pin bidirectional line
				(at 34.29 -1.27 180)
				(length 2.54)
				(name "RA6/SEG36")
				(number "40")
			)
			(pin power_in line
				(at 34.29 1.27 180)
				(length 2.54)
				(name "VSS")
				(number "41")
			)
			(pin bidirectional line
				(at 34.29 3.81 180)
				(length 2.54)
				(name "RB6/SEG38/ICSPCLK")
				(number "42")
			)
			(pin bidirectional line
				(at 34.29 6.35 180)
				(length 2.54)
				(name "RB5/SEG29")
				(number "43")
			)
			(pin bidirectional line
				(at 34.29 8.89 180)
				(length 2.54)
				(name "RB4/SEG11")
				(number "44")
			)
			(pin bidirectional line
				(at 34.29 11.43 180)
				(length 2.54)
				(name "RB3/SEG10")
				(number "45")
			)
			(pin bidirectional line
				(at 34.29 13.97 180)
				(length 2.54)
				(name "RB2/SEG9")
				(number "46")
			)
			(pin bidirectional line
				(at 34.29 16.51 180)
				(length 2.54)
				(name "RB1/SEG8")
				(number "47")
			)
			(pin bidirectional line
				(at 34.29 19.05 180)
				(length 2.54)
				(name "RB0/SEG30")
				(number "48")
			)
			(pin bidirectional line
				(at 19.05 34.29 270)
				(length 2.54)
				(name "RD7/SEG7")
				(number "49")
			)
			(pin bidirectional line
				(at -34.29 8.89 0)
				(length 2.54)
				(name "SEG44/RG2")
				(number "5")
			)
			(pin bidirectional line
				(at 16.51 34.29 270)
				(length 2.54)
				(name "RD6/SEG6")
				(number "50")
			)
			(pin bidirectional line
				(at 13.97 34.29 270)
				(length 2.54)
				(name "RD5/SEG5")
				(number "51")
			)
			(pin bidirectional line
				(at 11.43 34.29 270)
				(length 2.54)
				(name "RD4/SEG4")
				(number "52")
			)
			(pin bidirectional line
				(at 8.89 34.29 270)
				(length 2.54)
				(name "RD3/SEG3")
				(number "53")
			)
			(pin bidirectional line
				(at 6.35 34.29 270)
				(length 2.54)
				(name "RD2/SEG2")
				(number "54")
			)
			(pin bidirectional line
				(at 3.81 34.29 270)
				(length 2.54)
				(name "RD1/SEG1")
				(number "55")
			)
			(pin bidirectional line
				(at 1.27 34.29 270)
				(length 2.54)
				(name "CFLY2/SEG40/RH3")
				(number "56")
			)
			(pin bidirectional line
				(at -1.27 34.29 270)
				(length 2.54)
				(name "CFLY1/SEG32/RH2")
				(number "57")
			)
			(pin bidirectional line
				(at -3.81 34.29 270)
				(length 2.54)
				(name "RD0/SEG0")
				(number "58")
			)
			(pin bidirectional line
				(at -6.35 34.29 270)
				(length 2.54)
				(name "SEG31/RE7")
				(number "59")
			)
			(pin bidirectional line
				(at -34.29 6.35 0)
				(length 2.54)
				(name "SEG45/RG3")
				(number "6")
			)
			(pin bidirectional line
				(at -8.89 34.29 270)
				(length 2.54)
				(name "COM3/RE6")
				(number "60")
			)
			(pin bidirectional line
				(at -11.43 34.29 270)
				(length 2.54)
				(name "COM2/RE5")
				(number "61")
			)
			(pin bidirectional line
				(at -13.97 34.29 270)
				(length 2.54)
				(name "COM1/RE4")
				(number "62")
			)
			(pin bidirectional line
				(at -16.51 34.29 270)
				(length 2.54)
				(name "COM0/RE3")
				(number "63")
			)
			(pin input line
				(at -19.05 34.29 270)
				(length 2.54)
				(name "VLCD3")
				(number "64")
			)
			(pin power_in line
				(at -34.29 -1.27 0)
				(length 2.54) hide
				(name "VSS")
				(number "65")
			)
			(pin bidirectional line
				(at -34.29 3.81 0)
				(length 2.54)
				(name "VPP/~{MCLR}/RG5")
				(number "7")
			)
			(pin bidirectional line
				(at -34.29 1.27 0)
				(length 2.54)
				(name "SEG26/RG4")
				(number "8")
			)
			(pin power_in line
				(at -34.29 -1.27 0)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
		)
	)
	(symbol "ppc-board"
		(pin_numbers hide)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PPC"
			(at 0 0 0)
		)
		(property "Value" "ppc-board"
			(at 0 0 0)
		)
		(property "Footprint" "ppc-watch:ppc-board"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0.381 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(symbol "ppc-board_1_0"
			(text "+"
				(at -3.81 0 900)
			)
			(text "-"
				(at 3.81 0 900)
			)
			(text "3v"
				(at 0 1.778 0)
			)
			(text "CR2016"
				(at 0 -2.032 0)
			)
		)
		(symbol "ppc-board_1_1"
			(pin power_out line
				(at -6.35 0 0)
				(length 1.27) hide
				(name "VCC")
				(number "1")
			)
			(pin power_out line
				(at 6.35 0 180)
				(length 1.27) hide
				(name "GND")
				(number "2")
			)
		)
		(symbol "ppc-board_2_0")
		(symbol "ppc-board_2_1"
			(text "+"
				(at 3.81 0 0)
			)
			(text "BUZ"
				(at 0 0 0)
			)
			(pin input line
				(at 6.35 0 180)
				(length 1.27)
				(name "buzz_p")
				(number "3")
			)
		)
		(symbol "ppc-board_3_0")
		(symbol "ppc-board_3_1"
			(pin output line
				(at -3.81 2.54 0)
				(length 1.27)
				(name "MODE")
				(number "4")
			)
			(pin output line
				(at -3.81 -2.54 0)
				(length 1.27)
				(name "ADJ")
				(number "5")
			)
		)
		(symbol "ppc-board_4_0")
		(symbol "ppc-board_4_1"
			(pin bidirectional line
				(at 6.35 0 180)
				(length 2.54)
				(name "ROW0")
				(number "10")
			)
			(pin bidirectional line
				(at 6.35 -2.54 180)
				(length 2.54)
				(name "COL0")
				(number "11")
			)
			(pin bidirectional line
				(at 6.35 -5.08 180)
				(length 2.54)
				(name "COL1")
				(number "12")
			)
			(pin bidirectional line
				(at 6.35 -7.62 180)
				(length 2.54)
				(name "COL2")
				(number "13")
			)
			(pin bidirectional line
				(at 6.35 -10.16 180)
				(length 2.54)
				(name "COL3")
				(number "14")
			)
			(pin unspecified line
				(at 6.35 10.16 180)
				(length 2.54)
				(name "NC")
				(number "6")
			)
			(pin bidirectional line
				(at 6.35 7.62 180)
				(length 2.54)
				(name "ROW3")
				(number "7")
			)
			(pin bidirectional line
				(at 6.35 5.08 180)
				(length 2.54)
				(name "ROW2")
				(number "8")
			)
			(pin bidirectional line
				(at 6.35 2.54 180)
				(length 2.54)
				(name "ROW1")
				(number "9")
			)
		)
		(symbol "ppc-board_5_0")
		(symbol "ppc-board_5_1"
			(pin input line
				(at -6.35 41.91 0)
				(length 2.54)
				(name "COM0")
				(number "15")
			)
			(pin input line
				(at -6.35 39.37 0)
				(length 2.54)
				(name "COM1")
				(number "16")
			)
			(pin input line
				(at -6.35 36.83 0)
				(length 2.54)
				(name "COM2")
				(number "17")
			)
			(pin input line
				(at -6.35 34.29 0)
				(length 2.54)
				(name "COM3")
				(number "18")
			)
			(pin input line
				(at -6.35 31.75 0)
				(length 2.54)
				(name "SEG0")
				(number "19")
			)
			(pin input line
				(at -6.35 29.21 0)
				(length 2.54)
				(name "SEG1")
				(number "20")
			)
			(pin input line
				(at -6.35 26.67 0)
				(length 2.54)
				(name "SEG2")
				(number "21")
			)
			(pin input line
				(at -6.35 24.13 0)
				(length 2.54)
				(name "SEG3")
				(number "22")
			)
			(pin input line
				(at -6.35 21.59 0)
				(length 2.54)
				(name "SEG4")
				(number "23")
			)
			(pin input line
				(at -6.35 19.05 0)
				(length 2.54)
				(name "SEG5")
				(number "24")
			)
			(pin input line
				(at -6.35 16.51 0)
				(length 2.54)
				(name "SEG6")
				(number "25")
			)
			(pin input line
				(at -6.35 13.97 0)
				(length 2.54)
				(name "SEG7")
				(number "26")
			)
			(pin input line
				(at -6.35 11.43 0)
				(length 2.54)
				(name "SEG8")
				(number "27")
			)
			(pin input line
				(at -6.35 8.89 0)
				(length 2.54)
				(name "SEG9")
				(number "28")
			)
			(pin input line
				(at -6.35 6.35 0)
				(length 2.54)
				(name "SEG10")
				(number "29")
			)
			(pin input line
				(at -6.35 3.81 0)
				(length 2.54)
				(name "SEG11")
				(number "30")
			)
			(pin input line
				(at -6.35 1.27 0)
				(length 2.54)
				(name "SEG12")
				(number "31")
			)
			(pin input line
				(at -6.35 -1.27 0)
				(length 2.54)
				(name "SEG13")
				(number "32")
			)
			(pin input line
				(at -6.35 -3.81 0)
				(length 2.54)
				(name "SEG14")
				(number "33")
			)
			(pin input line
				(at -6.35 -6.35 0)
				(length 2.54)
				(name "SEG15")
				(number "34")
			)
			(pin input line
				(at -6.35 -8.89 0)
				(length 2.54)
				(name "SEG16")
				(number "35")
			)
			(pin input line
				(at -6.35 -11.43 0)
				(length 2.54)
				(name "SEG17")
				(number "36")
			)
			(pin input line
				(at -6.35 -13.97 0)
				(length 2.54)
				(name "SEG18")
				(number "37")
			)
			(pin input line
				(at -6.35 -16.51 0)
				(length 2.54)
				(name "SEG19")
				(number "38")
			)
			(pin input line
				(at -6.35 -19.05 0)
				(length 2.54)
				(name "SEG20")
				(number "39")
			)
			(pin input line
				(at -6.35 -21.59 0)
				(length 2.54)
				(name "SEG21")
				(number "40")
			)
			(pin input line
				(at -6.35 -24.13 0)
				(length 2.54)
				(name "SEG22")
				(number "41")
			)
			(pin input line
				(at -6.35 -26.67 0)
				(length 2.54)
				(name "SEG23")
				(number "42")
			)
			(pin input line
				(at -6.35 -29.21 0)
				(length 2.54)
				(name "SEG24")
				(number "43")
			)
			(pin input line
				(at -6.35 -31.75 0)
				(length 2.54)
				(name "SEG25")
				(number "44")
			)
			(pin input line
				(at -6.35 -34.29 0)
				(length 2.54)
				(name "SEG26")
				(number "45")
			)
			(pin input line
				(at -6.35 -36.83 0)
				(length 2.54)
				(name "SEG27")
				(number "46")
			)
			(pin input line
				(at -6.35 -39.37 0)
				(length 2.54)
				(name "SEG28")
				(number "47")
			)
			(pin input line
				(at -6.35 -41.91 0)
				(length 2.54)
				(name "SEG29")
				(number "48")
			)
			(pin input line
				(at -6.35 -44.45 0)
				(length 2.54)
				(name "SEG30")
				(number "49")
			)
		)
		(symbol "ppc-board_6_1"
			(pin input line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "~{MCLR}")
				(number "50")
			)
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "CLK")
				(number "51")
			)
			(pin input line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "DAT")
				(number "52")
			)
		)
		(symbol "ppc-board_7_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "DBG")
				(number "53")
			)
		)
	)
	(symbol "ppc-buttons"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "CSB"
			(at 0 5.715 0)
		)
		(property "Value" "ppc-buttons"
			(at 0 -5.715 0)
		)
		(property "Footprint" ""
			(at 34.29 0 0)
		)
		(property "Datasheet" ""
			(at 34.29 -5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "ppc-buttons_0_1")
		(symbol "ppc-buttons_1_1"
			(pin output line
				(at -4.826 2.54 0)
				(length 1.27)
				(name "MODE")
				(number "1")
			)
			(pin output line
				(at -4.826 -2.54 0)
				(length 1.27)
				(name "ADJ")
				(number "2")
			)
		)
	)
	(symbol "ppc-buzzer"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "BUZ"
			(at -0.635 3.81 0)
		)
		(property "Value" "ppc-buzzer"
			(at -0.635 -3.81 0)
		)
		(property "Footprint" ""
			(at 34.29 0.635 0)
		)
		(property "Datasheet" ""
			(at 34.29 -4.445 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "ppc-buzzer_0_1")
		(symbol "ppc-buzzer_1_1"
			(pin input line
				(at 3.81 0 180)
				(length 1.27)
				(name "BUZZ")
				(number "1")
			)
		)
	)
	(symbol "ppc-keypad"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "KPD"
			(at -5.08 13.335 0)
		)
		(property "Value" "ppc-keypad"
			(at -5.08 -13.335 0)
		)
		(property "Footprint" ""
			(at 2.54 0 0)
		)
		(property "Datasheet" ""
			(at -1.27 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "ppc-keypad_0_1")
		(symbol "ppc-keypad_1_1"
			(pin no_connect line
				(at 5.08 10.16 180)
				(length 1.27)
				(name "NC")
				(number "1")
			)
			(pin bidirectional line
				(at 5.08 7.62 180)
				(length 1.27)
				(name "ROW3")
				(number "2")
			)
			(pin bidirectional line
				(at 5.08 5.08 180)
				(length 1.27)
				(name "ROW2")
				(number "3")
			)
			(pin bidirectional line
				(at 5.08 2.54 180)
				(length 1.27)
				(name "ROW1")
				(number "4")
			)
			(pin bidirectional line
				(at 5.08 0 180)
				(length 1.27)
				(name "ROW0")
				(number "5")
			)
			(pin bidirectional line
				(at 5.08 -2.54 180)
				(length 1.27)
				(name "COL0")
				(number "6")
			)
			(pin bidirectional line
				(at 5.08 -5.08 180)
				(length 1.27)
				(name "COL1")
				(number "7")
			)
			(pin bidirectional line
				(at 5.08 -7.62 180)
				(length 1.27)
				(name "COL2")
				(number "8")
			)
			(pin bidirectional line
				(at 5.08 -10.16 180)
				(length 1.27)
				(name "COL3")
				(number "9")
			)
		)
	)
	(symbol "ppc-lcd"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LCD"
			(at -3.81 45.085 0)
		)
		(property "Value" "ppc-lcd"
			(at -3.81 -47.625 0)
		)
		(property "Footprint" ""
			(at 96.52 2.54 0)
		)
		(property "Datasheet" ""
			(at 96.52 2.54 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "ppc-lcd_0_1")
		(symbol "ppc-lcd_1_1"
			(pin input line
				(at -6.35 41.91 0)
				(length 2.54)
				(name "COM0")
				(number "1")
			)
			(pin input line
				(at -6.35 19.05 0)
				(length 2.54)
				(name "SEG5")
				(number "10")
			)
			(pin input line
				(at -6.35 16.51 0)
				(length 2.54)
				(name "SEG6")
				(number "11")
			)
			(pin input line
				(at -6.35 13.97 0)
				(length 2.54)
				(name "SEG7")
				(number "12")
			)
			(pin input line
				(at -6.35 11.43 0)
				(length 2.54)
				(name "SEG8")
				(number "13")
			)
			(pin input line
				(at -6.35 8.89 0)
				(length 2.54)
				(name "SEG9")
				(number "14")
			)
			(pin input line
				(at -6.35 6.35 0)
				(length 2.54)
				(name "SEG10")
				(number "15")
			)
			(pin input line
				(at -6.35 3.81 0)
				(length 2.54)
				(name "SEG11")
				(number "16")
			)
			(pin input line
				(at -6.35 1.27 0)
				(length 2.54)
				(name "SEG12")
				(number "17")
			)
			(pin input line
				(at -6.35 -1.27 0)
				(length 2.54)
				(name "SEG13")
				(number "18")
			)
			(pin input line
				(at -6.35 -3.81 0)
				(length 2.54)
				(name "SEG14")
				(number "19")
			)
			(pin input line
				(at -6.35 39.37 0)
				(length 2.54)
				(name "COM1")
				(number "2")
			)
			(pin input line
				(at -6.35 -6.35 0)
				(length 2.54)
				(name "SEG15")
				(number "20")
			)
			(pin input line
				(at -6.35 -8.89 0)
				(length 2.54)
				(name "SEG16")
				(number "21")
			)
			(pin input line
				(at -6.35 -11.43 0)
				(length 2.54)
				(name "SEG17")
				(number "22")
			)
			(pin input line
				(at -6.35 -13.97 0)
				(length 2.54)
				(name "SEG18")
				(number "23")
			)
			(pin input line
				(at -6.35 -16.51 0)
				(length 2.54)
				(name "SEG19")
				(number "24")
			)
			(pin input line
				(at -6.35 -19.05 0)
				(length 2.54)
				(name "SEG20")
				(number "25")
			)
			(pin input line
				(at -6.35 -21.59 0)
				(length 2.54)
				(name "SEG21")
				(number "26")
			)
			(pin input line
				(at -6.35 -24.13 0)
				(length 2.54)
				(name "SEG22")
				(number "27")
			)
			(pin input line
				(at -6.35 -26.67 0)
				(length 2.54)
				(name "SEG23")
				(number "28")
			)
			(pin input line
				(at -6.35 -29.21 0)
				(length 2.54)
				(name "SEG24")
				(number "29")
			)
			(pin input line
				(at -6.35 36.83 0)
				(length 2.54)
				(name "COM2")
				(number "3")
			)
			(pin input line
				(at -6.35 -31.75 0)
				(length 2.54)
				(name "SEG25")
				(number "30")
			)
			(pin input line
				(at -6.35 -34.29 0)
				(length 2.54)
				(name "SEG26")
				(number "31")
			)
			(pin input line
				(at -6.35 -36.83 0)
				(length 2.54)
				(name "SEG27")
				(number "32")
			)
			(pin input line
				(at -6.35 -39.37 0)
				(length 2.54)
				(name "SEG28")
				(number "33")
			)
			(pin input line
				(at -6.35 -41.91 0)
				(length 2.54)
				(name "SEG29")
				(number "34")
			)
			(pin input line
				(at -6.35 -44.45 0)
				(length 2.54)
				(name "SEG30")
				(number "35")
			)
			(pin input line
				(at -6.35 34.29 0)
				(length 2.54)
				(name "COM3")
				(number "4")
			)
			(pin input line
				(at -6.35 31.75 0)
				(length 2.54)
				(name "SEG0")
				(number "5")
			)
			(pin input line
				(at -6.35 29.21 0)
				(length 2.54)
				(name "SEG1")
				(number "6")
			)
			(pin input line
				(at -6.35 26.67 0)
				(length 2.54)
				(name "SEG2")
				(number "7")
			)
			(pin input line
				(at -6.35 24.13 0)
				(length 2.54)
				(name "SEG3")
				(number "8")
			)
			(pin input line
				(at -6.35 21.59 0)
				(length 2.54)
				(name "SEG4")
				(number "9")
			)
		)
	)
	(symbol "ppc-power"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PWR"
			(at 0 5.715 0)
		)
		(property "Value" "ppc-power"
			(at 0 -5.715 0)
		)
		(property "Footprint" ""
			(at 34.29 0 0)
		)
		(property "Datasheet" ""
			(at 34.29 -5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "ppc-power_0_0"
			(text "+"
				(at -3.81 0 900)
			)
			(text "-"
				(at 3.81 0 900)
			)
			(text "3v"
				(at 0 -2.032 0)
			)
			(text "CR2016"
				(at 0 2.032 0)
			)
		)
		(symbol "ppc-power_0_1")
		(symbol "ppc-power_1_1"
			(pin power_out line
				(at -6.35 0 0)
				(length 1.27)
				(name "~")
				(number "1")
			)
			(pin power_out line
				(at 6.35 0 180)
				(length 1.27)
				(name "~")
				(number "2")
			)
		)
	)
)